# Configuration information for video process test case.
#    This application will firstly load yuv frames to one type of surface(NV12/YV12/I420)
#  you require. After video processing, the processed content (NV12/YV12/I420 surface)
#  will be stored to frames(yv12 format in file).
#    Supported features include: sharpening, implicit format conversion(NV12<->YV12<->I420). Each
# time only one kind of processing will be executed in test application. Although libva supports
# multiple filters execution in one time. you can modify this configuration file to set the
# filter and the corresponding parameters.

#1.Source YUV(RGB) file information
SRC_FILE_NAME: ./flowersky_352x288.nv12
SRC_FRAME_WIDTH: 352 
SRC_FRAME_HEIGHT: 288
SRC_FRAME_FORMAT: NV12

#Note .nv12 files are in NV12 format
SRC_FILE_FORMAT: NV12

#2.Destination YUV(RGB) file information
DST_FILE_NAME:    ./flowersky_352x288_writer352x288.nv12
DST_FRAME_WIDTH:  352
DST_FRAME_HEIGHT: 288
DST_FRAME_FORMAT: NV12

DST_FILE_FORMAT: NV12

#3.How many frames to be processed
FRAME_SUM: 5

#4.VPP filter specific parameters. If they are not specified here,
#default value will be applied then.
FILTER_TYPE: VAProcFilterSharpening

#4.1 Sharpening parameters
# (0 ~ 64, default 44)
SHARPENING_INTENSITY: 44
