diff -urN linux.old/drivers/mtd/maps/Kconfig linux.dev/drivers/mtd/maps/Kconfig
--- linux.old/drivers/mtd/maps/Kconfig	2006-12-11 20:32:53.000000000 +0100
+++ linux.dev/drivers/mtd/maps/Kconfig	2007-01-03 02:26:02.000000000 +0100
@@ -299,6 +299,12 @@
 	  Mapping for the Flaga digital module. If you don't have one, ignore
 	  this setting.
 
+config MTD_BCM47XX
+	tristate "BCM47xx flash device"
+	depends on MIPS && MTD_CFI && BCM947XX
+	help
+	  Support for the flash chips on the BCM947xx board.
+	  
 config MTD_BEECH
 	tristate "CFI Flash device mapped on IBM 405LP Beech"
 	depends on MTD_CFI && BEECH
diff -urN linux.old/drivers/mtd/maps/Makefile linux.dev/drivers/mtd/maps/Makefile
--- linux.old/drivers/mtd/maps/Makefile	2006-12-11 20:32:53.000000000 +0100
+++ linux.dev/drivers/mtd/maps/Makefile	2007-01-03 02:26:02.000000000 +0100
@@ -29,6 +29,7 @@
 obj-$(CONFIG_MTD_PCMCIA)	+= pcmciamtd.o
 obj-$(CONFIG_MTD_RPXLITE)	+= rpxlite.o
 obj-$(CONFIG_MTD_TQM8XXL)	+= tqm8xxl.o
+obj-$(CONFIG_MTD_BCM47XX)	+= bcm47xx-flash.o
 obj-$(CONFIG_MTD_SA1100)	+= sa1100-flash.o
 obj-$(CONFIG_MTD_IPAQ)		+= ipaq-flash.o
 obj-$(CONFIG_MTD_SBC_GXX)	+= sbc_gxx.o

