diff -Nur linux-2.6.19.2/arch/arm/mach-ixp4xx/ixdp425-pci.c linux-2.6.19.2-owrt/arch/arm/mach-ixp4xx/ixdp425-pci.c
--- linux-2.6.19.2/arch/arm/mach-ixp4xx/ixdp425-pci.c	2007-04-15 14:26:04.000000000 +0200
+++ linux-2.6.19.2-owrt/arch/arm/mach-ixp4xx/ixdp425-pci.c	2007-05-10 11:10:40.000000000 +0200
@@ -66,7 +66,7 @@
 int __init ixdp425_pci_init(void)
 {
 	if (machine_is_ixdp425() || machine_is_ixcdp1100() ||
-			machine_is_avila() || machine_is_ixdp465() || machine_is_compex())
+			machine_is_ixdp465() || machine_is_compex())
 		pci_common_init(&ixdp425_pci);
 	return 0;
 }
diff -Nur linux-2.6.19.2/arch/arm/mach-ixp4xx/ixdp425-setup.c linux-2.6.19.2-owrt/arch/arm/mach-ixp4xx/ixdp425-setup.c
--- linux-2.6.19.2/arch/arm/mach-ixp4xx/ixdp425-setup.c	2007-04-15 14:26:49.000000000 +0200
+++ linux-2.6.19.2-owrt/arch/arm/mach-ixp4xx/ixdp425-setup.c	2007-05-10 11:10:01.000000000 +0200
@@ -205,23 +205,3 @@
 	.init_machine	= ixdp425_init,
 MACHINE_END
 #endif
-
-/*
- * Avila is functionally equivalent to IXDP425 except that it adds
- * a CF IDE slot hanging off the expansion bus. When we have a 
- * driver for IXP4xx CF IDE with driver model support we'll move
- * Avila to it's own setup file.
- */
-#ifdef CONFIG_ARCH_AVILA
-MACHINE_START(AVILA, "Gateworks Avila Network Platform")
-	/* Maintainer: Deepak Saxena <dsaxena@plexity.net> */
-	.phys_io	= IXP4XX_PERIPHERAL_BASE_PHYS,
-	.io_pg_offst	= ((IXP4XX_PERIPHERAL_BASE_VIRT) >> 18) & 0xfffc,
-	.map_io		= ixp4xx_map_io,
-	.init_irq	= ixp4xx_init_irq,
-	.timer		= &ixp4xx_timer,
-	.boot_params	= 0x0100,
-	.init_machine	= ixdp425_init,
-MACHINE_END
-#endif
-
