diff -ur madwifi.old/ath/if_ath.c madwifi.dev/ath/if_ath.c
--- madwifi.old/ath/if_ath.c	2007-05-21 07:53:37.247279824 +0200
+++ madwifi.dev/ath/if_ath.c	2007-05-21 07:55:23.290158856 +0200
@@ -5598,6 +5598,7 @@
 	u_int phyerr;
 	int processed = 0, early_stop = 0;
 	int rx_limit = dev->quota;
+	int mic_fail = 0;
 
 	/* Let the 802.11 layer know about the new noise floor */
 	ic->ic_channoise = sc->sc_channoise;
@@ -5692,31 +5693,16 @@
 			}
 			if (rs->rs_status & HAL_RXERR_MIC) {
 				sc->sc_stats.ast_rx_badmic++;
-				/*
-				 * Do minimal work required to hand off
-				 * the 802.11 header for notification.
-				 */
-				/* XXX frag's and QoS frames */
-				len = rs->rs_datalen;
-				if (len >= sizeof (struct ieee80211_frame)) {
-					bus_dma_sync_single(sc->sc_bdev,
-					    bf->bf_skbaddr, len,
-					    BUS_DMA_FROMDEVICE);
-#if 0
-/* XXX revalidate MIC, lookup ni to find VAP */
-					ieee80211_notify_michael_failure(ic,
-					    (struct ieee80211_frame *) skb->data,
-					    sc->sc_splitmic ?
-					        rs->rs_keyix - 32 : rs->rs_keyix
-					);
-#endif
-				}
+				mic_fail = 1;
 			}
 			/*
 			 * Reject error frames if we have no vaps that 
 			 * are operating in monitor mode.
 			 */
-			if(sc->sc_nmonvaps == 0) goto rx_next;
+			if ((rs->rs_status & ~HAL_RXERR_MIC) &&
+				((rs->rs_status &~ HAL_RXERR_DECRYPT) ||
+			     (sc->sc_ic.ic_opmode != IEEE80211_M_MONITOR)))
+					goto rx_next;
 		}
 rx_accept:
 		/*
@@ -5800,6 +5786,20 @@
 				   rs->rs_rssi);
 		}
 
+		/* MIC failure. Drop the packet in any case */
+		if (mic_fail) {
+			ni = ieee80211_find_rxnode(ic, 
+				(const struct ieee80211_frame_min *) skb->data);
+			if (ni != NULL) {
+				ieee80211_check_mic(ni, skb);
+				ieee80211_unref_node(&ni);
+			}
+			dev_kfree_skb_any(skb);
+			skb = NULL;
+			mic_fail = 0;
+			goto rx_next;
+ 		}
+
 		/*
 		 * Locate the node for sender, track state, and then
 		 * pass the (referenced) node up to the 802.11 layer
diff -ur madwifi.old/net80211/ieee80211_crypto_ccmp.c madwifi.dev/net80211/ieee80211_crypto_ccmp.c
--- madwifi.old/net80211/ieee80211_crypto_ccmp.c	2007-05-18 13:19:16.000000000 +0200
+++ madwifi.dev/net80211/ieee80211_crypto_ccmp.c	2007-05-21 07:54:24.892036720 +0200
@@ -78,7 +78,7 @@
 static int ccmp_encap(struct ieee80211_key *, struct sk_buff *, u_int8_t);
 static int ccmp_decap(struct ieee80211_key *, struct sk_buff *, int);
 static int ccmp_enmic(struct ieee80211_key *, struct sk_buff *, int);
-static int ccmp_demic(struct ieee80211_key *, struct sk_buff *, int);
+static int ccmp_demic(struct ieee80211_key *, struct sk_buff *, int, int);
 
 static const struct ieee80211_cipher ccmp = {
 	.ic_name	= "AES-CCM",
@@ -298,7 +298,7 @@
  * Verify and strip MIC from the frame.
  */
 static int
-ccmp_demic(struct ieee80211_key *k, struct sk_buff *skb, int hdrlen)
+ccmp_demic(struct ieee80211_key *k, struct sk_buff *skb, int hdrlen, int force)
 {
 	return 1;
 }
diff -ur madwifi.old/net80211/ieee80211_crypto.h madwifi.dev/net80211/ieee80211_crypto.h
--- madwifi.old/net80211/ieee80211_crypto.h	2007-05-04 15:45:58.000000000 +0200
+++ madwifi.dev/net80211/ieee80211_crypto.h	2007-05-21 07:54:24.893036568 +0200
@@ -145,7 +145,7 @@
 	int (*ic_encap)(struct ieee80211_key *, struct sk_buff *, u_int8_t);
 	int (*ic_decap)(struct ieee80211_key *, struct sk_buff *, int);
 	int (*ic_enmic)(struct ieee80211_key *, struct sk_buff *, int);
-	int (*ic_demic)(struct ieee80211_key *, struct sk_buff *, int);
+	int (*ic_demic)(struct ieee80211_key *, struct sk_buff *, int, int);
 };
 extern const struct ieee80211_cipher ieee80211_cipher_none;
 
@@ -163,10 +163,10 @@
  */
 static __inline int
 ieee80211_crypto_demic(struct ieee80211vap *vap, struct ieee80211_key *k,
-	struct sk_buff *skb, int hdrlen)
+	struct sk_buff *skb, int hdrlen, int force)
 {
 	const struct ieee80211_cipher *cip = k->wk_cipher;
-	return (cip->ic_miclen > 0 ? cip->ic_demic(k, skb, hdrlen) : 1);
+	return (cip->ic_miclen > 0 ? cip->ic_demic(k, skb, hdrlen, force) : 1);
 }
 
 /*
diff -ur madwifi.old/net80211/ieee80211_crypto_none.c madwifi.dev/net80211/ieee80211_crypto_none.c
--- madwifi.old/net80211/ieee80211_crypto_none.c	2006-09-20 10:45:13.000000000 +0200
+++ madwifi.dev/net80211/ieee80211_crypto_none.c	2007-05-21 07:54:24.893036568 +0200
@@ -52,7 +52,7 @@
 static int none_encap(struct ieee80211_key *, struct sk_buff *, u_int8_t);
 static int none_decap(struct ieee80211_key *, struct sk_buff *, int);
 static int none_enmic(struct ieee80211_key *, struct sk_buff *, int);
-static int none_demic(struct ieee80211_key *, struct sk_buff *, int);
+static int none_demic(struct ieee80211_key *, struct sk_buff *, int, int);
 
 const struct ieee80211_cipher ieee80211_cipher_none = {
 	.ic_name	= "NONE",
@@ -137,7 +137,7 @@
 }
 
 static int
-none_demic(struct ieee80211_key *k, struct sk_buff *skb, int hdrlen)
+none_demic(struct ieee80211_key *k, struct sk_buff *skb, int hdrlen, int force)
 {
 	struct ieee80211vap *vap = k->wk_private;
 
diff -ur madwifi.old/net80211/ieee80211_crypto_tkip.c madwifi.dev/net80211/ieee80211_crypto_tkip.c
--- madwifi.old/net80211/ieee80211_crypto_tkip.c	2007-05-18 13:19:16.000000000 +0200
+++ madwifi.dev/net80211/ieee80211_crypto_tkip.c	2007-05-21 07:54:24.893036568 +0200
@@ -57,7 +57,7 @@
 static int tkip_encap(struct ieee80211_key *, struct sk_buff *, u_int8_t);
 static int tkip_enmic(struct ieee80211_key *, struct sk_buff *, int);
 static int tkip_decap(struct ieee80211_key *, struct sk_buff *, int);
-static int tkip_demic(struct ieee80211_key *, struct sk_buff *, int);
+static int tkip_demic(struct ieee80211_key *, struct sk_buff *, int, int);
 
 static const struct ieee80211_cipher tkip  = {
 	.ic_name	= "TKIP",
@@ -339,7 +339,7 @@
  * Verify and strip MIC from the frame.
  */
 static int
-tkip_demic(struct ieee80211_key *k, struct sk_buff *skb0, int hdrlen)
+tkip_demic(struct ieee80211_key *k, struct sk_buff *skb0, int hdrlen, int force)
 {
 	struct tkip_ctx *ctx = k->wk_private;
 	struct sk_buff *skb;
@@ -355,7 +355,7 @@
 	}
 	wh = (struct ieee80211_frame *) skb0->data;
 	/* NB: skb left pointing at last in chain */
-	if (k->wk_flags & IEEE80211_KEY_SWMIC) {
+	if ((k->wk_flags & IEEE80211_KEY_SWMIC) || force) {
 		struct ieee80211vap *vap = ctx->tc_vap;
 		u8 mic[IEEE80211_WEP_MICLEN];
 		u8 mic0[IEEE80211_WEP_MICLEN];
diff -ur madwifi.old/net80211/ieee80211_crypto_wep.c madwifi.dev/net80211/ieee80211_crypto_wep.c
--- madwifi.old/net80211/ieee80211_crypto_wep.c	2006-09-20 10:45:13.000000000 +0200
+++ madwifi.dev/net80211/ieee80211_crypto_wep.c	2007-05-21 07:54:24.894036416 +0200
@@ -54,7 +54,7 @@
 static int wep_encap(struct ieee80211_key *, struct sk_buff *, u_int8_t);
 static int wep_decap(struct ieee80211_key *, struct sk_buff *, int);
 static int wep_enmic(struct ieee80211_key *, struct sk_buff *, int);
-static int wep_demic(struct ieee80211_key *, struct sk_buff *, int);
+static int wep_demic(struct ieee80211_key *, struct sk_buff *, int, int);
 
 static const struct ieee80211_cipher wep = {
 	.ic_name	= "WEP",
@@ -244,7 +244,7 @@
  * Verify and strip MIC from the frame.
  */
 static int
-wep_demic(struct ieee80211_key *k, struct sk_buff *skb, int hdrlen)
+wep_demic(struct ieee80211_key *k, struct sk_buff *skb, int hdrlen, int force)
 {
 	return 1;
 }
diff -ur madwifi.old/net80211/ieee80211_input.c madwifi.dev/net80211/ieee80211_input.c
--- madwifi.old/net80211/ieee80211_input.c	2007-05-21 07:53:37.249279520 +0200
+++ madwifi.dev/net80211/ieee80211_input.c	2007-05-21 07:54:24.895036264 +0200
@@ -654,7 +654,7 @@
 		 * Next strip any MSDU crypto bits.
 		 */
 		if (key != NULL &&
-		    !ieee80211_crypto_demic(vap, key, skb, hdrspace)) {
+		    !ieee80211_crypto_demic(vap, key, skb, hdrspace, 0)) {
 			IEEE80211_DISCARD_MAC(vap, IEEE80211_MSG_INPUT,
 				ni->ni_macaddr, "data", "%s", "demic error");
 			IEEE80211_NODE_STAT(ni, rx_demicfail);
@@ -3778,6 +3778,47 @@
 }
 #endif
 
+/*
+ * Process a frame w/ hw detected MIC failure. 
+ * The frame will be dropped in any case.
+ */
+void
+ieee80211_check_mic(struct ieee80211_node *ni, struct sk_buff *skb)
+{
+	struct ieee80211vap *vap = ni->ni_vap;
+
+	struct ieee80211_frame *wh;
+	struct ieee80211_key *key;
+	int hdrspace;
+	struct ieee80211com *ic = vap->iv_ic;
+	
+	if (skb->len < sizeof(struct ieee80211_frame_min)) {
+		IEEE80211_DISCARD_MAC(vap, IEEE80211_MSG_ANY,
+		    ni->ni_macaddr, NULL,
+		    "too short (1): len %u", skb->len);
+		vap->iv_stats.is_rx_tooshort++;
+		return;
+	}
+
+	wh = (struct ieee80211_frame *)skb->data;
+		
+	hdrspace = ieee80211_hdrspace(ic, wh);
+	key = ieee80211_crypto_decap(ni, skb, hdrspace);
+	if (key == NULL) {
+		/* NB: stats+msgs handled in crypto_decap */
+		IEEE80211_NODE_STAT(ni, rx_wepfail);
+		return;
+	}
+
+	if (!ieee80211_crypto_demic(vap, key, skb, hdrspace, 1)) {
+		IEEE80211_DISCARD_MAC(vap, IEEE80211_MSG_INPUT,
+			ni->ni_macaddr, "data", "%s", "demic error");
+			IEEE80211_NODE_STAT(ni, rx_demicfail);
+	}
+	return;
+}
+EXPORT_SYMBOL(ieee80211_check_mic);
+
 #ifdef IEEE80211_DEBUG
 /*
  * Debugging support.
diff -ur madwifi.old/net80211/ieee80211_linux.c madwifi.dev/net80211/ieee80211_linux.c
--- madwifi.old/net80211/ieee80211_linux.c	2007-05-21 07:49:54.528138280 +0200
+++ madwifi.dev/net80211/ieee80211_linux.c	2007-05-21 07:54:24.896036112 +0200
@@ -311,8 +311,8 @@
 
 	/* TODO: needed parameters: count, keyid, key type, src address, TSC */
 	snprintf(buf, sizeof(buf), "%s(keyid=%d %scast addr=%s)", tag,
-		keyix, IEEE80211_IS_MULTICAST(wh->i_addr1) ?  "broad" : "uni",
-		ether_sprintf(wh->i_addr1));
+		keyix, IEEE80211_IS_MULTICAST(wh->i_addr2) ?  "broad" : "uni",
+		ether_sprintf(wh->i_addr2));
 	memset(&wrqu, 0, sizeof(wrqu));
 	wrqu.data.length = strlen(buf);
 	wireless_send_event(dev, IWEVCUSTOM, &wrqu, buf);
diff -ur madwifi.old/net80211/ieee80211_proto.h madwifi.dev/net80211/ieee80211_proto.h
--- madwifi.old/net80211/ieee80211_proto.h	2007-05-21 07:49:54.574131288 +0200
+++ madwifi.dev/net80211/ieee80211_proto.h	2007-05-21 07:54:24.896036112 +0200
@@ -91,6 +91,7 @@
 void ieee80211_set11gbasicrates(struct ieee80211_rateset *, enum ieee80211_phymode);
 enum ieee80211_phymode ieee80211_get11gbasicrates(struct ieee80211_rateset *);
 void ieee80211_send_pspoll(struct ieee80211_node *);
+void ieee80211_check_mic(struct ieee80211_node *, struct sk_buff *);
 
 /*
  * Return the size of the 802.11 header for a management or data frame.
