diff -urN linux.old/drivers/mtd/devices/Kconfig linux.dev/drivers/mtd/devices/Kconfig
--- linux.old/drivers/mtd/devices/Kconfig	2007-02-04 04:30:26.145338240 +0100
+++ linux.dev/drivers/mtd/devices/Kconfig	2007-02-02 23:48:28.748969000 +0100
@@ -68,6 +68,10 @@
 	  used for program and data storage.  Set up your spi devices
 	  with the right board-specific platform data.
 
+config MTD_SPIFLASH
+	tristate "Atheros AR2315/6/7 SPI Flash support"
+	depends on MTD && ATHEROS_AR5315
+
 config MTD_SLRAM
 	tristate "Uncached system RAM"
 	depends on MTD
diff -urN linux.old/drivers/mtd/devices/Makefile linux.dev/drivers/mtd/devices/Makefile
--- linux.old/drivers/mtd/devices/Makefile	2007-02-04 04:30:26.146338088 +0100
+++ linux.dev/drivers/mtd/devices/Makefile	2007-02-02 23:48:28.749969000 +0100
@@ -17,3 +17,4 @@
 obj-$(CONFIG_MTD_BLOCK2MTD)	+= block2mtd.o
 obj-$(CONFIG_MTD_DATAFLASH)	+= mtd_dataflash.o
 obj-$(CONFIG_MTD_M25P80)	+= m25p80.o
+obj-$(CONFIG_MTD_SPIFLASH)	+= spiflash.o

