diff -urN linux-2.6.19/drivers/mtd/maps/Kconfig linux-2.6.19.new/drivers/mtd/maps/Kconfig
--- linux-2.6.19/drivers/mtd/maps/Kconfig	2006-11-29 22:57:37.000000000 +0100
+++ linux-2.6.19.new/drivers/mtd/maps/Kconfig	2006-12-18 17:21:07.000000000 +0100
@@ -224,6 +224,13 @@
 	  Flash memory access on 4G Systems MTX-1 Board. If you have one of
 	  these boards and would like to use the flash chips on it, say 'Y'.
 
+config MTD_BCM963XX
+        tristate "BCM963xx Flash device"
+        depends on MIPS && BCM963XX
+        help
+	  Flash memory access on BCM963xx boards. Currently only works with
+	  RedBoot and CFE.
+
 config MTD_DILNETPC
 	tristate "CFI Flash device mapped on DIL/Net PC"
 	depends on X86 && MTD_CONCAT && MTD_PARTITIONS && MTD_CFI_INTELEXT
diff -urN linux-2.6.19/drivers/mtd/maps/Makefile linux-2.6.19.new/drivers/mtd/maps/Makefile
--- linux-2.6.19/drivers/mtd/maps/Makefile	2006-11-29 22:57:37.000000000 +0100
+++ linux-2.6.19.new/drivers/mtd/maps/Makefile	2006-12-18 17:21:07.000000000 +0100
@@ -70,3 +70,4 @@
 obj-$(CONFIG_MTD_OMAP_NOR)	+= omap_nor.o
 obj-$(CONFIG_MTD_MTX1)		+= mtx-1_flash.o
 obj-$(CONFIG_MTD_TQM834x)	+= tqm834x.o
+obj-$(CONFIG_MTD_BCM963XX)      += bcm963xx-flash.o
diff -urN linux-2.6.19/drivers/mtd/redboot.c linux-2.6.19.new/drivers/mtd/redboot.c
--- linux-2.6.19/drivers/mtd/redboot.c	2006-12-18 17:09:14.000000000 +0100
+++ linux-2.6.19.new/drivers/mtd/redboot.c	2006-12-18 17:14:26.000000000 +0100
@@ -39,7 +39,7 @@
 	return 1;
 }
 
-static int parse_redboot_partitions(struct mtd_info *master,
+int parse_redboot_partitions(struct mtd_info *master,
                              struct mtd_partition **pparts,
                              unsigned long fis_origin)
 {
@@ -132,6 +132,14 @@
 		goto out;
 	}
 
+	if (!fis_origin) {
+		for (i = 0; i < numslots; i++) {
+			if (!strncmp(buf[i].name, "RedBoot", 8)) {
+				fis_origin = (buf[i].flash_base & (master->size << 1) - 1);
+			}
+		}
+	}
+
 	for (i = 0; i < numslots; i++) {
 		struct fis_list *new_fl, **prev;
 
@@ -154,9 +162,8 @@
 		new_fl->img = &buf[i];
                 if (fis_origin) {
                         buf[i].flash_base -= fis_origin;
-                } else {
-                        buf[i].flash_base &= master->size-1;
                 }
+		buf[i].flash_base &= (master->size << 1) - 1;
 
 		/* I'm sure the JFFS2 code has done me permanent damage.
 		 * I now think the following is _normal_
