/dts-v1/;

#include "bcm6348.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Broadcom BCM96348GW-11 reference board";
	compatible = "brcm,bcm96348gw-11", "brcm,bcm6348";

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;
		debounce-interval = <60>;

		reset {
			label = "reset";
			gpios = <&pinctrl 33 1>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		power_green {
			label = "96348GW-11:green:power";
			gpios = <&pinctrl 0 1>;
			default-state = "on";
		};
		stop_green {
			label = "96348GW-11:green:stop";
			gpios = <&pinctrl 1 1>;
		};
		adsl_fail_green {
			label = "96348GW-11:green:adsl-fail";
			gpios = <&pinctrl 2 1>;
		};
		ppp_green {
			label = "96348GW-11:green:ppp";
			gpios = <&pinctrl 3 1>;
		};
		ppp_fail_green {
			label = "96348GW-11:green:ppp-fail";
			gpios = <&pinctrl 4 1>;
		};
	};
};

&pflash {
	status = "ok";

	partitions {
		compatible = "brcm,bcm963xx-cfe-nor-partitions";
	};
};

&pinctrl {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_pci &pinctrl_ext_mii &pinctrl_mii_pccard>;
};

&uart0 {
	status = "ok";
};
