/*
 *  BSD LICENSE
 *
 *  Copyright (C) 2018 Piotr Dymacz <pepe2k@gmail.com>
 *  All rights reserved.
 *
 *  Redistribution and use in source and binary forms, with or without
 *  modification, are permitted provided that the following conditions
 *  are met:
 *
 *    1. Redistributions of source code must retain the above copyright
 *       notice, this list of conditions and the following disclaimer.
 *    2. Redistributions in binary form must reproduce the above copyright
 *       notice, this list of conditions and the following disclaimer in the
 *       documentation and/or other materials provided with the distribution.
 *    3. Neither the names of the copyright holders nor the names of any
 *       contributors may be used to endorse or promote products derived
 *       from this software without specific prior written permission.
 *
 *  THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
 *  "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
 *  LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR
 *  A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT
 *  HOLDER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
 *  SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
 *  LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
 *  DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY
 *  THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
 *  (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
 *  OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
 */

/dts-v1/;

#include "mt7628an.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "alfa-network,awusfree1", "mediatek,mt7628an-soc";
	model = "ALFA Network AWUSFREE1";

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio1 6 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "awusfree1:orange:system";
			gpios = <&gpio1 11 GPIO_ACTIVE_LOW>;
		};

		wlan {
			label = "awusfree1:blue:wlan";
			gpios = <&gpio1 12 GPIO_ACTIVE_LOW>;
		};
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};
};

&ehci {
	status = "disabled";
};

&esw {
	mediatek,portdisable = <0x1e>;
};

&ethernet {
	mtd-mac-address = <&factory 0x2e>;
};

&gpio1 {
	status = "okay";
};

&ohci {
	status = "disabled";
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "p0led_an", "wdt", "wled_an";
			ralink,function = "gpio";
		};

		ext_lna {
			ralink,group = "uart1";
			ralink,function = "sw_r";
		};

		ext_pa {
			ralink,group = "i2s";
			ralink,function = "antenna";
		};
	};
};

&spi0 {
	status = "okay";

	m25p80@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;
		m25p,chunked-io = <32>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x1000>;
			};

			partition@31000 {
				label = "config";
				reg = <0x31000 0xf000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				label = "firmware";
				reg = <0x50000 0x7b0000>;
			};
		};
	};
};

&wmac {
	status = "okay";
	mediatek,mtd-eeprom = <&factory 0x0>;
};
