From 3642843a06025ec333d7e92580cf52cb8db2a652 Mon Sep 17 00:00:00 2001
From: Govindraj Raja <Govindraj.Raja@imgtec.com>
Date: Fri, 8 Jan 2016 16:36:07 +0000
Subject: clk: pistachio: Fix wrong SDHost card speed

The SDHost currently clocks the card 4x slower than it
should do, because there is fixed divide by 4 in the
sdhost wrapper that is not present in the clock tree.
To model this add a fixed divide by 4 clock node in
the SDHost clock path.

This will ensure the right clock frequency is selected when
the mmc driver tries to configure frequency on card insert.

Signed-off-by: Govindraj Raja <Govindraj.Raja@imgtec.com>
---
 drivers/clk/pistachio/clk-pistachio.c     | 3 ++-
 include/dt-bindings/clock/pistachio-clk.h | 1 +
 2 files changed, 3 insertions(+), 1 deletion(-)

--- a/drivers/clk/pistachio/clk-pistachio.c
+++ b/drivers/clk/pistachio/clk-pistachio.c
@@ -44,7 +44,7 @@ static struct pistachio_gate pistachio_g
 	GATE(CLK_AUX_ADC_INTERNAL, "aux_adc_internal", "sys_internal_div",
 	     0x104, 22),
 	GATE(CLK_AUX_ADC, "aux_adc", "aux_adc_div", 0x104, 23),
-	GATE(CLK_SD_HOST, "sd_host", "sd_host_div", 0x104, 24),
+	GATE(CLK_SD_HOST, "sd_host", "sd_host_div4", 0x104, 24),
 	GATE(CLK_BT, "bt", "bt_div", 0x104, 25),
 	GATE(CLK_BT_DIV4, "bt_div4", "bt_div4_div", 0x104, 26),
 	GATE(CLK_BT_DIV8, "bt_div8", "bt_div8_div", 0x104, 27),
@@ -54,6 +54,7 @@ static struct pistachio_gate pistachio_g
 static struct pistachio_fixed_factor pistachio_ffs[] __initdata = {
 	FIXED_FACTOR(CLK_WIFI_DIV4, "wifi_div4", "wifi_pll", 4),
 	FIXED_FACTOR(CLK_WIFI_DIV8, "wifi_div8", "wifi_pll", 8),
+	FIXED_FACTOR(CLK_SDHOST_DIV4, "sd_host_div4", "sd_host_div", 4),
 };
 
 static struct pistachio_div pistachio_divs[] __initdata = {
--- a/include/dt-bindings/clock/pistachio-clk.h
+++ b/include/dt-bindings/clock/pistachio-clk.h
@@ -21,6 +21,7 @@
 /* Fixed-factor clocks */
 #define CLK_WIFI_DIV4			16
 #define CLK_WIFI_DIV8			17
+#define CLK_SDHOST_DIV4			18
 
 /* Gate clocks */
 #define CLK_MIPS			32
