From: Florian Fainelli <f.fainelli@gmail.com>
Date: Tue, 22 Nov 2016 11:40:56 -0800
Subject: [PATCH] net: phy: broadcom: Allow enabling or disabling of EEE

In preparation for adding support for Wirespeed/downshift, we need to
change bcm_phy_eee_enable() to allow enabling or disabling EEE, so make
the function take an extra enable/disable boolean parameter and rename
it to illustrate it sets EEE, not necessarily just enables it.

Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---

--- a/drivers/net/phy/bcm7xxx.c
+++ b/drivers/net/phy/bcm7xxx.c
@@ -199,7 +199,7 @@ static int bcm7xxx_28nm_config_init(stru
 	if (ret)
 		return ret;
 
-	ret = bcm_phy_enable_eee(phydev);
+	ret = bcm_phy_set_eee(phydev, true);
 	if (ret)
 		return ret;
 
--- a/drivers/net/phy/bcm-cygnus.c
+++ b/drivers/net/phy/bcm-cygnus.c
@@ -104,7 +104,7 @@ static int bcm_cygnus_config_init(struct
 		return rc;
 
 	/* Advertise EEE */
-	rc = bcm_phy_enable_eee(phydev);
+	rc = bcm_phy_set_eee(phydev, true);
 	if (rc)
 		return rc;
 
--- a/drivers/net/phy/bcm-phy-lib.c
+++ b/drivers/net/phy/bcm-phy-lib.c
@@ -195,7 +195,7 @@ int bcm_phy_enable_apd(struct phy_device
 }
 EXPORT_SYMBOL_GPL(bcm_phy_enable_apd);
 
-int bcm_phy_enable_eee(struct phy_device *phydev)
+int bcm_phy_set_eee(struct phy_device *phydev, bool enable)
 {
 	int val;
 
@@ -205,7 +205,10 @@ int bcm_phy_enable_eee(struct phy_device
 	if (val < 0)
 		return val;
 
-	val |= LPI_FEATURE_EN | LPI_FEATURE_EN_DIG1000X;
+	if (enable)
+		val |= LPI_FEATURE_EN | LPI_FEATURE_EN_DIG1000X;
+	else
+		val &= ~(LPI_FEATURE_EN | LPI_FEATURE_EN_DIG1000X);
 
 	phy_write_mmd_indirect(phydev, BRCM_CL45VEN_EEE_CONTROL,
 			       MDIO_MMD_AN, (u32)val);
@@ -216,14 +219,17 @@ int bcm_phy_enable_eee(struct phy_device
 	if (val < 0)
 		return val;
 
-	val |= (MDIO_AN_EEE_ADV_100TX | MDIO_AN_EEE_ADV_1000T);
+	if (enable)
+		val |= (MDIO_AN_EEE_ADV_100TX | MDIO_AN_EEE_ADV_1000T);
+	else
+		val &= ~(MDIO_AN_EEE_ADV_100TX | MDIO_AN_EEE_ADV_1000T);
 
 	phy_write_mmd_indirect(phydev, BCM_CL45VEN_EEE_ADV,
 			       MDIO_MMD_AN, (u32)val);
 
 	return 0;
 }
-EXPORT_SYMBOL_GPL(bcm_phy_enable_eee);
+EXPORT_SYMBOL_GPL(bcm_phy_set_eee);
 
 MODULE_DESCRIPTION("Broadcom PHY Library");
 MODULE_LICENSE("GPL v2");
--- a/drivers/net/phy/bcm-phy-lib.h
+++ b/drivers/net/phy/bcm-phy-lib.h
@@ -43,5 +43,5 @@ int bcm_phy_config_intr(struct phy_devic
 
 int bcm_phy_enable_apd(struct phy_device *phydev, bool dll_pwr_down);
 
-int bcm_phy_enable_eee(struct phy_device *phydev);
+int bcm_phy_set_eee(struct phy_device *phydev, bool enable);
 #endif /* _LINUX_BCM_PHY_LIB_H */
