/dts-v1/;

#include "vr9.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/mips/lantiq_rcu_gphy.h>

/ {
	compatible = "avm,fritz7360sl", "lantiq,xway", "lantiq,vr9";
	model = "1&1 HomeServer";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_green;

		led-dsl = &info_green;
		led-wifi = &wifi;
	};

	memory@0 {
		reg = <0x0 0x8000000>;
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;
		dect {
			label = "dect";
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_PHONE>;
		};
		wifi {
			label = "wifi";
			gpios = <&gpio 29 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_WLAN>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		power_green: power {
			label = "fritz7360sl:green:power";
			gpios = <&gpio 32 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		power_red: power2 {
			label = "fritz7360sl:red:power";
			gpios = <&gpio 33 GPIO_ACTIVE_LOW>;
		};
		info_red {
			label = "fritz7360sl:red:info";
			gpios = <&gpio 34 GPIO_ACTIVE_LOW>;
		};
		info_green: info_green {
			label = "fritz7360sl:green:info";
			gpios = <&gpio 47 GPIO_ACTIVE_LOW>;
		};
		wifi: wifi {
			label = "fritz7360sl:green:wlan";
			gpios = <&gpio 36 GPIO_ACTIVE_LOW>;
		};
		dect {
			label = "fritz7360sl:green:dect";
			gpios = <&gpio 35 GPIO_ACTIVE_LOW>;
		};
	};
};

&eth0 {
	lan: interface@0 {
		compatible = "lantiq,xrx200-pdi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0>;
		mtd-mac-address = <&urlader 0xa91>;
		mtd-mac-address-increment = <(-2)>;
		lantiq,switch;

		ethernet@0 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <0>;
			phy-mode = "rmii";
			phy-handle = <&phy0>;
		};
		ethernet@1 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <1>;
			phy-mode = "rmii";
			phy-handle = <&phy1>;
		};
		ethernet@2 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <2>;
			phy-mode = "gmii";
			phy-handle = <&phy11>;
		};
		ethernet@3 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <4>;
			phy-mode = "gmii";
			phy-handle = <&phy13>;
		};
	};

	mdio@0 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "lantiq,xrx200-mdio";
		reg = <0>;

		phy0: ethernet-phy@0 {
			reg = <0x00>;
			compatible = "ethernet-phy-ieee802.3-c22";
			reset-gpios = <&gpio 37 GPIO_ACTIVE_LOW>;
		};
		phy1: ethernet-phy@1 {
			reg = <0x01>;
			compatible = "ethernet-phy-ieee802.3-c22";
			reset-gpios = <&gpio 44 GPIO_ACTIVE_LOW>;
		};
		phy11: ethernet-phy@11 {
			reg = <0x11>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy13: ethernet-phy@13 {
			reg = <0x13>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
	};
};

&gphy0 {
	lantiq,gphy-mode = <GPHY_MODE_GE>;
};

&gphy1 {
	lantiq,gphy-mode = <GPHY_MODE_GE>;
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		mdio {
			lantiq,groups = "mdio";
			lantiq,function = "mdio";
		};
		phy-rst {
			lantiq,pins = "io37", "io44";
			lantiq,pull = <0>;
			lantiq,open-drain;
			lantiq,output = <1>;
		};
		pcie-rst {
			lantiq,pins = "io38";
			lantiq,pull = <0>;
			lantiq,output = <1>;
		};
	};
};

&localbus {
	nor@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x1000000>;
		#address-cells = <1>;
		#size-cells = <1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;
			urlader: partition@0 {
				label = "urlader";
				reg = <0x00000 0x20000>;
				read-only;
			};

			partition@20000 {
				label = "firmware";
				reg = <0x20000 0xf60000>;
			};

			partition@f80000 {
				label = "tffs (1)";
				reg = <0xf80000 0x40000>;
				read-only;
			};

			partition@fc0000 {
				label = "tffs (2)";
				reg = <0xfc0000 0x40000>;
				read-only;
			};
		};
	};
};

&pcie0 {
	pcie@0 {
		reg = <0 0 0 0 0>;
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		device_type = "pci";

		wifi@168c,002e {
			compatible = "pci168c,002e";
			reg = <0 0 0 0 0>;
			qca,no-eeprom; /* load from ath9k-eeprom-pci-0000:01:00.0.bin */
		};
	};
};

&usb_phy0 {
	status = "okay";
};

&usb_phy1 {
	status = "okay";
};

&usb0 {
	status = "okay";
};

&usb1 {
	status = "okay";
};
