diff -urN linux.old/drivers/mtd/maps/ar7-flash.c linux.dev/drivers/mtd/maps/ar7-flash.c
--- linux.old/drivers/mtd/maps/ar7-flash.c	1970-01-01 01:00:00.000000000 +0100
+++ linux.dev/drivers/mtd/maps/ar7-flash.c	2005-07-22 04:35:26.624453992 +0200
@@ -0,0 +1,267 @@
+/*
+ * $Id$
+ *
+ * Normal mappings of chips in physical memory
+ */
+
+#include <linux/module.h>
+#include <linux/types.h>
+#include <linux/kernel.h>
+#include <asm/io.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/map.h>
+#include <linux/config.h>
+#include <linux/mtd/partitions.h>
+#include <linux/squashfs_fs.h>
+
+#define WINDOW_ADDR CONFIG_MTD_AR7_START
+#define WINDOW_SIZE CONFIG_MTD_AR7_LEN
+#define BUSWIDTH CONFIG_MTD_AR7_BUSWIDTH
+
+#include <asm/mips-boards/prom.h>
+extern char *prom_getenv(char *name);
+
+static int create_mtd_partitions(void);
+static void __exit ar7_mtd_cleanup(void);
+	
+#define MAX_NUM_PARTITIONS 5
+static struct mtd_partition ar7_partinfo[MAX_NUM_PARTITIONS];
+
+static struct mtd_info *ar7_mtd_info;
+
+__u8 ar7_read8(struct map_info *map, unsigned long ofs)
+{
+	return __raw_readb(map->map_priv_1 + ofs);
+}
+
+__u16 ar7_read16(struct map_info *map, unsigned long ofs)
+{
+	return __raw_readw(map->map_priv_1 + ofs);
+}
+
+__u32 ar7_read32(struct map_info *map, unsigned long ofs)
+{
+	return __raw_readl(map->map_priv_1 + ofs);
+}
+
+void ar7_copy_from(struct map_info *map, void *to, unsigned long from, ssize_t len)
+{
+	memcpy_fromio(to, map->map_priv_1 + from, len);
+}
+
+void ar7_write8(struct map_info *map, __u8 d, unsigned long adr)
+{
+	__raw_writeb(d, map->map_priv_1 + adr);
+	mb();
+}
+
+void ar7_write16(struct map_info *map, __u16 d, unsigned long adr)
+{
+	__raw_writew(d, map->map_priv_1 + adr);
+	mb();
+}
+
+void ar7_write32(struct map_info *map, __u32 d, unsigned long adr)
+{
+	__raw_writel(d, map->map_priv_1 + adr);
+	mb();
+}
+
+void ar7_copy_to(struct map_info *map, unsigned long to, const void *from, ssize_t len)
+{
+	memcpy_toio(map->map_priv_1 + to, from, len);
+}
+
+struct map_info ar7_map = {
+	name: "Physically mapped flash",
+	size: WINDOW_SIZE,
+	buswidth: BUSWIDTH,
+	read8: ar7_read8,
+	read16: ar7_read16,
+	read32: ar7_read32,
+	copy_from: ar7_copy_from,
+	write8: ar7_write8,
+	write16: ar7_write16,
+	write32: ar7_write32,
+	copy_to: ar7_copy_to
+};
+
+int __init ar7_mtd_init(void)
+{
+	int partitions;
+	
+       	printk(KERN_NOTICE "ar7 flash device: 0x%lx at 0x%lx.\n", (unsigned long)WINDOW_SIZE, (unsigned long)WINDOW_ADDR);
+	ar7_map.map_priv_1 = (unsigned long)ioremap_nocache(WINDOW_ADDR, WINDOW_SIZE);
+
+	if (!ar7_map.map_priv_1) {
+		printk("Failed to ioremap\n");
+		return -EIO;
+	}
+	
+	ar7_mtd_info = do_map_probe("cfi_probe", &ar7_map);
+	if (!ar7_mtd_info)
+	{
+		ar7_mtd_cleanup();
+		return -ENXIO;
+	}
+	
+	ar7_mtd_info->module = THIS_MODULE;
+
+	if (!(partitions = create_mtd_partitions()))
+		add_mtd_device(ar7_mtd_info);
+	else		
+		add_mtd_partitions(ar7_mtd_info, ar7_partinfo, partitions);
+
+	return 0;
+}
+
+static char *strdup(char *str)
+{
+	int n = strlen(str)+1;
+	char *s = kmalloc(n, GFP_KERNEL);
+	if (!s) return NULL;
+	return strcpy(s, str);
+}
+
+
+static int create_mtd_partitions(void)
+{
+	unsigned int offset;
+	unsigned int size;
+	unsigned int found = 0;
+	unsigned int p = 0;
+	unsigned char *flash_base;
+	unsigned char *flash_end;
+	char *env_ptr;
+	char *base_ptr;
+	char *end_ptr;
+	unsigned int adam2_size = 0x20000;
+	unsigned int config_offset = WINDOW_SIZE;
+	unsigned int rootfs_start = 0xe0000;
+
+	printk("Parsing ADAM2 partition map...\n");
+	
+	do {
+		char	env_name[20];
+
+		/* get base and end addresses of flash file system from environment */
+		sprintf(env_name, "mtd%1u", p);
+		printk("Looking for mtd device :%s:\n", env_name);
+
+		env_ptr = prom_getenv(env_name);
+		if(env_ptr == NULL) {
+			/* No more partitions to find */
+			break;
+		}
+
+		/* Extract the start and stop addresses of the partition */
+		base_ptr = strtok(env_ptr, ",");
+		end_ptr = strtok(NULL, ",");
+		if ((base_ptr == NULL) || (end_ptr == NULL)) {	
+			printk("ADAM2 partition error: Invalid %s start,end.\n", env_name);
+			break;
+		}
+
+		flash_base = (unsigned char*) simple_strtol(base_ptr, NULL, 0);
+		flash_end = (unsigned char*) simple_strtol(end_ptr, NULL, 0);
+		if((!flash_base) || (!flash_end)) {
+			printk("ADAM2 partition error: Invalid %s start,end.\n", env_name);
+			break;
+		}
+
+		offset = virt_to_bus(flash_base) - WINDOW_ADDR;
+		size = flash_end - flash_base;
+		printk("Found a %s image (0x%x), with size (0x%x).\n",env_name, offset, size);
+
+		
+		if (offset == 0) {
+			printk("Assuming adam2 size of 0x%x\n", size);
+			adam2_size = size; 			// boot loader
+		} else if (offset > 0x120000) {
+			if (config_offset > offset)
+				config_offset = offset;		// reserved at the end of the flash chip
+		} else if (offset > 0x30000) {
+			printk("Assuming default rootfs offset of 0x%x\n", offset);
+			rootfs_start = offset;			// probably root fs
+		}
+		
+		p++;
+	} while (p < MAX_NUM_PARTITIONS);
+	
+	p = 0;
+	
+	ar7_partinfo[p].name = strdup("adam2");
+	ar7_partinfo[p].offset = 0;
+	ar7_partinfo[p].size = adam2_size;
+	ar7_partinfo[p++].mask_flags = 0;
+
+	ar7_partinfo[p].name = strdup("linux");
+	ar7_partinfo[p].offset = adam2_size;
+	ar7_partinfo[p].size = config_offset - adam2_size;
+	ar7_partinfo[p++].mask_flags = 0;
+
+	if (ar7_read32(&ar7_map, adam2_size) == 0xfeedfa42) {
+		rootfs_start = ar7_read32(&ar7_map, adam2_size + 4) + adam2_size + 28;
+		printk("Setting new rootfs offset to %08x\n", rootfs_start);
+	}
+	
+	ar7_partinfo[p].name = strdup("rootfs");
+	ar7_partinfo[p].offset = rootfs_start;
+	ar7_partinfo[p].size = config_offset - rootfs_start;
+	
+	ar7_partinfo[p++].mask_flags = 0;
+
+	ar7_partinfo[p].name = strdup("config");
+	ar7_partinfo[p].offset = config_offset;
+	ar7_partinfo[p].size = WINDOW_SIZE - config_offset;
+	ar7_partinfo[p++].mask_flags = 0;
+
+	if (ar7_read32(&ar7_map, rootfs_start) == SQUASHFS_MAGIC) {
+		int newsize, newoffset;
+		struct squashfs_super_block sb;
+
+		ar7_copy_from(&ar7_map, &sb, rootfs_start, sizeof(sb));
+		printk("Squashfs detected (size = 0x%08x)\n", sb.bytes_used);
+		
+		newoffset = rootfs_start + sb.bytes_used;
+
+		if ((newoffset % ar7_mtd_info->erasesize) > 0)
+			newoffset += ar7_mtd_info->erasesize - (newoffset % ar7_mtd_info->erasesize);
+		
+		ar7_partinfo[p - 2].size = newoffset - rootfs_start;
+		
+		ar7_partinfo[p].name = strdup("OpenWrt");
+		ar7_partinfo[p].offset = newoffset;
+		ar7_partinfo[p].size = config_offset - newoffset;
+		ar7_partinfo[p++].mask_flags = 0;
+	} else {
+		printk("Unknown filesystem. Moving rootfs partition to next erase block");
+		if ((rootfs_start % ar7_mtd_info->erasesize) > 0) {
+			ar7_partinfo[p - 2].offset += ar7_mtd_info->erasesize - (rootfs_start % ar7_mtd_info->erasesize);
+			ar7_partinfo[p - 2].size -= ar7_mtd_info->erasesize - (rootfs_start % ar7_mtd_info->erasesize);
+		}
+	}
+
+	return p;
+}
+
+static void __exit ar7_mtd_cleanup(void)
+{
+	if (ar7_mtd_info) {
+		del_mtd_partitions(ar7_mtd_info);
+		del_mtd_device(ar7_mtd_info);
+		map_destroy(ar7_mtd_info);
+	}
+
+	if (ar7_map.map_priv_1) {
+		iounmap((void *)ar7_map.map_priv_1);
+		ar7_map.map_priv_1 = 0;
+	}
+}
+
+module_init(ar7_mtd_init);
+module_exit(ar7_mtd_cleanup);
+
+MODULE_LICENSE("GPL");
+MODULE_AUTHOR("Felix Fietkau");
+MODULE_DESCRIPTION("AR7 CFI map driver");
diff -urN linux.old/drivers/mtd/maps/Config.in linux.dev/drivers/mtd/maps/Config.in
--- linux.old/drivers/mtd/maps/Config.in	2005-07-21 05:36:32.414242296 +0200
+++ linux.dev/drivers/mtd/maps/Config.in	2005-07-21 06:29:04.067118232 +0200
@@ -48,6 +48,21 @@
 fi
 
 if [ "$CONFIG_MIPS" = "y" ]; then
+    if [ "$CONFIG_AR7" = "y" ]; then
+      dep_tristate '  Flash chip mapping on Texas Instruments AR7' CONFIG_MTD_AR7 $CONFIG_MTD_CFI $CONFIG_MTD_PARTITIONS
+      dep_bool     '    Use defaults for Texas Instruments AR7' CONFIG_MTD_AR7_DEFAULTS $CONFIG_MTD_AR7
+      if [ "$CONFIG_MTD_AR7" = "y" -o "$CONFIG_MTD_AR7" = "m" ]; then
+         if [ "$CONFIG_MTD_AR7_DEFAULTS" = "y" ]; then
+            define_hex CONFIG_MTD_AR7_START 0x10000000
+            define_hex CONFIG_MTD_AR7_LEN 0x400000
+            define_int CONFIG_MTD_AR7_BUSWIDTH 2
+         else
+            hex '      Physical start address of flash mapping' CONFIG_MTD_AR7_START 0x10000000
+            hex '      Physical length of flash mapping' CONFIG_MTD_AR7_LEN 0x400000
+            int '      Bus width in octets' CONFIG_MTD_AR7_BUSWIDTH 2
+         fi
+      fi
+   fi
    dep_tristate '  Pb1000 MTD support' CONFIG_MTD_PB1000 $CONFIG_MIPS_PB1000
    dep_tristate '  Pb1500 MTD support' CONFIG_MTD_PB1500 $CONFIG_MIPS_PB1500
    dep_tristate '  Pb1100 MTD support' CONFIG_MTD_PB1100 $CONFIG_MIPS_PB1100
diff -urN linux.old/drivers/mtd/maps/Makefile linux.dev/drivers/mtd/maps/Makefile
--- linux.old/drivers/mtd/maps/Makefile	2005-07-21 05:36:32.414242296 +0200
+++ linux.dev/drivers/mtd/maps/Makefile	2005-07-21 06:56:33.265401984 +0200
@@ -10,6 +10,7 @@
 endif
 
 # Chip mappings
+obj-$(CONFIG_MTD_AR7)		+= ar7-flash.o
 obj-$(CONFIG_MTD_CDB89712)	+= cdb89712.o
 obj-$(CONFIG_MTD_ARM_INTEGRATOR)+= integrator-flash.o
 obj-$(CONFIG_MTD_CFI_FLAGADM)	+= cfi_flagadm.o
