#
# Routed point-to-point server
#
config openvpn_recipe server_tun_ptp
	option _description	'Simple server configuration for a routed point-to-point VPN'
	option _role		'server'
	option dev		'tun'
	option ifconfig		'10.0.0.1 10.0.0.2'
	option secret		'shared-secret.key'
	option keepalive	'10 60'
	option verb		'3'
	option mssfix		'1420'

#
# Routed point-to-point client
#
config openvpn_recipe client_tun_ptp
	option _description	'Simple client configuration for a routed point-to-point VPN'
	option _role		'client'
	option dev		'tun'
	list remote		'vpnserver.example.org'
	option ifconfig		'10.0.0.2 10.0.0.1'
	option secret		'shared-secret.key'
	option nobind		'1'
	option verb		'3'

#
# Routed multi-client server
#
config openvpn_recipe server_tun
	option _description	'Server configuration for a routed multi-client VPN'
	option _role		'server'
	option dev		'tun'
	option server		'10.0.100.0 255.255.255.0'
	option ca		'ca.crt'
	option cert		'server.crt'
	option key 		'server.key'
	option dh 		'dh1024.pem'
	option keepalive	'10 60'
	option verb		'3'
	option mssfix		'1420'

#
# Routed client
#
config openvpn_recipe client_tun
	option _description	'Client configuration for a routed multi-client VPN'
	option _role		'client'
	option client		'1'
	option dev		'tun'
	list remote		'vpnserver.example.org'
	option pkcs12		'my_client.p12'
	option remote_cert_tls	'server'
	option nobind		'1'
	option persist_key	'1'
	option persist_tun	'1'
	option verb		'3'
	option reneg_sec	'0'
	option float		'1'

#
# Multi-client ethernet bridge server
#
config openvpn_recipe server_tap_bridge
	option _description	'Server configuration for an ethernet bridge VPN'
	option _role		'server'
	option dev		'tap'
	option server_bridge	'192.168.1.1 255.255.255.0 192.168.1.128 192.168.1.254'
	option ca		'ca.crt'
	option cert		'server.crt'
	option key 		'server.key'
	option dh 		'dh1024.pem'
	option keepalive	'10 60'
	option verb		'3'
	option mssfix		'1420'

#
# Ethernet bridge client
#
config openvpn_recipe client_tap_bridge
	option _description	'Client configuration for an ethernet bridge VPN'
	option _role		'client'
	option client		'1'
	option dev 		'tap'
	list remote		'vpnserver.example.org'
	option ca 		'ca.crt'
	option cert		'my_client.crt'
	option key 		'my_client.key'
	option dh 		'dh1024.pem'
	option remote_cert_tls	'server'
	option nobind		'1'
	option persist_key	'1'
	option verb		'3'
	option reneg_sec	'0'
	option float		'1'
