--- a/drivers/net/bonding/bond_main.c
+++ b/drivers/net/bonding/bond_main.c
@@ -2046,6 +2046,8 @@ int bond_enslave(struct net_device *bond
 		goto err_unregister;
 	}
 
+	bond_lower_state_changed(new_slave);
+
 	res = bond_sysfs_slave_add(new_slave);
 	if (res) {
 		slave_dbg(bond_dev, slave_dev, "Error %d calling bond_sysfs_slave_add\n", res);
--- a/include/net/dsa.h
+++ b/include/net/dsa.h
@@ -149,8 +149,41 @@ struct dsa_switch_tree {
 
 	/* List of DSA links composing the routing table */
 	struct list_head rtable;
+
+	/* Maps offloaded LAG netdevs to a zero-based linear ID for
+	 * drivers that need it.
+	 */
+	struct net_device **lags;
+	unsigned int lags_len;
 };
 
+#define dsa_lags_foreach_id(_id, _dst)				\
+	for ((_id) = 0; (_id) < (_dst)->lags_len; (_id)++)	\
+		if ((_dst)->lags[(_id)])
+
+#define dsa_lag_foreach_port(_dp, _dst, _lag)			\
+	list_for_each_entry((_dp), &(_dst)->ports, list)	\
+		if ((_dp)->lag_dev == (_lag))
+
+static inline struct net_device *dsa_lag_dev(struct dsa_switch_tree *dst,
+					     unsigned int id)
+{
+	return dst->lags[id];
+}
+
+static inline int dsa_lag_id(struct dsa_switch_tree *dst,
+			     struct net_device *lag)
+{
+	unsigned int id;
+
+	dsa_lags_foreach_id(id, dst) {
+		if (dsa_lag_dev(dst, id) == lag)
+			return id;
+	}
+
+	return -ENODEV;
+}
+
 /* TC matchall action types */
 enum dsa_port_mall_action_type {
 	DSA_PORT_MALL_MIRROR,
@@ -220,6 +253,8 @@ struct dsa_port {
 	bool			devlink_port_setup;
 	struct phylink		*pl;
 	struct phylink_config	pl_config;
+	struct net_device	*lag_dev;
+	bool			lag_tx_enabled;
 
 	struct list_head list;
 
@@ -340,6 +375,14 @@ struct dsa_switch {
 	 */
 	bool			mtu_enforcement_ingress;
 
+	/* Drivers that benefit from having an ID associated with each
+	 * offloaded LAG should set this to the maximum number of
+	 * supported IDs. DSA will then maintain a mapping of _at
+	 * least_ these many IDs, accessible to drivers via
+	 * dsa_lag_id().
+	 */
+	unsigned int		num_lag_ids;
+
 	size_t num_ports;
 };
 
@@ -432,6 +475,18 @@ static inline bool dsa_port_is_vlan_filt
 		return dp->vlan_filtering;
 }
 
+static inline
+struct net_device *dsa_port_to_bridge_port(const struct dsa_port *dp)
+{
+	if (!dp->bridge_dev)
+		return NULL;
+
+	if (dp->lag_dev)
+		return dp->lag_dev;
+
+	return dp->slave;
+}
+
 typedef int dsa_fdb_dump_cb_t(const unsigned char *addr, u16 vid,
 			      bool is_static, void *data);
 struct dsa_switch_ops {
@@ -629,6 +684,13 @@ struct dsa_switch_ops {
 	void	(*crosschip_bridge_leave)(struct dsa_switch *ds, int tree_index,
 					  int sw_index, int port,
 					  struct net_device *br);
+	int	(*crosschip_lag_change)(struct dsa_switch *ds, int sw_index,
+					int port);
+	int	(*crosschip_lag_join)(struct dsa_switch *ds, int sw_index,
+				      int port, struct net_device *lag,
+				      struct netdev_lag_upper_info *info);
+	int	(*crosschip_lag_leave)(struct dsa_switch *ds, int sw_index,
+				       int port, struct net_device *lag);
 
 	/*
 	 * PTP functionality
@@ -660,6 +722,16 @@ struct dsa_switch_ops {
 	int	(*port_change_mtu)(struct dsa_switch *ds, int port,
 				   int new_mtu);
 	int	(*port_max_mtu)(struct dsa_switch *ds, int port);
+
+	/*
+	 * LAG integration
+	 */
+	int	(*port_lag_change)(struct dsa_switch *ds, int port);
+	int	(*port_lag_join)(struct dsa_switch *ds, int port,
+				 struct net_device *lag,
+				 struct netdev_lag_upper_info *info);
+	int	(*port_lag_leave)(struct dsa_switch *ds, int port,
+				  struct net_device *lag);
 };
 
 #define DSA_DEVLINK_PARAM_DRIVER(_id, _name, _type, _cmodes)		\
--- a/net/dsa/dsa.c
+++ b/net/dsa/dsa.c
@@ -220,11 +220,21 @@ static int dsa_switch_rcv(struct sk_buff
 	}
 
 	skb = nskb;
-	p = netdev_priv(skb->dev);
 	skb_push(skb, ETH_HLEN);
 	skb->pkt_type = PACKET_HOST;
 	skb->protocol = eth_type_trans(skb, skb->dev);
 
+	if (unlikely(!dsa_slave_dev_check(skb->dev))) {
+		/* Packet is to be injected directly on an upper
+		 * device, e.g. a team/bond, so skip all DSA-port
+		 * specific actions.
+		 */
+		netif_rx(skb);
+		return 0;
+	}
+
+	p = netdev_priv(skb->dev);
+
 	if (unlikely(cpu_dp->ds->untag_bridge_pvid)) {
 		nskb = dsa_untag_bridge_pvid(skb);
 		if (!nskb) {
--- a/net/dsa/dsa2.c
+++ b/net/dsa/dsa2.c
@@ -21,6 +21,65 @@
 static DEFINE_MUTEX(dsa2_mutex);
 LIST_HEAD(dsa_tree_list);
 
+/**
+ * dsa_lag_map() - Map LAG netdev to a linear LAG ID
+ * @dst: Tree in which to record the mapping.
+ * @lag: Netdev that is to be mapped to an ID.
+ *
+ * dsa_lag_id/dsa_lag_dev can then be used to translate between the
+ * two spaces. The size of the mapping space is determined by the
+ * driver by setting ds->num_lag_ids. It is perfectly legal to leave
+ * it unset if it is not needed, in which case these functions become
+ * no-ops.
+ */
+void dsa_lag_map(struct dsa_switch_tree *dst, struct net_device *lag)
+{
+	unsigned int id;
+
+	if (dsa_lag_id(dst, lag) >= 0)
+		/* Already mapped */
+		return;
+
+	for (id = 0; id < dst->lags_len; id++) {
+		if (!dsa_lag_dev(dst, id)) {
+			dst->lags[id] = lag;
+			return;
+		}
+	}
+
+	/* No IDs left, which is OK. Some drivers do not need it. The
+	 * ones that do, e.g. mv88e6xxx, will discover that dsa_lag_id
+	 * returns an error for this device when joining the LAG. The
+	 * driver can then return -EOPNOTSUPP back to DSA, which will
+	 * fall back to a software LAG.
+	 */
+}
+
+/**
+ * dsa_lag_unmap() - Remove a LAG ID mapping
+ * @dst: Tree in which the mapping is recorded.
+ * @lag: Netdev that was mapped.
+ *
+ * As there may be multiple users of the mapping, it is only removed
+ * if there are no other references to it.
+ */
+void dsa_lag_unmap(struct dsa_switch_tree *dst, struct net_device *lag)
+{
+	struct dsa_port *dp;
+	unsigned int id;
+
+	dsa_lag_foreach_port(dp, dst, lag)
+		/* There are remaining users of this mapping */
+		return;
+
+	dsa_lags_foreach_id(id, dst) {
+		if (dsa_lag_dev(dst, id) == lag) {
+			dst->lags[id] = NULL;
+			break;
+		}
+	}
+}
+
 struct dsa_switch *dsa_switch_find(int tree_index, int sw_index)
 {
 	struct dsa_switch_tree *dst;
@@ -597,6 +656,32 @@ static void dsa_tree_teardown_master(str
 			dsa_master_teardown(dp->master);
 }
 
+static int dsa_tree_setup_lags(struct dsa_switch_tree *dst)
+{
+	unsigned int len = 0;
+	struct dsa_port *dp;
+
+	list_for_each_entry(dp, &dst->ports, list) {
+		if (dp->ds->num_lag_ids > len)
+			len = dp->ds->num_lag_ids;
+	}
+
+	if (!len)
+		return 0;
+
+	dst->lags = kcalloc(len, sizeof(*dst->lags), GFP_KERNEL);
+	if (!dst->lags)
+		return -ENOMEM;
+
+	dst->lags_len = len;
+	return 0;
+}
+
+static void dsa_tree_teardown_lags(struct dsa_switch_tree *dst)
+{
+	kfree(dst->lags);
+}
+
 static int dsa_tree_setup(struct dsa_switch_tree *dst)
 {
 	bool complete;
@@ -624,12 +709,18 @@ static int dsa_tree_setup(struct dsa_swi
 	if (err)
 		goto teardown_switches;
 
+	err = dsa_tree_setup_lags(dst);
+	if (err)
+		goto teardown_master;
+
 	dst->setup = true;
 
 	pr_info("DSA: tree %d setup\n", dst->index);
 
 	return 0;
 
+teardown_master:
+	dsa_tree_teardown_master(dst);
 teardown_switches:
 	dsa_tree_teardown_switches(dst);
 teardown_default_cpu:
@@ -645,6 +736,8 @@ static void dsa_tree_teardown(struct dsa
 	if (!dst->setup)
 		return;
 
+	dsa_tree_teardown_lags(dst);
+
 	dsa_tree_teardown_master(dst);
 
 	dsa_tree_teardown_switches(dst);
--- a/net/dsa/dsa_priv.h
+++ b/net/dsa/dsa_priv.h
@@ -20,6 +20,9 @@ enum {
 	DSA_NOTIFIER_BRIDGE_LEAVE,
 	DSA_NOTIFIER_FDB_ADD,
 	DSA_NOTIFIER_FDB_DEL,
+	DSA_NOTIFIER_LAG_CHANGE,
+	DSA_NOTIFIER_LAG_JOIN,
+	DSA_NOTIFIER_LAG_LEAVE,
 	DSA_NOTIFIER_MDB_ADD,
 	DSA_NOTIFIER_MDB_DEL,
 	DSA_NOTIFIER_VLAN_ADD,
@@ -57,6 +60,15 @@ struct dsa_notifier_mdb_info {
 	int port;
 };
 
+/* DSA_NOTIFIER_LAG_* */
+struct dsa_notifier_lag_info {
+	struct net_device *lag;
+	int sw_index;
+	int port;
+
+	struct netdev_lag_upper_info *info;
+};
+
 /* DSA_NOTIFIER_VLAN_* */
 struct dsa_notifier_vlan_info {
 	const struct switchdev_obj_port_vlan *vlan;
@@ -149,6 +161,11 @@ void dsa_port_disable_rt(struct dsa_port
 void dsa_port_disable(struct dsa_port *dp);
 int dsa_port_bridge_join(struct dsa_port *dp, struct net_device *br);
 void dsa_port_bridge_leave(struct dsa_port *dp, struct net_device *br);
+int dsa_port_lag_change(struct dsa_port *dp,
+			struct netdev_lag_lower_state_info *linfo);
+int dsa_port_lag_join(struct dsa_port *dp, struct net_device *lag_dev,
+		      struct netdev_lag_upper_info *uinfo);
+void dsa_port_lag_leave(struct dsa_port *dp, struct net_device *lag_dev);
 int dsa_port_vlan_filtering(struct dsa_port *dp, bool vlan_filtering,
 			    struct switchdev_trans *trans);
 bool dsa_port_skip_vlan_configuration(struct dsa_port *dp);
@@ -181,6 +198,71 @@ int dsa_port_link_register_of(struct dsa
 void dsa_port_link_unregister_of(struct dsa_port *dp);
 extern const struct phylink_mac_ops dsa_port_phylink_mac_ops;
 
+static inline bool dsa_port_offloads_netdev(struct dsa_port *dp,
+					    struct net_device *dev)
+{
+	/* Switchdev offloading can be configured on: */
+
+	if (dev == dp->slave)
+		/* DSA ports directly connected to a bridge, and event
+		 * was emitted for the ports themselves.
+		 */
+		return true;
+
+	if (dp->bridge_dev == dev)
+		/* DSA ports connected to a bridge, and event was emitted
+		 * for the bridge.
+		 */
+		return true;
+
+	if (dp->lag_dev == dev)
+		/* DSA ports connected to a bridge via a LAG */
+		return true;
+
+	return false;
+}
+
+static inline bool dsa_port_offloads_bridge_port(struct dsa_port *dp,
+						 struct net_device *dev)
+{
+	return dsa_port_to_bridge_port(dp) == dev;
+}
+
+static inline bool dsa_port_offloads_bridge(struct dsa_port *dp,
+					    struct net_device *bridge_dev)
+{
+	/* DSA ports connected to a bridge, and event was emitted
+	 * for the bridge.
+	 */
+	return dp->bridge_dev == bridge_dev;
+}
+
+/* Returns true if any port of this tree offloads the given net_device */
+static inline bool dsa_tree_offloads_bridge_port(struct dsa_switch_tree *dst,
+						 struct net_device *dev)
+{
+	struct dsa_port *dp;
+
+	list_for_each_entry(dp, &dst->ports, list)
+		if (dsa_port_offloads_bridge_port(dp, dev))
+			return true;
+
+	return false;
+}
+
+/* Returns true if any port of this tree offloads the given net_device */
+static inline bool dsa_tree_offloads_netdev(struct dsa_switch_tree *dst,
+					    struct net_device *dev)
+{
+	struct dsa_port *dp;
+
+	list_for_each_entry(dp, &dst->ports, list)
+		if (dsa_port_offloads_netdev(dp, dev))
+			return true;
+
+	return false;
+}
+
 /* slave.c */
 extern const struct dsa_device_ops notag_netdev_ops;
 void dsa_slave_mii_bus_init(struct dsa_switch *ds);
@@ -285,6 +367,9 @@ int dsa_switch_register_notifier(struct
 void dsa_switch_unregister_notifier(struct dsa_switch *ds);
 
 /* dsa2.c */
+void dsa_lag_map(struct dsa_switch_tree *dst, struct net_device *lag);
+void dsa_lag_unmap(struct dsa_switch_tree *dst, struct net_device *lag);
+
 extern struct list_head dsa_tree_list;
 
 #endif
--- a/net/dsa/port.c
+++ b/net/dsa/port.c
@@ -193,6 +193,99 @@ void dsa_port_bridge_leave(struct dsa_po
 	dsa_port_set_state_now(dp, BR_STATE_FORWARDING);
 }
 
+int dsa_port_lag_change(struct dsa_port *dp,
+			struct netdev_lag_lower_state_info *linfo)
+{
+	struct dsa_notifier_lag_info info = {
+		.sw_index = dp->ds->index,
+		.port = dp->index,
+	};
+	bool tx_enabled;
+
+	if (!dp->lag_dev)
+		return 0;
+
+	/* On statically configured aggregates (e.g. loadbalance
+	 * without LACP) ports will always be tx_enabled, even if the
+	 * link is down. Thus we require both link_up and tx_enabled
+	 * in order to include it in the tx set.
+	 */
+	tx_enabled = linfo->link_up && linfo->tx_enabled;
+
+	if (tx_enabled == dp->lag_tx_enabled)
+		return 0;
+
+	dp->lag_tx_enabled = tx_enabled;
+
+	return dsa_port_notify(dp, DSA_NOTIFIER_LAG_CHANGE, &info);
+}
+
+int dsa_port_lag_join(struct dsa_port *dp, struct net_device *lag,
+		      struct netdev_lag_upper_info *uinfo)
+{
+	struct dsa_notifier_lag_info info = {
+		.sw_index = dp->ds->index,
+		.port = dp->index,
+		.lag = lag,
+		.info = uinfo,
+	};
+	struct net_device *bridge_dev;
+	int err;
+
+	dsa_lag_map(dp->ds->dst, lag);
+	dp->lag_dev = lag;
+
+	err = dsa_port_notify(dp, DSA_NOTIFIER_LAG_JOIN, &info);
+	if (err)
+		goto err_lag_join;
+
+	bridge_dev = netdev_master_upper_dev_get(lag);
+	if (!bridge_dev || !netif_is_bridge_master(bridge_dev))
+		return 0;
+
+	err = dsa_port_bridge_join(dp, bridge_dev);
+	if (err)
+		goto err_bridge_join;
+
+	return 0;
+
+err_bridge_join:
+	dsa_port_notify(dp, DSA_NOTIFIER_LAG_LEAVE, &info);
+err_lag_join:
+	dp->lag_dev = NULL;
+	dsa_lag_unmap(dp->ds->dst, lag);
+	return err;
+}
+
+void dsa_port_lag_leave(struct dsa_port *dp, struct net_device *lag)
+{
+	struct dsa_notifier_lag_info info = {
+		.sw_index = dp->ds->index,
+		.port = dp->index,
+		.lag = lag,
+	};
+	int err;
+
+	if (!dp->lag_dev)
+		return;
+
+	/* Port might have been part of a LAG that in turn was
+	 * attached to a bridge.
+	 */
+	if (dp->bridge_dev)
+		dsa_port_bridge_leave(dp, dp->bridge_dev);
+
+	dp->lag_tx_enabled = false;
+	dp->lag_dev = NULL;
+
+	err = dsa_port_notify(dp, DSA_NOTIFIER_LAG_LEAVE, &info);
+	if (err)
+		pr_err("DSA: failed to notify DSA_NOTIFIER_LAG_LEAVE: %d\n",
+		       err);
+
+	dsa_lag_unmap(dp->ds->dst, lag);
+}
+
 /* Must be called under rcu_read_lock() */
 static bool dsa_port_can_apply_vlan_filtering(struct dsa_port *dp,
 					      bool vlan_filtering)
--- a/net/dsa/slave.c
+++ b/net/dsa/slave.c
@@ -337,9 +337,6 @@ static int dsa_slave_vlan_add(struct net
 	struct switchdev_obj_port_vlan vlan;
 	int vid, err;
 
-	if (obj->orig_dev != dev)
-		return -EOPNOTSUPP;
-
 	if (dsa_port_skip_vlan_configuration(dp))
 		return 0;
 
@@ -394,11 +391,13 @@ static int dsa_slave_port_obj_add(struct
 
 	switch (obj->id) {
 	case SWITCHDEV_OBJ_ID_PORT_MDB:
-		if (obj->orig_dev != dev)
+		if (!dsa_port_offloads_bridge_port(dp, obj->orig_dev))
 			return -EOPNOTSUPP;
 		err = dsa_port_mdb_add(dp, SWITCHDEV_OBJ_PORT_MDB(obj), trans);
 		break;
 	case SWITCHDEV_OBJ_ID_HOST_MDB:
+		if (!dsa_port_offloads_bridge(dp, obj->orig_dev))
+			return -EOPNOTSUPP;
 		/* DSA can directly translate this to a normal MDB add,
 		 * but on the CPU port.
 		 */
@@ -406,6 +405,9 @@ static int dsa_slave_port_obj_add(struct
 				       trans);
 		break;
 	case SWITCHDEV_OBJ_ID_PORT_VLAN:
+		if (!dsa_port_offloads_bridge_port(dp, obj->orig_dev))
+			return -EOPNOTSUPP;
+
 		err = dsa_slave_vlan_add(dev, obj, trans);
 		break;
 	default:
@@ -424,9 +426,6 @@ static int dsa_slave_vlan_del(struct net
 	struct switchdev_obj_port_vlan *vlan;
 	int vid, err;
 
-	if (obj->orig_dev != dev)
-		return -EOPNOTSUPP;
-
 	if (dsa_port_skip_vlan_configuration(dp))
 		return 0;
 
@@ -453,17 +452,22 @@ static int dsa_slave_port_obj_del(struct
 
 	switch (obj->id) {
 	case SWITCHDEV_OBJ_ID_PORT_MDB:
-		if (obj->orig_dev != dev)
+		if (!dsa_port_offloads_bridge_port(dp, obj->orig_dev))
 			return -EOPNOTSUPP;
 		err = dsa_port_mdb_del(dp, SWITCHDEV_OBJ_PORT_MDB(obj));
 		break;
 	case SWITCHDEV_OBJ_ID_HOST_MDB:
+		if (!dsa_port_offloads_bridge(dp, obj->orig_dev))
+			return -EOPNOTSUPP;
 		/* DSA can directly translate this to a normal MDB add,
 		 * but on the CPU port.
 		 */
 		err = dsa_port_mdb_del(dp->cpu_dp, SWITCHDEV_OBJ_PORT_MDB(obj));
 		break;
 	case SWITCHDEV_OBJ_ID_PORT_VLAN:
+		if (!dsa_port_offloads_bridge_port(dp, obj->orig_dev))
+			return -EOPNOTSUPP;
+
 		err = dsa_slave_vlan_del(dev, obj);
 		break;
 	default:
@@ -1993,6 +1997,46 @@ static int dsa_slave_changeupper(struct
 			dsa_port_bridge_leave(dp, info->upper_dev);
 			err = NOTIFY_OK;
 		}
+	} else if (netif_is_lag_master(info->upper_dev)) {
+		if (info->linking) {
+			err = dsa_port_lag_join(dp, info->upper_dev,
+						info->upper_info);
+			if (err == -EOPNOTSUPP) {
+				NL_SET_ERR_MSG_MOD(info->info.extack,
+						   "Offloading not supported");
+				err = 0;
+			}
+			err = notifier_from_errno(err);
+		} else {
+			dsa_port_lag_leave(dp, info->upper_dev);
+			err = NOTIFY_OK;
+		}
+	}
+
+	return err;
+}
+
+static int
+dsa_slave_lag_changeupper(struct net_device *dev,
+			  struct netdev_notifier_changeupper_info *info)
+{
+	struct net_device *lower;
+	struct list_head *iter;
+	int err = NOTIFY_DONE;
+	struct dsa_port *dp;
+
+	netdev_for_each_lower_dev(dev, lower, iter) {
+		if (!dsa_slave_dev_check(lower))
+			continue;
+
+		dp = dsa_slave_to_port(lower);
+		if (!dp->lag_dev)
+			/* Software LAG */
+			continue;
+
+		err = dsa_slave_changeupper(lower, info);
+		if (notifier_to_errno(err))
+			break;
 	}
 
 	return err;
@@ -2078,10 +2122,26 @@ static int dsa_slave_netdevice_event(str
 		break;
 	}
 	case NETDEV_CHANGEUPPER:
+		if (dsa_slave_dev_check(dev))
+			return dsa_slave_changeupper(dev, ptr);
+
+		if (netif_is_lag_master(dev))
+			return dsa_slave_lag_changeupper(dev, ptr);
+
+		break;
+	case NETDEV_CHANGELOWERSTATE: {
+		struct netdev_notifier_changelowerstate_info *info = ptr;
+		struct dsa_port *dp;
+		int err;
+
 		if (!dsa_slave_dev_check(dev))
-			return NOTIFY_DONE;
+			break;
 
-		return dsa_slave_changeupper(dev, ptr);
+		dp = dsa_slave_to_port(dev);
+
+		err = dsa_port_lag_change(dp, info->lower_state_info);
+		return notifier_from_errno(err);
+	}
 	}
 
 	return NOTIFY_DONE;
@@ -2229,6 +2289,15 @@ static int dsa_slave_switchdev_event(str
 			if (!fdb_info->added_by_user &&
 			    !dp->ds->assisted_learning_on_cpu_port)
 				return NOTIFY_DONE;
+
+			/* When the bridge learns an address on an offloaded
+			 * LAG we don't want to send traffic to the CPU, the
+			 * other ports bridged with the LAG should be able to
+			 * autonomously forward towards it.
+			 */
+			if (dsa_tree_offloads_netdev(dp->ds->dst, dev))
+				return NOTIFY_DONE;
+
 		}
 
 		if (!dp->ds->ops->port_fdb_add || !dp->ds->ops->port_fdb_del)
--- a/net/dsa/switch.c
+++ b/net/dsa/switch.c
@@ -193,6 +193,47 @@ static int dsa_switch_fdb_del(struct dsa
 	return ds->ops->port_fdb_del(ds, port, info->addr, info->vid);
 }
 
+static int dsa_switch_lag_change(struct dsa_switch *ds,
+				 struct dsa_notifier_lag_info *info)
+{
+	if (ds->index == info->sw_index && ds->ops->port_lag_change)
+		return ds->ops->port_lag_change(ds, info->port);
+
+	if (ds->index != info->sw_index && ds->ops->crosschip_lag_change)
+		return ds->ops->crosschip_lag_change(ds, info->sw_index,
+						     info->port);
+
+	return 0;
+}
+
+static int dsa_switch_lag_join(struct dsa_switch *ds,
+			       struct dsa_notifier_lag_info *info)
+{
+	if (ds->index == info->sw_index && ds->ops->port_lag_join)
+		return ds->ops->port_lag_join(ds, info->port, info->lag,
+					      info->info);
+
+	if (ds->index != info->sw_index && ds->ops->crosschip_lag_join)
+		return ds->ops->crosschip_lag_join(ds, info->sw_index,
+						   info->port, info->lag,
+						   info->info);
+
+	return -EOPNOTSUPP;
+}
+
+static int dsa_switch_lag_leave(struct dsa_switch *ds,
+				struct dsa_notifier_lag_info *info)
+{
+	if (ds->index == info->sw_index && ds->ops->port_lag_leave)
+		return ds->ops->port_lag_leave(ds, info->port, info->lag);
+
+	if (ds->index != info->sw_index && ds->ops->crosschip_lag_leave)
+		return ds->ops->crosschip_lag_leave(ds, info->sw_index,
+						    info->port, info->lag);
+
+	return -EOPNOTSUPP;
+}
+
 static bool dsa_switch_mdb_match(struct dsa_switch *ds, int port,
 				 struct dsa_notifier_mdb_info *info)
 {
@@ -340,6 +381,15 @@ static int dsa_switch_event(struct notif
 	case DSA_NOTIFIER_FDB_DEL:
 		err = dsa_switch_fdb_del(ds, info);
 		break;
+	case DSA_NOTIFIER_LAG_CHANGE:
+		err = dsa_switch_lag_change(ds, info);
+		break;
+	case DSA_NOTIFIER_LAG_JOIN:
+		err = dsa_switch_lag_join(ds, info);
+		break;
+	case DSA_NOTIFIER_LAG_LEAVE:
+		err = dsa_switch_lag_leave(ds, info);
+		break;
 	case DSA_NOTIFIER_MDB_ADD:
 		err = dsa_switch_mdb_add(ds, info);
 		break;
--- a/net/dsa/tag_dsa.c
+++ b/net/dsa/tag_dsa.c
@@ -82,7 +82,19 @@ static struct sk_buff *dsa_rcv(struct sk
 	source_device = dsa_header[0] & 0x1f;
 	source_port = (dsa_header[1] >> 3) & 0x1f;
 
-	skb->dev = dsa_master_find_slave(dev, source_device, source_port);
+	if (trunk) {
+		struct dsa_port *cpu_dp = dev->dsa_ptr;
+
+		/* The exact source port is not available in the tag,
+		 * so we inject the frame directly on the upper
+		 * team/bond.
+		 */
+		skb->dev = dsa_lag_dev(cpu_dp->dst, source_port);
+	} else {
+		skb->dev = dsa_master_find_slave(dev, source_device,
+						 source_port);
+	}
+
 	if (!skb->dev)
 		return NULL;
 
