From 90f1afc7f96c8f7cf19c82e5f4b39e61a63b053d Mon Sep 17 00:00:00 2001
From: Emil Renner Berthing <kernel@esmil.dk>
Date: Sun, 31 Jan 2021 00:47:29 +0100
Subject: [PATCH] net: usb: r8152: use new tasklet API

commit f3163f1cb87141c7a41a15a5d4c98b353f807b04 upstream.

This converts the driver to use the new tasklet API introduced in
commit 12cc923f1ccc ("tasklet: Introduce new initialization API")

Signed-off-by: Emil Renner Berthing <kernel@esmil.dk>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/usb/r8152.c | 8 +++-----
 1 file changed, 3 insertions(+), 5 deletions(-)

--- a/drivers/net/usb/r8152.c
+++ b/drivers/net/usb/r8152.c
@@ -2393,11 +2393,9 @@ static void tx_bottom(struct r8152 *tp)
 	} while (res == 0);
 }
 
-static void bottom_half(unsigned long data)
+static void bottom_half(struct tasklet_struct *t)
 {
-	struct r8152 *tp;
-
-	tp = (struct r8152 *)data;
+	struct r8152 *tp = from_tasklet(tp, t, tx_tl);
 
 	if (test_bit(RTL8152_UNPLUG, &tp->flags))
 		return;
@@ -6695,7 +6693,7 @@ static int rtl8152_probe(struct usb_inte
 	mutex_init(&tp->control);
 	INIT_DELAYED_WORK(&tp->schedule, rtl_work_func_t);
 	INIT_DELAYED_WORK(&tp->hw_phy_work, rtl_hw_phy_work_func_t);
-	tasklet_init(&tp->tx_tl, bottom_half, (unsigned long)tp);
+	tasklet_setup(&tp->tx_tl, bottom_half);
 	tasklet_disable(&tp->tx_tl);
 
 	netdev->netdev_ops = &rtl8152_netdev_ops;
