From 0e37ad71b2ff772009595002da2860999e98e14e Mon Sep 17 00:00:00 2001
From: "Russell King (Oracle)" <rmk+kernel@armlinux.org.uk>
Date: Wed, 18 May 2022 15:55:12 +0100
Subject: [PATCH 09/12] net: mtk_eth_soc: move MAC_MCR setting to mac_finish()

Move the setting of the MTK_MAC_MCR register from the end of mac_config
into the phylink mac_finish() method, to keep it as the very last write
that is done during configuration.

Signed-off-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 33 ++++++++++++++-------
 1 file changed, 22 insertions(+), 11 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -316,8 +316,8 @@ static void mtk_mac_config(struct phylin
 	struct mtk_mac *mac = container_of(config, struct mtk_mac,
 					   phylink_config);
 	struct mtk_eth *eth = mac->hw;
-	u32 mcr_cur, mcr_new, sid, i;
 	int val, ge_mode, err = 0;
+	u32 sid, i;
 
 	/* MT76x8 has no hardware settings between for the MAC */
 	if (!MTK_HAS_CAPS(eth->soc->caps, MTK_SOC_MT7628) &&
@@ -455,16 +455,6 @@ static void mtk_mac_config(struct phylin
 		return;
 	}
 
-	/* Setup gmac */
-	mcr_cur = mtk_r32(mac->hw, MTK_MAC_MCR(mac->id));
-	mcr_new = mcr_cur;
-	mcr_new |= MAC_MCR_IPG_CFG | MAC_MCR_FORCE_MODE |
-		   MAC_MCR_BACKOFF_EN | MAC_MCR_BACKPR_EN | MAC_MCR_FORCE_LINK;
-
-	/* Only update control register when needed! */
-	if (mcr_new != mcr_cur)
-		mtk_w32(mac->hw, mcr_new, MTK_MAC_MCR(mac->id));
-
 	return;
 
 err_phy:
@@ -477,6 +467,26 @@ init_err:
 		mac->id, phy_modes(state->interface), err);
 }
 
+static int mtk_mac_finish(struct phylink_config *config, unsigned int mode,
+			  phy_interface_t interface)
+{
+	struct mtk_mac *mac = container_of(config, struct mtk_mac,
+					   phylink_config);
+	u32 mcr_cur, mcr_new;
+
+	/* Setup gmac */
+	mcr_cur = mtk_r32(mac->hw, MTK_MAC_MCR(mac->id));
+	mcr_new = mcr_cur;
+	mcr_new |= MAC_MCR_IPG_CFG | MAC_MCR_FORCE_MODE |
+		   MAC_MCR_BACKOFF_EN | MAC_MCR_BACKPR_EN | MAC_MCR_FORCE_LINK;
+
+	/* Only update control register when needed! */
+	if (mcr_new != mcr_cur)
+		mtk_w32(mac->hw, mcr_new, MTK_MAC_MCR(mac->id));
+
+	return 0;
+}
+
 static void mtk_mac_pcs_get_state(struct phylink_config *config,
 				  struct phylink_link_state *state)
 {
@@ -581,6 +591,7 @@ static const struct phylink_mac_ops mtk_
 	.mac_pcs_get_state = mtk_mac_pcs_get_state,
 	.mac_an_restart = mtk_mac_an_restart,
 	.mac_config = mtk_mac_config,
+	.mac_finish = mtk_mac_finish,
 	.mac_link_down = mtk_mac_link_down,
 	.mac_link_up = mtk_mac_link_up,
 };
