// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "extreme-networks,ws-ap3805i", "qca,qca9557";
	model = "Extreme Networks AP3805i";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_amber;
		led-running = &led_power_green;
		led-upgrade = &led_power_amber;
		label-mac-device = &eth0;
	};

	leds {
		compatible = "gpio-leds";

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};

		led_power_amber: power_amber {
			label = "amber:power";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
		};

		wlan5 {
			label = "green:wlan5";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wlan2 {
			label = "green:wlan2";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
		};
	};

	watchdog {
		compatible = "linux,wdt-gpio";
		gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		hw_algo = "toggle";
		hw_margin_ms = <20000>;
		always-running;
	};
};

&wdt {
	status = "disabled";
};

&wmac {
	status = "okay";

	qca,no-eeprom;
};

&pcie0 {
	status = "okay";

	wifi@0,0,0 {
		compatible = "qcom,ath10k";
		reg = <0x0 0 0 0 0>;
	};
};

&mdio0 {
	status = "okay";

	phy5: ethernet-phy@5 {
		reg = <5>;
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&phy5>;
	phy-mode = "rgmii-id";

	pll-data = <0x82000000 0x80000101 0x80001313>;

	gmac-config {
		device = <&gmac>;
		rgmii-enabled = <1>;
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;
		m25p,fast-read;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot-bak";
				reg = <0x0 0x80000>;
				read-only;
			};

			partition@80000 {
				label = "u-boot";
				reg = <0x080000 0x80000>;
				read-only;
			};

			partition@100000 {
				label = "cfg1";
				reg = <0x100000 0x40000>;
				read-only;
			};

			partition@140000 {
				label = "cfg2";
				reg = <0x140000 0x40000>;
				read-only;
			};

			partition@180000 {
				label = "nvram4";
				reg = <0x180000 0x40000>;
				read-only;
			};

			partition@1c0000 {
				label = "nvram3";
				reg = <0x1c0000 0x40000>;
				read-only;
			};

			partition@200000 {
				label = "nvram2";
				reg = <0x200000 0x40000>;
				read-only;
			};

			partition@240000 {
				label = "nvram1";
				reg = <0x240000 0x40000>;
				read-only;
			};

			partition@280000 {
				label = "PriImg";
				reg = <0x280000 0x1000000>;
				read-only;
			};

			partition@1280000 {
				label = "SecImg";
				reg = <0x1280000 0x1000000>;
				read-only;
			};

			partition@2280000 {
				label = "firmware";
				compatible = "denx,uimage";
				reg = <0x2280000 0x1cc0000>;
			};

			partition@3f40000 {
				label = "cert";
				reg = <0x3f40000 0x80000>;
				read-only;
			};

			partition@3fc0000 {
				label = "art";
				reg = <0x3fc0000 0x40000>;
				read-only;
			};
		};
	};
};
