// SPDX-License-Identifier: GPL-2.0-or-later

#include "rtl838x.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	compatible = "tplink,sg2008p-v1", "realtek,rtl838x-soc";
	model = "TP-Link SG2008P v1";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x10000000>;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio-restart {
		compatible = "gpio-restart";
		gpios = <&gpio0 3 GPIO_ACTIVE_LOW>;
	};

	leds {
		compatible = "gpio-leds";

		led_power: led-0 {
			label = "green:power";
			gpios = <&gpio0 13 GPIO_ACTIVE_HIGH>;
		};
	};

	i2c1: i2c-gpio-1 {
		compatible = "i2c-gpio";
		scl-gpios = <&gpio0 0 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		sda-gpios = <&gpio0 1 (GPIO_ACTIVE_HIGH | GPIO_OPEN_DRAIN)>;
		i2c-gpio,delay-us = <2>;
		#address-cells = <1>;
		#size-cells = <0>;

		tps23861@28 {
			compatible = "ti,tps23861";
			reg = <0x28>;
			shunt-resistor-micro-ohms = <255000>;
		};
	};

	watchdog {
		compatible = "linux,wdt-gpio";
		gpios = <&gpio0 11 GPIO_ACTIVE_HIGH>;
		hw_algo = "toggle";
		/* SGM706 specs: typical 1.6s, but minimum 1.0s. */
		hw_margin_ms = <1000>;
	};

	virtual_flash {
		compatible = "mtd-concat";

		devices = <&syspart &usrpart>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x0 0x1a00000>;
			};
		};
	};
};

&gpio0 {
	watchdog-enable {
		gpio-hog;
		gpios = <14 GPIO_ACTIVE_LOW>;
		output-low;
		line-name = "watchdog-enable";
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0xe0000>;
				read-only;
			};
			partition@e0000 {
				label = "u-boot-env";
				reg = <0xe0000 0x20000>;
			};
			syspart: partition@100000 {
				label = "sys";
				reg = <0x100000 0x600000>;
			};
			usrpart: partition@700000 {
				label = "usrimg1";
				reg = <0x700000 0x1400000>;
			};
			partition@1b00000 {
				label = "usrappfs";
				reg = <0x1b00000 0x400000>;
			};
			partition@1f00000 {
				label = "para";
				reg = <0x1f00000 0x100000>;
				read-only;
			};
		};
	};
};

&ethernet0 {
	mdio: mdio-bus {
		compatible = "realtek,rtl838x-mdio";
		#address-cells = <1>;
		#size-cells = <0>;

		INTERNAL_PHY(8)
		INTERNAL_PHY(9)
		INTERNAL_PHY(10)
		INTERNAL_PHY(11)
		INTERNAL_PHY(12)
		INTERNAL_PHY(13)
		INTERNAL_PHY(14)
		INTERNAL_PHY(15)
	};
};

&switch0 {
	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		SWITCH_PORT(15, 1, internal)
		SWITCH_PORT(14, 2, internal)
		SWITCH_PORT(13, 3, internal)
		SWITCH_PORT(12, 4, internal)
		SWITCH_PORT(11, 5, internal)
		SWITCH_PORT(10, 6, internal)
		SWITCH_PORT(9, 7, internal)
		SWITCH_PORT(8, 8, internal)

		port@28 {
			ethernet = <&ethernet0>;
			reg = <28>;
			phy-mode = "internal";

			fixed-link {
				speed = <1000>;
				full-duplex;
			};
		};
	};
};
