From 47ed8b22fd561b65e8541919becc76ab3d86f7a3 Mon Sep 17 00:00:00 2001
From: Jae Hyun Yoo <quic_jaehyoo@quicinc.com>
Date: Fri, 8 Jul 2022 12:03:19 -0700
Subject: [PATCH] mtd: spi-nor-ids: add winbond w25q512nw family support
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Add Winbond w25q512nwq/n and w25q512nwm support.

datasheet:
https://www.winbond.com/resource-files/W25Q512NW%20RevB%2007192021.pdf

Signed-off-by: Jae Hyun Yoo <quic_jaehyoo@quicinc.com>
Reviewed-by: Cédric Le Goater <clg@kaod.org>
Reviewed-by: Jagan Teki <jagan@amarulasolutions.com>
---
 drivers/mtd/spi/spi-nor-ids.c | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/drivers/mtd/spi/spi-nor-ids.c
+++ b/drivers/mtd/spi/spi-nor-ids.c
@@ -415,6 +415,16 @@ const struct flash_info spi_nor_ids[] =
 			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
 	},
 	{
+		INFO("w25q512nwq", 0xef6020, 0, 64 * 1024, 1024,
+			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
+			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
+	},
+	{
+		INFO("w25q512nwm", 0xef8020, 0, 64 * 1024, 1024,
+			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
+			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
+	},
+	{
 		INFO("w25q01jv", 0xef4021, 0, 64 * 1024, 2048,
 			SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
 			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
