From 64bab887e1861c3db19a37cfab41a45e296e2cc1 Mon Sep 17 00:00:00 2001
From: David Plowman <david.plowman@raspberrypi.com>
Date: Mon, 7 Mar 2022 10:00:33 +0000
Subject: [PATCH] staging: vc04_services: codec: Add support for
 V4L2_PIX_FMT_RGBA32 format

We already support V4L2_PIX_FMT_BGR32 which is the same thing with red
and blue swapped, so it makes sense to include this variant as well.

Signed-off-by: David Plowman <david.plowman@raspberrypi.com>
---
 .../vc04_services/bcm2835-codec/bcm2835-v4l2-codec.c       | 7 +++++++
 1 file changed, 7 insertions(+)

--- a/drivers/staging/vc04_services/bcm2835-codec/bcm2835-v4l2-codec.c
+++ b/drivers/staging/vc04_services/bcm2835-codec/bcm2835-v4l2-codec.c
@@ -241,6 +241,13 @@ static const struct bcm2835_codec_fmt su
 		.mmal_fmt		= MMAL_ENCODING_BGRA,
 		.size_multiplier_x2	= 2,
 	}, {
+		.fourcc			= V4L2_PIX_FMT_RGBA32,
+		.depth			= 32,
+		.bytesperline_align	= { 32, 32, 32, 32 },
+		.flags			= 0,
+		.mmal_fmt		= MMAL_ENCODING_RGBA,
+		.size_multiplier_x2	= 2,
+	}, {
 		/* Bayer formats */
 		/* 8 bit */
 		.fourcc			= V4L2_PIX_FMT_SRGGB8,
