--- a/include/linux/if_bridge.h
+++ b/include/linux/if_bridge.h
@@ -57,6 +57,7 @@ struct br_ip_list {
 #define BR_MRP_LOST_CONT	BIT(18)
 #define BR_MRP_LOST_IN_CONT	BIT(19)
 #define BR_BPDU_FILTER		BIT(20)
+#define BR_OFFLOAD		BIT(21)
 
 #define BR_DEFAULT_AGEING_TIME	(300 * HZ)
 
--- a/net/bridge/Makefile
+++ b/net/bridge/Makefile
@@ -5,7 +5,7 @@
 
 obj-$(CONFIG_BRIDGE) += bridge.o
 
-bridge-y	:= br.o br_device.o br_fdb.o br_forward.o br_if.o br_input.o \
+bridge-y	:= br.o br_device.o br_fdb.o br_forward.o br_if.o br_input.o br_offload.o \
 			br_ioctl.o br_stp.o br_stp_bpdu.o \
 			br_stp_if.o br_stp_timer.o br_netlink.o \
 			br_netlink_tunnel.o br_arp_nd_proxy.o
--- a/net/bridge/br.c
+++ b/net/bridge/br.c
@@ -18,6 +18,7 @@
 #include <net/switchdev.h>
 
 #include "br_private.h"
+#include "br_private_offload.h"
 
 /*
  * Handle changes in state of network devices enslaved to a bridge.
@@ -332,6 +333,10 @@ static int __init br_init(void)
 	if (err)
 		goto err_out;
 
+	err = br_offload_init();
+	if (err)
+		goto err_out0;
+
 	err = register_pernet_subsys(&br_net_ops);
 	if (err)
 		goto err_out1;
@@ -375,6 +380,8 @@ err_out3:
 err_out2:
 	unregister_pernet_subsys(&br_net_ops);
 err_out1:
+	br_offload_fini();
+err_out0:
 	br_fdb_fini();
 err_out:
 	stp_proto_unregister(&br_stp_proto);
@@ -396,6 +403,7 @@ static void __exit br_deinit(void)
 #if IS_ENABLED(CONFIG_ATM_LANE)
 	br_fdb_test_addr_hook = NULL;
 #endif
+	br_offload_fini();
 	br_fdb_fini();
 }
 
--- a/net/bridge/br_device.c
+++ b/net/bridge/br_device.c
@@ -529,6 +529,8 @@ void br_dev_setup(struct net_device *dev
 	br->bridge_hello_time = br->hello_time = 2 * HZ;
 	br->bridge_forward_delay = br->forward_delay = 15 * HZ;
 	br->bridge_ageing_time = br->ageing_time = BR_DEFAULT_AGEING_TIME;
+	br->offload_cache_size = 128;
+	br->offload_cache_reserved = 8;
 	dev->max_mtu = ETH_MAX_MTU;
 
 	br_netfilter_rtable_init(br);
--- a/net/bridge/br_fdb.c
+++ b/net/bridge/br_fdb.c
@@ -23,6 +23,7 @@
 #include <net/switchdev.h>
 #include <trace/events/bridge.h>
 #include "br_private.h"
+#include "br_private_offload.h"
 
 static const struct rhashtable_params br_fdb_rht_params = {
 	.head_offset = offsetof(struct net_bridge_fdb_entry, rhnode),
@@ -513,6 +514,8 @@ static struct net_bridge_fdb_entry *fdb_
 		fdb->key.vlan_id = vid;
 		fdb->flags = flags;
 		fdb->updated = fdb->used = jiffies;
+		INIT_HLIST_HEAD(&fdb->offload_in);
+		INIT_HLIST_HEAD(&fdb->offload_out);
 		if (rhashtable_lookup_insert_fast(&br->fdb_hash_tbl,
 						  &fdb->rhnode,
 						  br_fdb_rht_params)) {
@@ -734,6 +737,8 @@ static void fdb_notify(struct net_bridge
 	struct sk_buff *skb;
 	int err = -ENOBUFS;
 
+	br_offload_fdb_update(fdb);
+
 	if (swdev_notify)
 		br_switchdev_fdb_notify(br, fdb, type);
 
--- a/net/bridge/br_forward.c
+++ b/net/bridge/br_forward.c
@@ -16,6 +16,7 @@
 #include <linux/if_vlan.h>
 #include <linux/netfilter_bridge.h>
 #include "br_private.h"
+#include "br_private_offload.h"
 
 /* Don't forward packets to originating port or forwarding disabled */
 static inline int should_deliver(const struct net_bridge_port *p,
@@ -32,6 +33,8 @@ static inline int should_deliver(const s
 
 int br_dev_queue_push_xmit(struct net *net, struct sock *sk, struct sk_buff *skb)
 {
+	br_offload_output(skb);
+
 	skb_push(skb, ETH_HLEN);
 	if (!is_skb_forwardable(skb->dev, skb))
 		goto drop;
--- a/net/bridge/br_if.c
+++ b/net/bridge/br_if.c
@@ -25,6 +25,7 @@
 #include <net/net_namespace.h>
 
 #include "br_private.h"
+#include "br_private_offload.h"
 
 /*
  * Determine initial path cost based on speed.
@@ -427,7 +428,7 @@ static struct net_bridge_port *new_nbp(s
 	p->path_cost = port_cost(dev);
 	p->priority = 0x8000 >> BR_PORT_BITS;
 	p->port_no = index;
-	p->flags = BR_LEARNING | BR_FLOOD | BR_MCAST_FLOOD | BR_BCAST_FLOOD;
+	p->flags = BR_LEARNING | BR_FLOOD | BR_MCAST_FLOOD | BR_BCAST_FLOOD | BR_OFFLOAD;
 	br_init_port(p);
 	br_set_state(p, BR_STATE_DISABLED);
 	br_stp_port_timer_init(p);
@@ -777,6 +778,9 @@ void br_port_flags_change(struct net_bri
 
 	if (mask & BR_NEIGH_SUPPRESS)
 		br_recalculate_neigh_suppress_enabled(br);
+
+	if (mask & BR_OFFLOAD)
+		br_offload_port_state(p);
 }
 
 bool br_port_flag_is_set(const struct net_device *dev, unsigned long flag)
--- a/net/bridge/br_input.c
+++ b/net/bridge/br_input.c
@@ -22,6 +22,7 @@
 #include <linux/rculist.h>
 #include "br_private.h"
 #include "br_private_tunnel.h"
+#include "br_private_offload.h"
 
 static int
 br_netif_receive_skb(struct net *net, struct sock *sk, struct sk_buff *skb)
@@ -169,6 +170,7 @@ int br_handle_frame_finish(struct net *n
 			dst->used = now;
 		br_forward(dst->dst, skb, local_rcv, false);
 	} else {
+		br_offload_skb_disable(skb);
 		if (!mcast_hit)
 			br_flood(br, skb, pkt_type, local_rcv, false);
 		else
@@ -287,6 +289,9 @@ static rx_handler_result_t br_handle_fra
 	memset(skb->cb, 0, sizeof(struct br_input_skb_cb));
 
 	p = br_port_get_rcu(skb->dev);
+	if (br_offload_input(p, skb))
+		return RX_HANDLER_CONSUMED;
+
 	if (p->flags & BR_VLAN_TUNNEL) {
 		if (br_handle_ingress_vlan_tunnel(skb, p,
 						  nbp_vlan_group_rcu(p)))
--- /dev/null
+++ b/net/bridge/br_offload.c
@@ -0,0 +1,436 @@
+// SPDX-License-Identifier: GPL-2.0-only
+#include <linux/kernel.h>
+#include <linux/workqueue.h>
+#include "br_private.h"
+#include "br_private_offload.h"
+
+static DEFINE_SPINLOCK(offload_lock);
+
+struct bridge_flow_key {
+	u8 dest[ETH_ALEN];
+	u8 src[ETH_ALEN];
+#ifdef CONFIG_BRIDGE_VLAN_FILTERING
+	u16 vlan_tag;
+	bool vlan_present;
+#endif
+};
+
+struct bridge_flow {
+	struct net_bridge_port *port;
+	struct rhash_head node;
+	struct bridge_flow_key key;
+#ifdef CONFIG_BRIDGE_VLAN_FILTERING
+	bool vlan_out_present;
+	u16 vlan_out;
+#endif
+
+	unsigned long used;
+	struct net_bridge_fdb_entry *fdb_in, *fdb_out;
+	struct hlist_node fdb_list_in, fdb_list_out;
+
+	struct rcu_head rcu;
+};
+
+static const struct rhashtable_params flow_params = {
+	.automatic_shrinking = true,
+	.head_offset = offsetof(struct bridge_flow, node),
+	.key_len = sizeof(struct bridge_flow_key),
+	.key_offset = offsetof(struct bridge_flow, key),
+};
+
+static struct kmem_cache *offload_cache __read_mostly;
+
+static void
+flow_rcu_free(struct rcu_head *head)
+{
+	struct bridge_flow *flow;
+
+	flow = container_of(head, struct bridge_flow, rcu);
+	kmem_cache_free(offload_cache, flow);
+}
+
+static void
+__br_offload_flow_free(struct bridge_flow *flow)
+{
+	flow->used = 0;
+	hlist_del(&flow->fdb_list_in);
+	hlist_del(&flow->fdb_list_out);
+
+	call_rcu(&flow->rcu, flow_rcu_free);
+}
+
+static void
+br_offload_flow_free(struct bridge_flow *flow)
+{
+	if (rhashtable_remove_fast(&flow->port->offload.rht, &flow->node,
+				   flow_params) != 0)
+		return;
+
+	__br_offload_flow_free(flow);
+}
+
+static bool
+br_offload_flow_fdb_refresh_time(struct bridge_flow *flow,
+				 struct net_bridge_fdb_entry *fdb)
+{
+	if (!time_after(flow->used, fdb->updated))
+		return false;
+
+	fdb->updated = flow->used;
+
+	return true;
+}
+
+
+static void
+br_offload_flow_refresh_time(struct bridge_flow *flow)
+{
+	br_offload_flow_fdb_refresh_time(flow, flow->fdb_in);
+	br_offload_flow_fdb_refresh_time(flow, flow->fdb_out);
+}
+
+static void
+br_offload_destroy_cb(void *ptr, void *arg)
+{
+	struct bridge_flow *flow = ptr;
+
+	__br_offload_flow_free(flow);
+}
+
+static bool
+br_offload_need_gc(struct net_bridge_port *p)
+{
+	return (atomic_read(&p->offload.rht.nelems) +
+	        p->br->offload_cache_reserved) >= p->br->offload_cache_size;
+}
+
+static void
+br_offload_gc_work(struct work_struct *work)
+{
+	struct rhashtable_iter hti;
+	struct net_bridge_port *p;
+	struct bridge_flow *gc_flow = NULL;
+	struct bridge_flow *flow;
+	unsigned long gc_used;
+
+	p = container_of(work, struct net_bridge_port, offload.gc_work);
+
+	if (!br_offload_need_gc(p))
+		return;
+
+	rhashtable_walk_enter(&p->offload.rht, &hti);
+	rhashtable_walk_start(&hti);
+	while ((flow = rhashtable_walk_next(&hti)) != NULL) {
+		unsigned long used;
+
+		if (IS_ERR(flow))
+			continue;
+
+		used = READ_ONCE(flow->used);
+		if (!used)
+			continue;
+
+		if (gc_flow && !time_before(used, gc_used))
+			continue;
+
+		gc_flow = flow;
+		gc_used = used;
+	}
+	rhashtable_walk_stop(&hti);
+	rhashtable_walk_exit(&hti);
+
+	if (!gc_flow)
+		return;
+
+	spin_lock_bh(&offload_lock);
+	if (br_offload_need_gc(p) && gc_flow &&
+	    gc_flow->used == gc_used)
+		br_offload_flow_free(gc_flow);
+	if (p->offload.enabled && br_offload_need_gc(p))
+		queue_work(system_long_wq, work);
+	spin_unlock_bh(&offload_lock);
+
+}
+
+void br_offload_port_state(struct net_bridge_port *p)
+{
+	struct net_bridge_port_offload *o = &p->offload;
+	bool enabled = true;
+	bool flush = false;
+
+	if (p->state != BR_STATE_FORWARDING ||
+	    !(p->flags & BR_OFFLOAD))
+		enabled = false;
+
+	spin_lock_bh(&offload_lock);
+	if (o->enabled == enabled)
+		goto out;
+
+	if (enabled) {
+		if (!o->gc_work.func)
+			INIT_WORK(&o->gc_work, br_offload_gc_work);
+		rhashtable_init(&o->rht, &flow_params);
+	} else {
+		flush = true;
+		rhashtable_free_and_destroy(&o->rht, br_offload_destroy_cb, o);
+	}
+
+	o->enabled = enabled;
+
+out:
+	spin_unlock_bh(&offload_lock);
+
+	if (flush)
+		flush_work(&o->gc_work);
+}
+
+void br_offload_fdb_update(const struct net_bridge_fdb_entry *fdb)
+{
+	struct bridge_flow *f;
+	struct hlist_node *tmp;
+
+	spin_lock_bh(&offload_lock);
+
+	hlist_for_each_entry_safe(f, tmp, &fdb->offload_in, fdb_list_in)
+		br_offload_flow_free(f);
+
+	hlist_for_each_entry_safe(f, tmp, &fdb->offload_out, fdb_list_out)
+		br_offload_flow_free(f);
+
+	spin_unlock_bh(&offload_lock);
+}
+
+static void
+br_offload_prepare_key(struct net_bridge_port *p, struct bridge_flow_key *key,
+		       struct sk_buff *skb)
+{
+	memset(key, 0, sizeof(*key));
+	memcpy(key, eth_hdr(skb), 2 * ETH_ALEN);
+#ifdef CONFIG_BRIDGE_VLAN_FILTERING
+	if (!br_opt_get(p->br, BROPT_VLAN_ENABLED))
+		return;
+
+	if (!skb_vlan_tag_present(skb) || skb->vlan_proto != p->br->vlan_proto)
+		return;
+
+	key->vlan_present = true;
+	key->vlan_tag = skb_vlan_tag_get_id(skb);
+#endif
+}
+
+void br_offload_output(struct sk_buff *skb)
+{
+	struct net_bridge_port_offload *o;
+	struct br_input_skb_cb *cb = (struct br_input_skb_cb *)skb->cb;
+	struct net_bridge_port *p, *inp;
+	struct net_device *dev;
+	struct net_bridge_fdb_entry *fdb_in, *fdb_out;
+	struct net_bridge_vlan_group *vg;
+	struct bridge_flow_key key;
+	struct bridge_flow *flow;
+	u16 vlan;
+
+	if (!cb->offload)
+		return;
+
+	rcu_read_lock();
+
+	p = br_port_get_rcu(skb->dev);
+	if (!p)
+		goto out;
+
+	o = &p->offload;
+	if (!o->enabled)
+		goto out;
+
+	if (atomic_read(&p->offload.rht.nelems) >= p->br->offload_cache_size)
+		goto out;
+
+	dev = dev_get_by_index_rcu(dev_net(p->br->dev), cb->input_ifindex);
+	if (!dev)
+		goto out;
+
+	inp = br_port_get_rcu(dev);
+	if (!inp)
+		goto out;
+
+	vg = nbp_vlan_group_rcu(inp);
+	vlan = cb->input_vlan_present ? cb->input_vlan_tag : br_get_pvid(vg);
+	fdb_in = br_fdb_find_rcu(p->br, eth_hdr(skb)->h_source, vlan);
+	if (!fdb_in || !fdb_in->dst)
+		goto out;
+
+	vg = nbp_vlan_group_rcu(p);
+	vlan = skb_vlan_tag_present(skb) ? skb_vlan_tag_get_id(skb) : br_get_pvid(vg);
+	fdb_out = br_fdb_find_rcu(p->br, eth_hdr(skb)->h_dest, vlan);
+	if (!fdb_out || !fdb_out->dst)
+		goto out;
+
+	br_offload_prepare_key(p, &key, skb);
+#ifdef CONFIG_BRIDGE_VLAN_FILTERING
+	key.vlan_present = cb->input_vlan_present;
+	key.vlan_tag = cb->input_vlan_tag;
+#endif
+
+	flow = kmem_cache_alloc(offload_cache, GFP_ATOMIC);
+	flow->port = inp;
+	memcpy(&flow->key, &key, sizeof(key));
+
+#ifdef CONFIG_BRIDGE_VLAN_FILTERING
+	flow->vlan_out_present = skb_vlan_tag_present(skb);
+	flow->vlan_out = skb_vlan_tag_get(skb);
+#endif
+
+	flow->fdb_in = fdb_in;
+	flow->fdb_out = fdb_out;
+	flow->used = jiffies;
+
+	spin_lock_bh(&offload_lock);
+	if (!o->enabled ||
+	    atomic_read(&p->offload.rht.nelems) >= p->br->offload_cache_size ||
+	    rhashtable_insert_fast(&inp->offload.rht, &flow->node, flow_params)) {
+		kmem_cache_free(offload_cache, flow);
+		goto out_unlock;
+	}
+
+	hlist_add_head(&flow->fdb_list_in, &fdb_in->offload_in);
+	hlist_add_head(&flow->fdb_list_out, &fdb_out->offload_out);
+
+	if (br_offload_need_gc(p))
+		queue_work(system_long_wq, &p->offload.gc_work);
+
+out_unlock:
+	spin_unlock_bh(&offload_lock);
+
+out:
+	rcu_read_unlock();
+}
+
+bool br_offload_input(struct net_bridge_port *p, struct sk_buff *skb)
+{
+	struct net_bridge_port_offload *o = &p->offload;
+	struct br_input_skb_cb *cb = (struct br_input_skb_cb *)skb->cb;
+	struct bridge_flow_key key;
+	struct net_bridge_port *dst;
+	struct bridge_flow *flow;
+	unsigned long now = jiffies;
+	bool ret = false;
+
+	if (skb->len < sizeof(key))
+		return false;
+
+	if (!o->enabled)
+		return false;
+
+	if (is_multicast_ether_addr(eth_hdr(skb)->h_dest))
+		return false;
+
+	br_offload_prepare_key(p, &key, skb);
+
+	rcu_read_lock();
+	flow = rhashtable_lookup(&o->rht, &key, flow_params);
+	if (!flow) {
+		cb->offload = 1;
+#ifdef CONFIG_BRIDGE_VLAN_FILTERING
+		cb->input_vlan_present = key.vlan_present != 0;
+		cb->input_vlan_tag = key.vlan_tag;
+#endif
+		cb->input_ifindex = p->dev->ifindex;
+		goto out;
+	}
+
+	if (flow->fdb_in->dst != p)
+		goto out;
+
+	dst = flow->fdb_out->dst;
+	if (!dst)
+		goto out;
+
+	ret = true;
+#ifdef CONFIG_BRIDGE_VLAN_FILTERING
+	if (!flow->vlan_out_present && key.vlan_present) {
+		__vlan_hwaccel_clear_tag(skb);
+	} else if (flow->vlan_out_present) {
+		if (skb_vlan_tag_present(skb) &&
+		    skb->vlan_proto != p->br->vlan_proto) {
+			/* Protocol-mismatch, empty out vlan_tci for new tag */
+			skb_push(skb, ETH_HLEN);
+			skb = vlan_insert_tag_set_proto(skb, skb->vlan_proto,
+							skb_vlan_tag_get(skb));
+			if (unlikely(!skb))
+				goto out;
+
+			skb_pull(skb, ETH_HLEN);
+			skb_reset_mac_len(skb);
+		}
+
+		__vlan_hwaccel_put_tag(skb, p->br->vlan_proto,
+				       flow->vlan_out);
+	}
+#endif
+
+	skb->dev = dst->dev;
+	skb_push(skb, ETH_HLEN);
+
+	if (skb_warn_if_lro(skb) || !is_skb_forwardable(skb->dev, skb)) {
+		kfree_skb(skb);
+		goto out;
+	}
+
+	if (now - flow->used >= HZ) {
+		flow->used = now;
+		br_offload_flow_refresh_time(flow);
+	}
+
+	skb_forward_csum(skb);
+	dev_queue_xmit(skb);
+
+out:
+	rcu_read_unlock();
+	return ret;
+}
+
+static void
+br_offload_check_gc(struct net_bridge *br)
+{
+	struct net_bridge_port *p;
+
+	spin_lock_bh(&br->lock);
+	list_for_each_entry(p, &br->port_list, list)
+		if (br_offload_need_gc(p))
+			queue_work(system_long_wq, &p->offload.gc_work);
+	spin_unlock_bh(&br->lock);
+}
+
+
+int br_offload_set_cache_size(struct net_bridge *br, unsigned long val)
+{
+	br->offload_cache_size = val;
+	br_offload_check_gc(br);
+
+	return 0;
+}
+
+int br_offload_set_cache_reserved(struct net_bridge *br, unsigned long val)
+{
+	br->offload_cache_reserved = val;
+	br_offload_check_gc(br);
+
+	return 0;
+}
+
+int __init br_offload_init(void)
+{
+	offload_cache = kmem_cache_create("bridge_offload_cache",
+					  sizeof(struct bridge_flow),
+					  0, SLAB_HWCACHE_ALIGN, NULL);
+	if (!offload_cache)
+		return -ENOMEM;
+
+	return 0;
+}
+
+void br_offload_fini(void)
+{
+	kmem_cache_destroy(offload_cache);
+}
--- a/net/bridge/br_private.h
+++ b/net/bridge/br_private.h
@@ -207,7 +207,13 @@ struct net_bridge_fdb_entry {
 	unsigned long			updated ____cacheline_aligned_in_smp;
 	unsigned long			used;
 
-	struct rcu_head			rcu;
+	union {
+		struct {
+			struct hlist_head		offload_in;
+			struct hlist_head		offload_out;
+		};
+		struct rcu_head			rcu;
+	};
 };
 
 #define MDB_PG_FLAGS_PERMANENT	BIT(0)
@@ -280,6 +286,12 @@ struct net_bridge_mdb_entry {
 	struct rcu_head			rcu;
 };
 
+struct net_bridge_port_offload {
+	struct rhashtable		rht;
+	struct work_struct		gc_work;
+	bool				enabled;
+};
+
 struct net_bridge_port {
 	struct net_bridge		*br;
 	struct net_device		*dev;
@@ -337,6 +349,7 @@ struct net_bridge_port {
 	u16				backup_redirected_cnt;
 
 	struct bridge_stp_xstats	stp_xstats;
+	struct net_bridge_port_offload	offload;
 };
 
 #define kobj_to_brport(obj)	container_of(obj, struct net_bridge_port, kobj)
@@ -475,6 +488,9 @@ struct net_bridge {
 	struct kobject			*ifobj;
 	u32				auto_cnt;
 
+	u32				offload_cache_size;
+	u32				offload_cache_reserved;
+
 #ifdef CONFIG_NET_SWITCHDEV
 	int offload_fwd_mark;
 #endif
@@ -501,6 +517,10 @@ struct br_input_skb_cb {
 #ifdef CONFIG_NETFILTER_FAMILY_BRIDGE
 	u8 br_netfilter_broute:1;
 #endif
+	u8 offload:1;
+	u8 input_vlan_present:1;
+	u16 input_vlan_tag;
+	int input_ifindex;
 
 #ifdef CONFIG_NET_SWITCHDEV
 	int offload_fwd_mark;
--- /dev/null
+++ b/net/bridge/br_private_offload.h
@@ -0,0 +1,21 @@
+#ifndef __BR_OFFLOAD_H
+#define __BR_OFFLOAD_H
+
+bool br_offload_input(struct net_bridge_port *p, struct sk_buff *skb);
+void br_offload_output(struct sk_buff *skb);
+void br_offload_port_state(struct net_bridge_port *p);
+void br_offload_fdb_update(const struct net_bridge_fdb_entry *fdb);
+int br_offload_init(void);
+void br_offload_fini(void);
+int br_offload_set_cache_size(struct net_bridge *br, unsigned long val);
+int br_offload_set_cache_reserved(struct net_bridge *br, unsigned long val);
+
+static inline void br_offload_skb_disable(struct sk_buff *skb)
+{
+	struct br_input_skb_cb *cb = (struct br_input_skb_cb *)skb->cb;
+
+	if (cb->offload)
+		cb->offload = 0;
+}
+
+#endif
--- a/net/bridge/br_stp.c
+++ b/net/bridge/br_stp.c
@@ -12,6 +12,7 @@
 
 #include "br_private.h"
 #include "br_private_stp.h"
+#include "br_private_offload.h"
 
 /* since time values in bpdu are in jiffies and then scaled (1/256)
  * before sending, make sure that is at least one STP tick.
@@ -52,6 +53,8 @@ void br_set_state(struct net_bridge_port
 				(unsigned int) p->port_no, p->dev->name,
 				br_port_state_names[p->state]);
 
+	br_offload_port_state(p);
+
 	if (p->br->stp_enabled == BR_KERNEL_STP) {
 		switch (p->state) {
 		case BR_STATE_BLOCKING:
--- a/net/bridge/br_sysfs_br.c
+++ b/net/bridge/br_sysfs_br.c
@@ -18,6 +18,7 @@
 #include <linux/sched/signal.h>
 
 #include "br_private.h"
+#include "br_private_offload.h"
 
 #define to_bridge(cd)	((struct net_bridge *)netdev_priv(to_net_dev(cd)))
 
@@ -842,6 +843,38 @@ static ssize_t vlan_stats_per_port_store
 static DEVICE_ATTR_RW(vlan_stats_per_port);
 #endif
 
+static ssize_t offload_cache_size_show(struct device *d,
+				       struct device_attribute *attr,
+				       char *buf)
+{
+	struct net_bridge *br = to_bridge(d);
+	return sprintf(buf, "%u\n", br->offload_cache_size);
+}
+
+static ssize_t offload_cache_size_store(struct device *d,
+					struct device_attribute *attr,
+					const char *buf, size_t len)
+{
+	return store_bridge_parm(d, buf, len, br_offload_set_cache_size);
+}
+static DEVICE_ATTR_RW(offload_cache_size);
+
+static ssize_t offload_cache_reserved_show(struct device *d,
+				       struct device_attribute *attr,
+				       char *buf)
+{
+	struct net_bridge *br = to_bridge(d);
+	return sprintf(buf, "%u\n", br->offload_cache_reserved);
+}
+
+static ssize_t offload_cache_reserved_store(struct device *d,
+					struct device_attribute *attr,
+					const char *buf, size_t len)
+{
+	return store_bridge_parm(d, buf, len, br_offload_set_cache_reserved);
+}
+static DEVICE_ATTR_RW(offload_cache_reserved);
+
 static struct attribute *bridge_attrs[] = {
 	&dev_attr_forward_delay.attr,
 	&dev_attr_hello_time.attr,
@@ -896,6 +929,8 @@ static struct attribute *bridge_attrs[]
 	&dev_attr_vlan_stats_enabled.attr,
 	&dev_attr_vlan_stats_per_port.attr,
 #endif
+	&dev_attr_offload_cache_size.attr,
+	&dev_attr_offload_cache_reserved.attr,
 	NULL
 };
 
--- a/net/bridge/br_sysfs_if.c
+++ b/net/bridge/br_sysfs_if.c
@@ -234,6 +234,7 @@ BRPORT_ATTR_FLAG(broadcast_flood, BR_BCA
 BRPORT_ATTR_FLAG(neigh_suppress, BR_NEIGH_SUPPRESS);
 BRPORT_ATTR_FLAG(isolated, BR_ISOLATED);
 BRPORT_ATTR_FLAG(bpdu_filter, BR_BPDU_FILTER);
+BRPORT_ATTR_FLAG(offload, BR_OFFLOAD);
 
 #ifdef CONFIG_BRIDGE_IGMP_SNOOPING
 static ssize_t show_multicast_router(struct net_bridge_port *p, char *buf)
@@ -288,6 +289,7 @@ static const struct brport_attribute *br
 	&brport_attr_isolated,
 	&brport_attr_bpdu_filter,
 	&brport_attr_backup_port,
+	&brport_attr_offload,
 	NULL
 };
 
--- a/net/bridge/br_vlan_tunnel.c
+++ b/net/bridge/br_vlan_tunnel.c
@@ -15,6 +15,7 @@
 
 #include "br_private.h"
 #include "br_private_tunnel.h"
+#include "br_private_offload.h"
 
 static inline int br_vlan_tunid_cmp(struct rhashtable_compare_arg *arg,
 				    const void *ptr)
@@ -180,6 +181,7 @@ int br_handle_ingress_vlan_tunnel(struct
 	skb_dst_drop(skb);
 
 	__vlan_hwaccel_put_tag(skb, p->br->vlan_proto, vlan->vid);
+	br_offload_skb_disable(skb);
 
 	return 0;
 }
@@ -203,6 +205,7 @@ int br_handle_egress_vlan_tunnel(struct
 	if (err)
 		return err;
 
+	br_offload_skb_disable(skb);
 	tunnel_dst = rcu_dereference(vlan->tinfo.tunnel_dst);
 	if (tunnel_dst && dst_hold_safe(&tunnel_dst->dst))
 		skb_dst_set(skb, &tunnel_dst->dst);
