From 9a352062b7e3857742389dff6f64393481dc755e Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Thu, 23 Sep 2021 19:37:05 +0200
Subject: [PATCH] Revert "PCI: aardvark: Fix initialization with old Marvell's
 Arm Trusted Firmware"
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This reverts commit b0c6ae0f8948a2be6bf4e8b4bbab9ca1343289b6.

Armada 3720 phy driver (phy-mvebu-a3700-comphy.c) does not return
-EOPNOTSUPP from phy_power_on() callback anymore.

So remove dead code which handles -EOPNOTSUPP return value.

Signed-off-by: Pali Rohár <pali@kernel.org>
Signed-off-by: Marek Behún <kabel@kernel.org>
Acked-by: Miquel Raynal <miquel.raynal@bootlin.com>
---
 drivers/pci/controller/pci-aardvark.c | 4 +---
 1 file changed, 1 insertion(+), 3 deletions(-)

--- a/drivers/pci/controller/pci-aardvark.c
+++ b/drivers/pci/controller/pci-aardvark.c
@@ -1634,9 +1634,7 @@ static int advk_pcie_enable_phy(struct a
 	}
 
 	ret = phy_power_on(pcie->phy);
-	if (ret == -EOPNOTSUPP) {
-		dev_warn(&pcie->pdev->dev, "PHY unsupported by firmware\n");
-	} else if (ret) {
+	if (ret) {
 		phy_exit(pcie->phy);
 		return ret;
 	}
