From 84909e85881d67244240c9f40974ce12a51e3886 Mon Sep 17 00:00:00 2001
From: Ansuel Smith <ansuelsmth@gmail.com>
Date: Tue, 11 May 2021 23:09:45 +0200
Subject: [PATCH] ARM: dts: qcom: reduce pci IO size to 64K

The current value is probably a typo and is actually uncommon to find
1MB IO space even on a x86 arch. Also with recent changes to the pci
driver, pci1 and pci2 now fails to function as any connected device
fails any reg read/write. Reduce this to 64K as it should be more than
enough and 3 * 64K of total IO space doesn't exceed the IO_SPACE_LIMIT
hardcoded for the ARM arch.

Signed-off-by: Ansuel Smith <ansuelsmth@gmail.com>
---
 arch/arm/boot/dts/qcom-ipq8064.dtsi | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/arch/arm/boot/dts/qcom-ipq8064.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq8064.dtsi
@@ -1086,7 +1086,7 @@
 			#address-cells = <3>;
 			#size-cells = <2>;
 
-			ranges = <0x81000000 0 0x0fe00000 0x0fe00000 0 0x00100000   /* downstream I/O */
+			ranges = <0x81000000 0 0x0fe00000 0x0fe00000 0 0x00010000   /* downstream I/O */
 				  0x82000000 0 0x08000000 0x08000000 0 0x07e00000>; /* non-prefetchable memory */
 
 			interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
@@ -1137,7 +1137,7 @@
 			#address-cells = <3>;
 			#size-cells = <2>;
 
-			ranges = <0x81000000 0 0x31e00000 0x31e00000 0 0x00100000   /* downstream I/O */
+			ranges = <0x81000000 0 0x31e00000 0x31e00000 0 0x00010000   /* downstream I/O */
 				  0x82000000 0 0x2e000000 0x2e000000 0 0x03e00000>; /* non-prefetchable memory */
 
 			interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>;
@@ -1188,7 +1188,7 @@
 			#address-cells = <3>;
 			#size-cells = <2>;
 
-			ranges = <0x81000000 0 0x35e00000 0x35e00000 0 0x00100000   /* downstream I/O */
+			ranges = <0x81000000 0 0x35e00000 0x35e00000 0 0x00010000   /* downstream I/O */
 				  0x82000000 0 0x32000000 0x32000000 0 0x03e00000>; /* non-prefetchable memory */
 
 			interrupts = <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
