From 001f4261fe4d5ae710cf1f445b6cae6d9d3ae26e Mon Sep 17 00:00:00 2001
From: "Russell King (Oracle)" <rmk+kernel@armlinux.org.uk>
Date: Thu, 9 Dec 2021 13:11:48 +0000
Subject: [PATCH] net: phylink: use legacy_pre_march2020

Use the legacy flag to indicate whether we should operate in legacy
mode. This allows us to stop using the presence of a PCS as an
indicator to the age of the phylink user, and make PCS presence
optional.

Legacy mode involves:
1) calling mac_config() whenever the link comes up
2) calling mac_config() whenever the inband advertisement changes,
   possibly followed by a call to mac_an_restart()
3) making use of mac_an_restart()
4) making use of mac_pcs_get_state()

All the above functionality was moved to a seperate "PCS" block of
operations in March 2020.

Update the documents to indicate that the differences that this flag
makes.

Signed-off-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/phy/phylink.c | 12 ++++++------
 include/linux/phylink.h   | 17 +++++++++++++++++
 2 files changed, 23 insertions(+), 6 deletions(-)

--- a/drivers/net/phy/phylink.c
+++ b/drivers/net/phy/phylink.c
@@ -777,7 +777,7 @@ static void phylink_mac_pcs_an_restart(s
 	    phylink_autoneg_inband(pl->cur_link_an_mode)) {
 		if (pl->pcs_ops)
 			pl->pcs_ops->pcs_an_restart(pl->pcs);
-		else
+		else if (pl->config->legacy_pre_march2020)
 			pl->mac_ops->mac_an_restart(pl->config);
 	}
 }
@@ -855,7 +855,7 @@ static int phylink_change_inband_advert(
 	if (test_bit(PHYLINK_DISABLE_STOPPED, &pl->phylink_disable_state))
 		return 0;
 
-	if (!pl->pcs_ops) {
+	if (!pl->pcs_ops && pl->config->legacy_pre_march2020) {
 		/* Legacy method */
 		phylink_mac_config(pl, &pl->link_config);
 		phylink_mac_pcs_an_restart(pl);
@@ -900,7 +900,8 @@ static void phylink_mac_pcs_get_state(st
 
 	if (pl->pcs_ops)
 		pl->pcs_ops->pcs_get_state(pl->pcs, state);
-	else if (pl->mac_ops->mac_pcs_get_state)
+	else if (pl->mac_ops->mac_pcs_get_state &&
+		 pl->config->legacy_pre_march2020)
 		pl->mac_ops->mac_pcs_get_state(pl->config, state);
 	else
 		state->link = 0;
@@ -1094,12 +1095,11 @@ static void phylink_resolve(struct work_
 			}
 			phylink_major_config(pl, false, &link_state);
 			pl->link_config.interface = link_state.interface;
-		} else if (!pl->pcs_ops) {
+		} else if (!pl->pcs_ops && pl->config->legacy_pre_march2020) {
 			/* The interface remains unchanged, only the speed,
 			 * duplex or pause settings have changed. Call the
 			 * old mac_config() method to configure the MAC/PCS
-			 * only if we do not have a PCS installed (an
-			 * unconverted user.)
+			 * only if we do not have a legacy MAC driver.
 			 */
 			phylink_mac_config(pl, &link_state);
 		}
--- a/include/linux/phylink.h
+++ b/include/linux/phylink.h
@@ -208,6 +208,10 @@ struct phylink_pcs *mac_select_pcs(struc
  * negotiation completion state in @state->an_complete, and link up state
  * in @state->link. If possible, @state->lp_advertising should also be
  * populated.
+ *
+ * Note: This is a legacy method. This function will not be called unless
+ * legacy_pre_march2020 is set in &struct phylink_config and there is no
+ * PCS attached.
  */
 void mac_pcs_get_state(struct phylink_config *config,
 		       struct phylink_link_state *state);
@@ -248,6 +252,15 @@ int mac_prepare(struct phylink_config *c
  * guaranteed to be correct, and so any mac_config() implementation must
  * never reference these fields.
  *
+ * Note: For legacy March 2020 drivers (drivers with legacy_pre_march2020 set
+ * in their &phylnk_config and which don't have a PCS), this function will be
+ * called on each link up event, and to also change the in-band advert. For
+ * non-legacy drivers, it will only be called to reconfigure the MAC for a
+ * "major" change in e.g. interface mode. It will not be called for changes
+ * in speed, duplex or pause modes or to change the in-band advertisement.
+ * In any case, it is strongly preferred that speed, duplex and pause settings
+ * are handled in the mac_link_up() method and not in this method.
+ *
  * (this requires a rewrite - please refer to mac_link_up() for situations
  *  where the PCS and MAC are not tightly integrated.)
  *
@@ -332,6 +345,10 @@ int mac_finish(struct phylink_config *co
 /**
  * mac_an_restart() - restart 802.3z BaseX autonegotiation
  * @config: a pointer to a &struct phylink_config.
+ *
+ * Note: This is a legacy method. This function will not be called unless
+ * legacy_pre_march2020 is set in &struct phylink_config and there is no
+ * PCS attached.
  */
 void mac_an_restart(struct phylink_config *config);
 
