--- a/arch/arm/boot/dts/qcom-ipq8064-rb3011.dts
+++ b/arch/arm/boot/dts/qcom-ipq8064-rb3011.dts
@@ -24,73 +24,6 @@
 		device_type = "memory";
 	};
 
-	mdio0: mdio-0 {
-		status = "okay";
-		compatible = "virtual,mdio-gpio";
-		gpios = <&qcom_pinmux 1 GPIO_ACTIVE_HIGH>,
-			<&qcom_pinmux 0 GPIO_ACTIVE_HIGH>;
-		#address-cells = <1>;
-		#size-cells = <0>;
-
-		pinctrl-0 = <&mdio0_pins>;
-		pinctrl-names = "default";
-
-		switch0: switch@10 {
-			compatible = "qca,qca8337";
-			#address-cells = <1>;
-			#size-cells = <0>;
-
-			dsa,member = <0 0>;
-
-			pinctrl-0 = <&sw0_reset_pin>;
-			pinctrl-names = "default";
-
-			reset-gpios = <&qcom_pinmux 16 GPIO_ACTIVE_LOW>;
-			reg = <0x10>;
-
-			ports {
-				#address-cells = <1>;
-				#size-cells = <0>;
-
-				switch0cpu: port@0 {
-					reg = <0>;
-					label = "cpu";
-					ethernet = <&gmac0>;
-					phy-mode = "rgmii-id";
-					fixed-link {
-						speed = <1000>;
-						full-duplex;
-					};
-				};
-
-				port@1 {
-					reg = <1>;
-					label = "sw1";
-				};
-
-				port@2 {
-					reg = <2>;
-					label = "sw2";
-				};
-
-				port@3 {
-					reg = <3>;
-					label = "sw3";
-				};
-
-				port@4 {
-					reg = <4>;
-					label = "sw4";
-				};
-
-				port@5 {
-					reg = <5>;
-					label = "sw5";
-				};
-			};
-		};
-	};
-
 	mdio1: mdio-1 {
 		status = "okay";
 		compatible = "virtual,mdio-gpio";
@@ -216,6 +149,68 @@
 	};
 };
 
+&mdio0 {
+	status = "okay";
+
+	pinctrl-0 = <&mdio0_pins>;
+	pinctrl-names = "default";
+
+	switch0: switch@10 {
+		compatible = "qca,qca8337";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		dsa,member = <0 0>;
+
+		pinctrl-0 = <&sw0_reset_pin>;
+		pinctrl-names = "default";
+
+		reset-gpios = <&qcom_pinmux 16 GPIO_ACTIVE_LOW>;
+		reg = <0x10>;
+
+		ports {
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			switch0cpu: port@0 {
+				reg = <0>;
+				label = "cpu";
+				ethernet = <&gmac0>;
+				phy-mode = "rgmii-id";
+				fixed-link {
+					speed = <1000>;
+					full-duplex;
+				};
+			};
+
+			port@1 {
+				reg = <1>;
+				label = "sw1";
+			};
+
+			port@2 {
+				reg = <2>;
+				label = "sw2";
+			};
+
+			port@3 {
+				reg = <3>;
+				label = "sw3";
+			};
+
+			port@4 {
+				reg = <4>;
+				label = "sw4";
+			};
+
+			port@5 {
+				reg = <5>;
+				label = "sw5";
+			};
+		};
+	};
+};
+
 &gmac0 {
 	status = "okay";
 
