--- a/arch/mips/ath79/Kconfig
+++ b/arch/mips/ath79/Kconfig
@@ -240,6 +240,18 @@
 	select ATH79_DEV_M25P80
 	select ATH79_DEV_USB
 
+config ATH79_MACH_EW_DORIN
+	bool "embedded wireless Dorin Platform support"
+	select SOC_AR933X
+	select ATH79_DEV_M25P80
+	select ATH79_DEV_GPIO_BUTTONS
+	select ATH79_DEV_LEDS_GPIO
+	select ATH79_DEV_WMAC
+	select ATH79_DEV_ETH
+	help
+	  Say 'Y' here if you want your kernel to support the
+	  Dorin Platform from www.80211.de .
+
 config ATH79_MACH_JA76PF
 	bool "jjPlus JA76PF board support"
 	select SOC_AR71XX
--- a/arch/mips/ath79/machtypes.h
+++ b/arch/mips/ath79/machtypes.h
@@ -32,6 +32,7 @@
 	ATH79_MACH_DIR_615_C1,		/* D-Link DIR-615 rev. C1 */
 	ATH79_MACH_DIR_615_E4,		/* D-Link DIR-615 rev. E4 */
 	ATH79_MACH_DIR_825_B1,		/* D-Link DIR-825 rev. B1 */
+	ATH79_MACH_EW_DORIN,		/* embedded wireless Dorin Platform */
 	ATH79_MACH_EAP7660D,		/* Senao EAP7660D */
 	ATH79_MACH_JA76PF,		/* jjPlus JA76PF */
 	ATH79_MACH_JA76PF2,		/* jjPlus JA76PF2 */
--- a/arch/mips/ath79/Makefile
+++ b/arch/mips/ath79/Makefile
@@ -49,6 +49,7 @@
 obj-$(CONFIG_ATH79_MACH_DIR_600_A1)	+= mach-dir-600-a1.o
 obj-$(CONFIG_ATH79_MACH_DIR_615_C1)	+= mach-dir-615-c1.o
 obj-$(CONFIG_ATH79_MACH_DIR_825_B1)	+= mach-dir-825-b1.o
+obj-$(CONFIG_ATH79_MACH_EW_DORIN)	+= mach-ew-dorin.o
 obj-$(CONFIG_ATH79_MACH_EAP7660D)	+= mach-eap7660d.o
 obj-$(CONFIG_ATH79_MACH_JA76PF)		+= mach-ja76pf.o
 obj-$(CONFIG_ATH79_MACH_JWAP003)	+= mach-jwap003.o
