From 7971cef3f4036da74066aa4ca9b78fd1c9573a6c Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Thu, 16 Feb 2012 20:17:50 +0100
Subject: [PATCH 30/70] WDT: MIPS: lantiq: convert watchdog driver to clkdev
 api

Refrence the IO region clock via its new access function.

Signed-off-by: John Crispin <blogic@openwrt.org>
Cc: linux-watchdog@vger.kernel.org
---
 drivers/watchdog/lantiq_wdt.c |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

--- a/drivers/watchdog/lantiq_wdt.c
+++ b/drivers/watchdog/lantiq_wdt.c
@@ -206,7 +206,7 @@ ltq_wdt_probe(struct platform_device *pd
 	}
 
 	/* we do not need to enable the clock as it is always running */
-	clk = clk_get(&pdev->dev, "io");
+	clk = clk_get_io();
 	WARN_ON(!clk);
 	ltq_io_region_clk_rate = clk_get_rate(clk);
 	clk_put(clk);
