From 7ab075944587e4fe7e2688b1df85452e3d86edb5 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Tue, 21 Feb 2012 14:25:21 +0100
Subject: [PATCH 28/70] MIPS: lantiq: convert falcon debug uart to clkdev api

On Falcon SoCs we have a secondary serial port that can be used to help
debug the voice core. For the port to work several clocking bits need to
be activated. We convert the code to clkdev api.

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 arch/mips/lantiq/falcon/prom.c |    4 +---
 drivers/tty/serial/lantiq.c    |    7 ++++---
 2 files changed, 5 insertions(+), 6 deletions(-)

--- a/arch/mips/lantiq/falcon/prom.c
+++ b/arch/mips/lantiq/falcon/prom.c
@@ -43,10 +43,8 @@ ltq_soc_setup(void)
 	ltq_register_asc(0);
 	ltq_register_wdt();
 	falcon_register_gpio();
-	if (register_asc1) {
+	if (register_asc1)
 		ltq_register_asc(1);
-		ltq_sysctl_activate(SYSCTL_SYS1, ACTS_ASC1_ACT);
-	}
 }
 
 void __init
--- a/drivers/tty/serial/lantiq.c
+++ b/drivers/tty/serial/lantiq.c
@@ -117,6 +117,7 @@ static DEFINE_SPINLOCK(ltq_asc_lock);
 
 struct ltq_uart_port {
 	struct uart_port	port;
+	struct clk		*fpiclk;
 	struct clk		*clk;
 	unsigned int		tx_irq;
 	unsigned int		rx_irq;
@@ -319,7 +320,7 @@ lqasc_startup(struct uart_port *port)
 	struct ltq_uart_port *ltq_port = to_ltq_uart_port(port);
 	int retval;
 
-	port->uartclk = clk_get_rate(ltq_port->clk);
+	port->uartclk = clk_get_rate(ltq_port->fpiclk);
 
 	ltq_w32_mask(ASCCLC_DISS | ASCCLC_RMCMASK, (1 << ASCCLC_RMCOFFSET),
 		port->membase + LTQ_ASC_CLC);
@@ -646,7 +647,7 @@ lqasc_console_setup(struct console *co,
 
 	port = &ltq_port->port;
 
-	port->uartclk = clk_get_rate(ltq_port->clk);
+	port->uartclk = clk_get_rate(ltq_port->fpiclk);
 
 	if (options)
 		uart_parse_options(options, &baud, &parity, &bits, &flow);
@@ -731,7 +732,7 @@ lqasc_probe(struct platform_device *pdev
 	port->irq	= tx_irq; /* unused, just to be backward-compatibe */
 	port->mapbase	= mmres->start;
 
-	ltq_port->clk	= clk;
+	ltq_port->fpiclk = clk;
 
 	ltq_port->tx_irq = tx_irq;
 	ltq_port->rx_irq = rx_irq;
