From 66808f706b3dcd83a9f5157997ff478a880a2906 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Mon, 30 Apr 2012 09:10:51 +0200
Subject: [PATCH 70/79] MIPS: BCM63XX: Add board definition for D-Link
 DSL-274xB rev F1

---
 arch/mips/bcm63xx/boards/board_bcm963xx.c |  104 +++++++++++++++++++++++++++++
 1 files changed, 104 insertions(+), 0 deletions(-)

--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -195,6 +195,109 @@ static struct board_info __initdata boar
 
 	},
 };
+
+static struct board_info __initdata board_dsl_274xb_f1 = {
+	.name				= "AW4339U",
+	.expected_cpu_id		= 0x6328,
+
+	.has_uart0			= 1,
+	.has_pci			= 1,
+
+	.has_caldata			= 1,
+	.caldata = {
+		{
+			.caldata_offset	= 0x7d1000,
+			.slot		= 0,
+		},
+	},
+
+	.has_enetsw			= 1,
+
+	.enetsw = {
+		.used_ports = {
+			[0] = {
+				.used	= 1,
+				.phy_id = 1,
+				.name	= "Port 4",
+			},
+			[1] = {
+				.used	= 1,
+				.phy_id	= 2,
+				.name	= "Port 3",
+			},
+			[2] = {
+				.used	= 1,
+				.phy_id	= 3,
+				.name	= "Port 2",
+			},
+			[3] = {
+				.used	= 1,
+				.phy_id	= 4,
+				.name	= "Port 1",
+			},
+		},
+	},
+
+	.leds = {
+		{
+			.name		= "dsl-274xb:red:internet",
+			.gpio		= 2,
+			.active_low	= 1,
+		},
+		{
+			.name		= "dsl-274xb:green:dsl",
+			.gpio		= 3,
+			.active_low	= 1,
+		},
+		{
+			.name		= "dsl-274xb:green:power",
+			.gpio		= 4,
+			.active_low	= 1,
+			.default_trigger = "default-on",
+		},
+		{
+			.name		= "dsl-274xb:red:power",
+			.gpio		= 8,
+			.active_low	= 1,
+		},
+		{
+			.name		= "dsl-274xb:blue:wps",
+			.gpio		= 9,
+			.active_low	= 1,
+		},
+		{
+			.name		= "dsl-274xb:green:internet",
+			.gpio		= 11,
+			.active_low	= 1,
+		},
+	},
+
+	.buttons = {
+		{
+			.desc		= "wifi",
+			.gpio		= 10,
+			.active_low	= 1,
+			.type		= EV_KEY,
+			.code		= BTN_0,
+			.debounce_interval = BCM963XX_KEYS_DEBOUNCE_INTERVAL,
+		},
+		{
+			.desc		= "reset",
+			.gpio		= 23,
+			.active_low	= 1,
+			.type		= EV_KEY,
+			.code		= KEY_RESTART,
+			.debounce_interval = BCM963XX_KEYS_DEBOUNCE_INTERVAL,
+		},
+		{
+			.desc		= "wps",
+			.gpio		= 24,
+			.active_low	= 1,
+			.code		= KEY_WPS_BUTTON,
+			.debounce_interval = BCM963XX_KEYS_DEBOUNCE_INTERVAL,
+		},
+	},
+};
 #endif
 
 /*
@@ -2305,6 +2408,7 @@ static const struct board_info __initdat
 #ifdef CONFIG_BCM63XX_CPU_6328
 	&board_96328avng,
 	&board_963281TAN,
+	&board_dsl_274xb_f1,
 #endif
 #ifdef CONFIG_BCM63XX_CPU_6338
 	&board_96338gw,
