--- a/compat/Makefile
+++ b/compat/Makefile
@@ -44,8 +44,6 @@ compat-$(CONFIG_COMPAT_KERNEL_3_3) += \
 	flow_dissector.o
 compat-$(CONFIG_COMPAT_KERNEL_3_4) += compat-3.4.o
 
-compat-$(CONFIG_COMPAT_CORDIC) += cordic.o
-compat-$(CONFIG_COMPAT_CRC8) += crc8.o
 
 ifndef CONFIG_64BIT
 ifndef CONFIG_GENERIC_ATOMIC64
--- a/include/linux/cordic.h
+++ /dev/null
@@ -1,48 +0,0 @@
-/*
- * Copyright (c) 2011 Broadcom Corporation
- *
- * Permission to use, copy, modify, and/or distribute this software for any
- * purpose with or without fee is hereby granted, provided that the above
- * copyright notice and this permission notice appear in all copies.
- *
- * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
- * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
- * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
- * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
- * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
- * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
- * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
- */
-#ifndef __CORDIC_H_
-#define __CORDIC_H_
-
-#include <linux/types.h>
-
-/**
- * struct cordic_iq - i/q coordinate.
- *
- * @i: real part of coordinate (in phase).
- * @q: imaginary part of coordinate (quadrature).
- */
-struct cordic_iq {
-	s32 i;
-	s32 q;
-};
-
-/**
- * cordic_calc_iq() - calculates the i/q coordinate for given angle.
- *
- * @theta: angle in degrees for which i/q coordinate is to be calculated.
- * @coord: function output parameter holding the i/q coordinate.
- *
- * The function calculates the i/q coordinate for a given angle using
- * cordic algorithm. The coordinate consists of a real (i) and an
- * imaginary (q) part. The real part is essentially the cosine of the
- * angle and the imaginary part is the sine of the angle. The returned
- * values are scaled by 2^16 for precision. The range for theta is
- * for -180 degrees to +180 degrees. Passed values outside this range are
- * converted before doing the actual calculation.
- */
-struct cordic_iq cordic_calc_iq(s32 theta);
-
-#endif /* __CORDIC_H_ */
--- a/include/linux/crc8.h
+++ /dev/null
@@ -1,101 +0,0 @@
-/*
- * Copyright (c) 2011 Broadcom Corporation
- *
- * Permission to use, copy, modify, and/or distribute this software for any
- * purpose with or without fee is hereby granted, provided that the above
- * copyright notice and this permission notice appear in all copies.
- *
- * THE SOFTWARE IS PROVIDED "AS IS" AND THE AUTHOR DISCLAIMS ALL WARRANTIES
- * WITH REGARD TO THIS SOFTWARE INCLUDING ALL IMPLIED WARRANTIES OF
- * MERCHANTABILITY AND FITNESS. IN NO EVENT SHALL THE AUTHOR BE LIABLE FOR ANY
- * SPECIAL, DIRECT, INDIRECT, OR CONSEQUENTIAL DAMAGES OR ANY DAMAGES
- * WHATSOEVER RESULTING FROM LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION
- * OF CONTRACT, NEGLIGENCE OR OTHER TORTIOUS ACTION, ARISING OUT OF OR IN
- * CONNECTION WITH THE USE OR PERFORMANCE OF THIS SOFTWARE.
- */
-#ifndef __CRC8_H_
-#define __CRC8_H_
-
-#include <linux/types.h>
-
-/* see usage of this value in crc8() description */
-#define CRC8_INIT_VALUE		0xFF
-
-/*
- * Return value of crc8() indicating valid message+crc. This is true
- * if a CRC is inverted before transmission. The CRC computed over the
- * whole received bitstream is _table[x], where x is the bit pattern
- * of the modification (almost always 0xff).
- */
-#define CRC8_GOOD_VALUE(_table)	(_table[0xFF])
-
-/* required table size for crc8 algorithm */
-#define CRC8_TABLE_SIZE			256
-
-/* helper macro assuring right table size is used */
-#define DECLARE_CRC8_TABLE(_table) \
-	static u8 _table[CRC8_TABLE_SIZE]
-
-/**
- * crc8_populate_lsb - fill crc table for given polynomial in regular bit order.
- *
- * @table:	table to be filled.
- * @polynomial:	polynomial for which table is to be filled.
- *
- * This function fills the provided table according the polynomial provided for
- * regular bit order (lsb first). Polynomials in CRC algorithms are typically
- * represented as shown below.
- *
- *	poly = x^8 + x^7 + x^6 + x^4 + x^2 + 1
- *
- * For lsb first direction x^7 maps to the lsb. So the polynomial is as below.
- *
- * - lsb first: poly = 10101011(1) = 0xAB
- */
-void crc8_populate_lsb(u8 table[CRC8_TABLE_SIZE], u8 polynomial);
-
-/**
- * crc8_populate_msb - fill crc table for given polynomial in reverse bit order.
- *
- * @table:	table to be filled.
- * @polynomial:	polynomial for which table is to be filled.
- *
- * This function fills the provided table according the polynomial provided for
- * reverse bit order (msb first). Polynomials in CRC algorithms are typically
- * represented as shown below.
- *
- *	poly = x^8 + x^7 + x^6 + x^4 + x^2 + 1
- *
- * For msb first direction x^7 maps to the msb. So the polynomial is as below.
- *
- * - msb first: poly = (1)11010101 = 0xD5
- */
-void crc8_populate_msb(u8 table[CRC8_TABLE_SIZE], u8 polynomial);
-
-/**
- * crc8() - calculate a crc8 over the given input data.
- *
- * @table:	crc table used for calculation.
- * @pdata:	pointer to data buffer.
- * @nbytes:	number of bytes in data buffer.
- * @crc:	previous returned crc8 value.
- *
- * The CRC8 is calculated using the polynomial given in crc8_populate_msb()
- * or crc8_populate_lsb().
- *
- * The caller provides the initial value (either %CRC8_INIT_VALUE
- * or the previous returned value) to allow for processing of
- * discontiguous blocks of data.  When generating the CRC the
- * caller is responsible for complementing the final return value
- * and inserting it into the byte stream.  When validating a byte
- * stream (including CRC8), a final return value of %CRC8_GOOD_VALUE
- * indicates the byte stream data can be considered valid.
- *
- * Reference:
- * "A Painless Guide to CRC Error Detection Algorithms", ver 3, Aug 1993
- * Williams, Ross N., ross<at>ross.net
- * (see URL http://www.ross.net/crc/download/crc_v3.txt).
- */
-u8 crc8(const u8 table[CRC8_TABLE_SIZE], u8 *pdata, size_t nbytes, u8 crc);
-
-#endif /* __CRC8_H_ */
