From 55a43c346d24434e46ef7fcc09a9df8179c346e4 Mon Sep 17 00:00:00 2001
From: Heiko Stuebner <heiko@sntech.de>
Date: Sun, 16 Feb 2025 16:27:42 +0100
Subject: [PATCH] arm64: dts: rockchip: change rng reset id back to its
 constant value

With the binding header now providing the SCMI_SRST_H_TRNG_NS constant,
switch back to it from the temporary numeric value.

Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 arch/arm64/boot/dts/rockchip/rk3588-base.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/rockchip/rk3588-base.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588-base.dtsi
@@ -1768,7 +1768,7 @@
 		reg = <0x0 0xfe378000 0x0 0x200>;
 		interrupts = <GIC_SPI 400 IRQ_TYPE_LEVEL_HIGH 0>;
 		clocks = <&scmi_clk SCMI_HCLK_SECURE_NS>;
-		resets = <&scmi_reset 48>;
+		resets = <&scmi_reset SCMI_SRST_H_TRNG_NS>;
 	};
 
 	i2s0_8ch: i2s@fe470000 {
