From 88759af56f126e6e151f07fa9efc7447079fca9d Mon Sep 17 00:00:00 2001
From: Cheong2K <cheong@redbear.cc>
Date: Fri, 26 Feb 2016 18:20:10 +0800
Subject: [PATCH] brcmfmac: adds support for BCM43341 wifi

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c     | 3 ++-
 3 files changed, 4 insertions(+), 3 deletions(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/sdio.c
@@ -609,6 +609,7 @@ BRCMF_FW_DEF(4329, "brcmfmac4329-sdio");
 BRCMF_FW_DEF(4330, "brcmfmac4330-sdio");
 BRCMF_FW_DEF(4334, "brcmfmac4334-sdio");
 BRCMF_FW_DEF(43340, "brcmfmac43340-sdio");
+BRCMF_FW_DEF(43341, "brcmfmac43341-sdio");
 BRCMF_FW_DEF(4335, "brcmfmac4335-sdio");
 BRCMF_FW_DEF(43362, "brcmfmac43362-sdio");
 BRCMF_FW_DEF(4339, "brcmfmac4339-sdio");
@@ -641,7 +642,7 @@ static const struct brcmf_firmware_mappi
 	BRCMF_FW_ENTRY(BRCM_CC_4330_CHIP_ID, 0xFFFFFFFF, 4330),
 	BRCMF_FW_ENTRY(BRCM_CC_4334_CHIP_ID, 0xFFFFFFFF, 4334),
 	BRCMF_FW_ENTRY(BRCM_CC_43340_CHIP_ID, 0xFFFFFFFF, 43340),
-	BRCMF_FW_ENTRY(BRCM_CC_43341_CHIP_ID, 0xFFFFFFFF, 43340),
+	BRCMF_FW_ENTRY(BRCM_CC_43341_CHIP_ID, 0xFFFFFFFF, 43341),
 	BRCMF_FW_ENTRY(BRCM_CC_4335_CHIP_ID, 0xFFFFFFFF, 4335),
 	BRCMF_FW_ENTRY(BRCM_CC_43362_CHIP_ID, 0xFFFFFFFE, 43362),
 	BRCMF_FW_ENTRY(BRCM_CC_4339_CHIP_ID, 0xFFFFFFFF, 4339),
