From 68604e89335ccb3e893b5a05b2c0d5cd2eaaf6ec Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Petr=20=C5=A0tetiar?= <ynezz@true.cz>
Date: Tue, 3 Mar 2020 15:14:40 +0100
Subject: [PATCH] ARM: dts: imx6q-apalis: ixora: add status LEDs aliases
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Petr Štetiar <ynezz@true.cz>
---
 arch/arm/boot/dts/imx6q-apalis-ixora-v1.1.dts | 16 ++++++++++------
 arch/arm/boot/dts/imx6q-apalis-ixora.dts      | 12 ++++++++----
 2 files changed, 18 insertions(+), 10 deletions(-)

--- a/arch/arm/boot/dts/imx6q-apalis-ixora.dts
+++ b/arch/arm/boot/dts/imx6q-apalis-ixora.dts
@@ -24,6 +24,10 @@
 		i2c2 = &i2c2;
 		rtc0 = &rtc_i2c;
 		rtc1 = &snvs_rtc;
+		led-boot = &led_boot;
+		led-failsafe = &led_failsafe;
+		led-running = &led_running;
+		led-upgrade = &led_upgrade;
 	};
 
 	chosen {
@@ -35,22 +39,22 @@
 		pinctrl-names = "default";
 		pinctrl-0 = <&pinctrl_leds_ixora>;
 
-		led4-green {
+		led_running: led4-green {
 			gpios = <&gpio1 17 GPIO_ACTIVE_HIGH>;
 			label = "LED_4_GREEN";
 		};
 
-		led4-red {
+		led_upgrade: led4-red {
 			gpios = <&gpio1 21 GPIO_ACTIVE_HIGH>;
 			label = "LED_4_RED";
 		};
 
-		led5-green {
+		led_boot: led5-green {
 			gpios = <&gpio2 1 GPIO_ACTIVE_HIGH>;
 			label = "LED_5_GREEN";
 		};
 
-		led5-red {
+		led_failsafe: led5-red {
 			gpios = <&gpio2 2 GPIO_ACTIVE_HIGH>;
 			label = "LED_5_RED";
 		};
--- a/arch/arm/boot/dts/imx6q-apalis-ixora-v1.2.dts
+++ b/arch/arm/boot/dts/imx6q-apalis-ixora-v1.2.dts
@@ -24,6 +24,10 @@
 		i2c2 = &i2c2;
 		rtc0 = &rtc_i2c;
 		rtc1 = &snvs_rtc;
+		led-boot = &led_boot;
+		led-failsafe = &led_failsafe;
+		led-running = &led_running;
+		led-upgrade = &led_upgrade;
 	};
 
 	chosen {
@@ -36,22 +40,22 @@
 		pinctrl-names = "default";
 		pinctrl-0 = <&pinctrl_leds_ixora>;
 
-		led4-green {
-			gpios = <&gpio1 14 GPIO_ACTIVE_HIGH>;
+		led_running: led4-green {
+			gpios = <&gpio1 17 GPIO_ACTIVE_HIGH>;
 			label = "LED_4_GREEN";
 		};
 
-		led4-red {
-			gpios = <&gpio1 12 GPIO_ACTIVE_HIGH>;
+		led_upgrade: led4-red {
+			gpios = <&gpio1 21 GPIO_ACTIVE_HIGH>;
 			label = "LED_4_RED";
 		};
 
-		led5-green {
+		led_boot: led5-green {
 			gpios = <&gpio2 1 GPIO_ACTIVE_HIGH>;
 			label = "LED_5_GREEN";
 		};
 
-		led5-red {
+		led_failsafe: led5-red {
 			gpios = <&gpio2 2 GPIO_ACTIVE_HIGH>;
 			label = "LED_5_RED";
 		};
