From: qizhong cheng <qizhong.cheng@mediatek.com>
Date: Mon, 27 Dec 2021 21:31:10 +0800
Subject: [PATCH] PCI: mediatek: Assert PERST# for 100ms for power and clock to
 stabilize
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Described in PCIe CEM specification sections 2.2 (PERST# Signal) and
2.2.1 (Initial Power-Up (G3 to S0)). The deassertion of PERST# should
be delayed 100ms (TPVPERL) for the power and clock to become stable.

Link: https://lore.kernel.org/r/20211227133110.14500-1-qizhong.cheng@mediatek.com
Signed-off-by: qizhong cheng <qizhong.cheng@mediatek.com>
Signed-off-by: Lorenzo Pieralisi <lorenzo.pieralisi@arm.com>
Acked-by: Pali Rohár <pali@kernel.org>
---

--- a/drivers/pci/controller/pcie-mediatek.c
+++ b/drivers/pci/controller/pcie-mediatek.c
@@ -708,6 +708,13 @@ static int mtk_pcie_startup_port_v2(stru
 	 */
 	msleep(100);
 
+	/*
+	 * Described in PCIe CEM specification sections 2.2 (PERST# Signal) and
+	 * 2.2.1 (Initial Power-Up (G3 to S0)). The deassertion of PERST# should
+	 * be delayed 100ms (TPVPERL) for the power and clock to become stable.
+	 */
+	msleep(100);
+
 	/* De-assert PHY, PE, PIPE, MAC and configuration reset	*/
 	val = readl(port->base + PCIE_RST_CTRL);
 	val |= PCIE_PHY_RSTB | PCIE_PERSTB | PCIE_PIPE_SRSTB |
