From 5d9075ed7e73dc6ccebf78710c78f39ddc2dd78e Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Mon, 8 Jan 2024 11:42:57 +0000
Subject: [PATCH] spi: bcm2835: Support spi0-0cs and SPI_NO_CS mode

The forced conversion of native CS lines into software CS lines is done
whether or not the controller has been given any CS lines to use. This
breaks the use of the spi0-0cs overlay to prevent SPI from claiming any
CS lines, particularly with spidev which doesn't pass in the SPI_NO_CS
flag at creation.

Use the presence of an empty cs-gpios property as an indication that no
CS lines should be used, bypassing the native CS conversion code.

See: https://github.com/raspberrypi/linux/issues/5835

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 drivers/spi/spi-bcm2835.c | 5 +++++
 1 file changed, 5 insertions(+)

--- a/drivers/spi/spi-bcm2835.c
+++ b/drivers/spi/spi-bcm2835.c
@@ -1222,6 +1222,7 @@ static int bcm2835_spi_setup(struct spi_
 	struct bcm2835_spi *bs = spi_controller_get_devdata(ctlr);
 	struct bcm2835_spidev *slv = spi_get_ctldata(spi);
 	struct gpio_chip *chip;
+	int len;
 	int ret;
 	u32 cs;
 
@@ -1287,6 +1288,10 @@ static int bcm2835_spi_setup(struct spi_
 		goto err_cleanup;
 	}
 
+	/* Skip forced CS conversion if controller has an empty cs-gpios property */
+	if (of_find_property(ctlr->dev.of_node, "cs-gpios", &len) && len == 0)
+		return 0;
+
 	/*
 	 * Translate native CS to GPIO
 	 *
