From 9a02d66b0515d987037d0229b99367412b9eb38c Mon Sep 17 00:00:00 2001
From: Emil Renner Berthing <emil.renner.berthing@canonical.com>
Date: Thu, 18 May 2023 18:12:25 +0800
Subject: [PATCH 052/122] clk: starfive: Add StarFive JH7110 System-Top-Group
 clock driver

Add driver for the StarFive JH7110 System-Top-Group clock controller.

Co-developed-by: Xingyu Wu <xingyu.wu@starfivetech.com>
Signed-off-by: Xingyu Wu <xingyu.wu@starfivetech.com>
Signed-off-by: Emil Renner Berthing <emil.renner.berthing@canonical.com>
---
 drivers/clk/starfive/Kconfig                  |  11 ++
 drivers/clk/starfive/Makefile                 |   1 +
 .../clk/starfive/clk-starfive-jh7110-stg.c    | 173 ++++++++++++++++++
 3 files changed, 185 insertions(+)
 create mode 100644 drivers/clk/starfive/clk-starfive-jh7110-stg.c

--- a/drivers/clk/starfive/Kconfig
+++ b/drivers/clk/starfive/Kconfig
@@ -51,3 +51,14 @@ config CLK_STARFIVE_JH7110_AON
 	help
 	  Say yes here to support the always-on clock controller on the
 	  StarFive JH7110 SoC.
+
+config CLK_STARFIVE_JH7110_STG
+	tristate "StarFive JH7110 System-Top-Group clock support"
+	depends on CLK_STARFIVE_JH7110_SYS
+	select AUXILIARY_BUS
+	select CLK_STARFIVE_JH71X0
+	select RESET_STARFIVE_JH7110
+	default m if ARCH_STARFIVE
+	help
+	  Say yes here to support the System-Top-Group clock controller
+	  on the StarFive JH7110 SoC.
--- a/drivers/clk/starfive/Makefile
+++ b/drivers/clk/starfive/Makefile
@@ -7,3 +7,4 @@ obj-$(CONFIG_CLK_STARFIVE_JH7100_AUDIO)
 obj-$(CONFIG_CLK_STARFIVE_JH7110_PLL)	+= clk-starfive-jh7110-pll.o
 obj-$(CONFIG_CLK_STARFIVE_JH7110_SYS)	+= clk-starfive-jh7110-sys.o
 obj-$(CONFIG_CLK_STARFIVE_JH7110_AON)	+= clk-starfive-jh7110-aon.o
+obj-$(CONFIG_CLK_STARFIVE_JH7110_STG)	+= clk-starfive-jh7110-stg.o
--- /dev/null
+++ b/drivers/clk/starfive/clk-starfive-jh7110-stg.c
@@ -0,0 +1,173 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * StarFive JH7110 System-Top-Group Clock Driver
+ *
+ * Copyright (C) 2022 Emil Renner Berthing <kernel@esmil.dk>
+ * Copyright (C) 2022 StarFive Technology Co., Ltd.
+ */
+
+#include <linux/clk-provider.h>
+#include <linux/io.h>
+#include <linux/platform_device.h>
+
+#include <dt-bindings/clock/starfive,jh7110-crg.h>
+
+#include "clk-starfive-jh7110.h"
+
+/* external clocks */
+#define JH7110_STGCLK_OSC			(JH7110_STGCLK_END + 0)
+#define JH7110_STGCLK_HIFI4_CORE		(JH7110_STGCLK_END + 1)
+#define JH7110_STGCLK_STG_AXIAHB		(JH7110_STGCLK_END + 2)
+#define JH7110_STGCLK_USB_125M			(JH7110_STGCLK_END + 3)
+#define JH7110_STGCLK_CPU_BUS			(JH7110_STGCLK_END + 4)
+#define JH7110_STGCLK_HIFI4_AXI			(JH7110_STGCLK_END + 5)
+#define JH7110_STGCLK_NOCSTG_BUS		(JH7110_STGCLK_END + 6)
+#define JH7110_STGCLK_APB_BUS			(JH7110_STGCLK_END + 7)
+#define JH7110_STGCLK_EXT_END			(JH7110_STGCLK_END + 8)
+
+static const struct jh71x0_clk_data jh7110_stgclk_data[] = {
+	/* hifi4 */
+	JH71X0_GATE(JH7110_STGCLK_HIFI4_CLK_CORE, "hifi4_clk_core", 0,
+		    JH7110_STGCLK_HIFI4_CORE),
+	/* usb */
+	JH71X0_GATE(JH7110_STGCLK_USB0_APB, "usb0_apb", 0, JH7110_STGCLK_APB_BUS),
+	JH71X0_GATE(JH7110_STGCLK_USB0_UTMI_APB, "usb0_utmi_apb", 0, JH7110_STGCLK_APB_BUS),
+	JH71X0_GATE(JH7110_STGCLK_USB0_AXI, "usb0_axi", 0, JH7110_STGCLK_STG_AXIAHB),
+	JH71X0_GDIV(JH7110_STGCLK_USB0_LPM, "usb0_lpm", 0, 2, JH7110_STGCLK_OSC),
+	JH71X0_GDIV(JH7110_STGCLK_USB0_STB, "usb0_stb", 0, 4, JH7110_STGCLK_OSC),
+	JH71X0_GATE(JH7110_STGCLK_USB0_APP_125, "usb0_app_125", 0, JH7110_STGCLK_USB_125M),
+	JH71X0__DIV(JH7110_STGCLK_USB0_REFCLK, "usb0_refclk", 2, JH7110_STGCLK_OSC),
+	/* pci-e */
+	JH71X0_GATE(JH7110_STGCLK_PCIE0_AXI_MST0, "pcie0_axi_mst0", 0,
+		    JH7110_STGCLK_STG_AXIAHB),
+	JH71X0_GATE(JH7110_STGCLK_PCIE0_APB, "pcie0_apb", 0, JH7110_STGCLK_APB_BUS),
+	JH71X0_GATE(JH7110_STGCLK_PCIE0_TL, "pcie0_tl", 0, JH7110_STGCLK_STG_AXIAHB),
+	JH71X0_GATE(JH7110_STGCLK_PCIE1_AXI_MST0, "pcie1_axi_mst0", 0,
+		    JH7110_STGCLK_STG_AXIAHB),
+	JH71X0_GATE(JH7110_STGCLK_PCIE1_APB, "pcie1_apb", 0, JH7110_STGCLK_APB_BUS),
+	JH71X0_GATE(JH7110_STGCLK_PCIE1_TL, "pcie1_tl", 0, JH7110_STGCLK_STG_AXIAHB),
+	JH71X0_GATE(JH7110_STGCLK_PCIE_SLV_MAIN, "pcie_slv_main", CLK_IS_CRITICAL,
+		    JH7110_STGCLK_STG_AXIAHB),
+	/* security */
+	JH71X0_GATE(JH7110_STGCLK_SEC_AHB, "sec_ahb", 0, JH7110_STGCLK_STG_AXIAHB),
+	JH71X0_GATE(JH7110_STGCLK_SEC_MISC_AHB, "sec_misc_ahb", 0, JH7110_STGCLK_STG_AXIAHB),
+	/* stg mtrx */
+	JH71X0_GATE(JH7110_STGCLK_GRP0_MAIN, "mtrx_grp0_main", CLK_IS_CRITICAL,
+		    JH7110_STGCLK_CPU_BUS),
+	JH71X0_GATE(JH7110_STGCLK_GRP0_BUS, "mtrx_grp0_bus", CLK_IS_CRITICAL,
+		    JH7110_STGCLK_NOCSTG_BUS),
+	JH71X0_GATE(JH7110_STGCLK_GRP0_STG, "mtrx_grp0_stg", CLK_IS_CRITICAL,
+		    JH7110_STGCLK_STG_AXIAHB),
+	JH71X0_GATE(JH7110_STGCLK_GRP1_MAIN, "mtrx_grp1_main", CLK_IS_CRITICAL,
+		    JH7110_STGCLK_CPU_BUS),
+	JH71X0_GATE(JH7110_STGCLK_GRP1_BUS, "mtrx_grp1_bus", CLK_IS_CRITICAL,
+		    JH7110_STGCLK_NOCSTG_BUS),
+	JH71X0_GATE(JH7110_STGCLK_GRP1_STG, "mtrx_grp1_stg", CLK_IS_CRITICAL,
+		    JH7110_STGCLK_STG_AXIAHB),
+	JH71X0_GATE(JH7110_STGCLK_GRP1_HIFI, "mtrx_grp1_hifi", CLK_IS_CRITICAL,
+		    JH7110_STGCLK_HIFI4_AXI),
+	/* e24_rvpi */
+	JH71X0_GDIV(JH7110_STGCLK_E2_RTC, "e2_rtc", 0, 24, JH7110_STGCLK_OSC),
+	JH71X0_GATE(JH7110_STGCLK_E2_CORE, "e2_core", 0, JH7110_STGCLK_STG_AXIAHB),
+	JH71X0_GATE(JH7110_STGCLK_E2_DBG, "e2_dbg", 0, JH7110_STGCLK_STG_AXIAHB),
+	/* dw_sgdma1p */
+	JH71X0_GATE(JH7110_STGCLK_DMA1P_AXI, "dma1p_axi", 0, JH7110_STGCLK_STG_AXIAHB),
+	JH71X0_GATE(JH7110_STGCLK_DMA1P_AHB, "dma1p_ahb", 0, JH7110_STGCLK_STG_AXIAHB),
+};
+
+static struct clk_hw *jh7110_stgclk_get(struct of_phandle_args *clkspec, void *data)
+{
+	struct jh71x0_clk_priv *priv = data;
+	unsigned int idx = clkspec->args[0];
+
+	if (idx < JH7110_STGCLK_END)
+		return &priv->reg[idx].hw;
+
+	return ERR_PTR(-EINVAL);
+}
+
+static int jh7110_stgcrg_probe(struct platform_device *pdev)
+{
+	struct jh71x0_clk_priv *priv;
+	unsigned int idx;
+	int ret;
+
+	priv = devm_kzalloc(&pdev->dev, struct_size(priv, reg, JH7110_STGCLK_END),
+			    GFP_KERNEL);
+	if (!priv)
+		return -ENOMEM;
+
+	spin_lock_init(&priv->rmw_lock);
+	priv->dev = &pdev->dev;
+	priv->base = devm_platform_ioremap_resource(pdev, 0);
+	if (IS_ERR(priv->base))
+		return PTR_ERR(priv->base);
+
+	for (idx = 0; idx < JH7110_STGCLK_END; idx++) {
+		u32 max = jh7110_stgclk_data[idx].max;
+		struct clk_parent_data parents[4] = {};
+		struct clk_init_data init = {
+			.name = jh7110_stgclk_data[idx].name,
+			.ops = starfive_jh71x0_clk_ops(max),
+			.parent_data = parents,
+			.num_parents =
+				((max & JH71X0_CLK_MUX_MASK) >> JH71X0_CLK_MUX_SHIFT) + 1,
+			.flags = jh7110_stgclk_data[idx].flags,
+		};
+		struct jh71x0_clk *clk = &priv->reg[idx];
+		const char *fw_name[JH7110_STGCLK_EXT_END - JH7110_STGCLK_END] = {
+			"osc",
+			"hifi4_core",
+			"stg_axiahb",
+			"usb_125m",
+			"cpu_bus",
+			"hifi4_axi",
+			"nocstg_bus",
+			"apb_bus"
+		};
+		unsigned int i;
+
+		for (i = 0; i < init.num_parents; i++) {
+			unsigned int pidx = jh7110_stgclk_data[idx].parents[i];
+
+			if (pidx < JH7110_STGCLK_END)
+				parents[i].hw = &priv->reg[pidx].hw;
+			else if (pidx < JH7110_STGCLK_EXT_END)
+				parents[i].fw_name = fw_name[pidx - JH7110_STGCLK_END];
+		}
+
+		clk->hw.init = &init;
+		clk->idx = idx;
+		clk->max_div = max & JH71X0_CLK_DIV_MASK;
+
+		ret = devm_clk_hw_register(&pdev->dev, &clk->hw);
+		if (ret)
+			return ret;
+	}
+
+	ret = devm_of_clk_add_hw_provider(&pdev->dev, jh7110_stgclk_get, priv);
+	if (ret)
+		return ret;
+
+	return jh7110_reset_controller_register(priv, "rst-stg", 2);
+}
+
+static const struct of_device_id jh7110_stgcrg_match[] = {
+	{ .compatible = "starfive,jh7110-stgcrg" },
+	{ /* sentinel */ }
+};
+MODULE_DEVICE_TABLE(of, jh7110_stgcrg_match);
+
+static struct platform_driver jh7110_stgcrg_driver = {
+	.probe = jh7110_stgcrg_probe,
+	.driver = {
+		.name = "clk-starfive-jh7110-stg",
+		.of_match_table = jh7110_stgcrg_match,
+	},
+};
+module_platform_driver(jh7110_stgcrg_driver);
+
+MODULE_AUTHOR("Xingyu Wu <xingyu.wu@starfivetech.com>");
+MODULE_AUTHOR("Emil Renner Berthing <kernel@esmil.dk>");
+MODULE_DESCRIPTION("StarFive JH7110 System-Top-Group clock driver");
+MODULE_LICENSE("GPL");
