From 5148d8f41352d28fac3752c7aa116fd213e50c98 Mon Sep 17 00:00:00 2001
From: David Plowman <david.plowman@raspberrypi.com>
Date: Tue, 10 Jan 2023 13:14:27 +0000
Subject: [PATCH] drivers: media: i2c: imx708: Fix crop information

The 1536x864 mode contained incorrect crop information.

Signed-off-by: David Plowman <david.plowman@raspberrypi.com>
---
 drivers/media/i2c/imx708.c | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

--- a/drivers/media/i2c/imx708.c
+++ b/drivers/media/i2c/imx708.c
@@ -673,10 +673,10 @@ static const struct imx708_mode supporte
 		.height = 864,
 		.line_length_pix = 0x1460,
 		.crop = {
-			.left = IMX708_PIXEL_ARRAY_LEFT,
-			.top = IMX708_PIXEL_ARRAY_TOP,
-			.width = 4608,
-			.height = 2592,
+			.left = IMX708_PIXEL_ARRAY_LEFT + 768,
+			.top = IMX708_PIXEL_ARRAY_TOP + 432,
+			.width = 3072,
+			.height = 1728,
 		},
 		.vblank_min = 40,
 		.vblank_default = 2755,
