From 505f9c8653fc218ca47a153ec58ebc16bef5502f Mon Sep 17 00:00:00 2001
From: Mantas Pucka <mantas@8devices.com>
Date: Tue, 16 Jan 2024 10:42:40 +0200
Subject: [PATCH 16/19] remoteproc: q6v5_wcss: change ssr name for ipq6018 wifi
 subsystem

On IPQ6018 this string ends up being sent to RPM when remoteproc stops
(on crash or rmmod ath11k). "q6wcss" is not a valid name (not found by
`strings` in rpm.mbn), so this causes RPM do 'something' (presumably crash)
causing a system reboot followed by hang in XBL, with no WDT running.
Let's change ssr_name to a more sensible 'wcnss', that does not cause such
issues.

Signed-off-by: Mantas Pucka <mantas@8devices.com>
---
 drivers/remoteproc/qcom_q6v5_wcss.c | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/drivers/remoteproc/qcom_q6v5_wcss.c
+++ b/drivers/remoteproc/qcom_q6v5_wcss.c
@@ -1143,8 +1143,8 @@ static int q6v5_wcss_probe(struct platfo
 	if (ret)
 		goto free_rproc;
 
-	qcom_add_glink_subdev(rproc, &wcss->glink_subdev, "q6wcss");
-	qcom_add_ssr_subdev(rproc, &wcss->ssr_subdev, "q6wcss");
+	qcom_add_glink_subdev(rproc, &wcss->glink_subdev, desc->ssr_name);
+	qcom_add_ssr_subdev(rproc, &wcss->ssr_subdev, desc->ssr_name);
 
 	if (desc->ssctl_id)
 		wcss->sysmon = qcom_add_sysmon_subdev(rproc,
@@ -1201,7 +1201,7 @@ static const struct wcss_data wcss_ipq60
 	.aon_reset_required = true,
 	.wcss_q6_reset_required = true,
 	.bcr_reset_required = false,
-	.ssr_name = "q6wcss",
+	.ssr_name = "wcnss",
 	.ops = &q6v5_wcss_ipq8074_ops,
 	.requires_force_stop = true,
 	.need_mem_protection = true,
