From ee990c664fad993275b2615d0ff06af5d04922f0 Mon Sep 17 00:00:00 2001
From: William Qiu <william.qiu@starfivetech.com>
Date: Wed, 15 Feb 2023 19:32:47 +0800
Subject: [PATCH 108/122] mmc: starfive: Add sdio/emmc driver support

Add sdio/emmc driver support for StarFive JH7110 soc.

Tested-by: Conor Dooley <conor.dooley@microchip.com>
Signed-off-by: William Qiu <william.qiu@starfivetech.com>
---
 MAINTAINERS                        |   6 +
 drivers/mmc/host/Kconfig           |  10 ++
 drivers/mmc/host/Makefile          |   1 +
 drivers/mmc/host/dw_mmc-starfive.c | 186 +++++++++++++++++++++++++++++
 4 files changed, 203 insertions(+)
 create mode 100644 drivers/mmc/host/dw_mmc-starfive.c

--- a/MAINTAINERS
+++ b/MAINTAINERS
@@ -19664,6 +19664,12 @@ S:	Maintained
 F:	Documentation/devicetree/bindings/net/starfive,jh7110-dwmac.yaml
 F:	drivers/net/ethernet/stmicro/stmmac/dwmac-starfive.c
 
+STARFIVE JH7110 MMC/SD/SDIO DRIVER
+M:	William Qiu <william.qiu@starfivetech.com>
+S:	Supported
+F:	Documentation/devicetree/bindings/mmc/starfive*
+F:	drivers/mmc/host/dw_mmc-starfive.c
+
 STARFIVE JH7110 PLL CLOCK DRIVER
 M:	Xingyu Wu <xingyu.wu@starfivetech.com>
 S:	Supported
--- a/drivers/mmc/host/Kconfig
+++ b/drivers/mmc/host/Kconfig
@@ -872,6 +872,16 @@ config MMC_DW_ROCKCHIP
 	  Synopsys DesignWare Memory Card Interface driver. Select this option
 	  for platforms based on RK3066, RK3188 and RK3288 SoC's.
 
+config MMC_DW_STARFIVE
+	tristate "StarFive specific extensions for Synopsys DW Memory Card Interface"
+	depends on SOC_STARFIVE
+	depends on MMC_DW
+	select MMC_DW_PLTFM
+	help
+	  This selects support for StarFive JH7110 SoC specific extensions to the
+	  Synopsys DesignWare Memory Card Interface driver. Select this option
+	  for platforms based on StarFive JH7110 SoC.
+
 config MMC_SH_MMCIF
 	tristate "SuperH Internal MMCIF support"
 	depends on SUPERH || ARCH_RENESAS || COMPILE_TEST
--- a/drivers/mmc/host/Makefile
+++ b/drivers/mmc/host/Makefile
@@ -56,6 +56,7 @@ obj-$(CONFIG_MMC_DW_HI3798CV200) += dw_m
 obj-$(CONFIG_MMC_DW_K3)		+= dw_mmc-k3.o
 obj-$(CONFIG_MMC_DW_PCI)	+= dw_mmc-pci.o
 obj-$(CONFIG_MMC_DW_ROCKCHIP)	+= dw_mmc-rockchip.o
+obj-$(CONFIG_MMC_DW_STARFIVE)	+= dw_mmc-starfive.o
 obj-$(CONFIG_MMC_SH_MMCIF)	+= sh_mmcif.o
 obj-$(CONFIG_MMC_JZ4740)	+= jz4740_mmc.o
 obj-$(CONFIG_MMC_VUB300)	+= vub300.o
--- /dev/null
+++ b/drivers/mmc/host/dw_mmc-starfive.c
@@ -0,0 +1,186 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * StarFive Designware Mobile Storage Host Controller Driver
+ *
+ * Copyright (c) 2022 StarFive Technology Co., Ltd.
+ */
+
+#include <linux/clk.h>
+#include <linux/delay.h>
+#include <linux/mfd/syscon.h>
+#include <linux/mmc/host.h>
+#include <linux/module.h>
+#include <linux/of_address.h>
+#include <linux/platform_device.h>
+#include <linux/regmap.h>
+
+#include "dw_mmc.h"
+#include "dw_mmc-pltfm.h"
+
+#define ALL_INT_CLR		0x1ffff
+#define MAX_DELAY_CHAIN		32
+
+struct starfive_priv {
+	struct device *dev;
+	struct regmap *reg_syscon;
+	u32 syscon_offset;
+	u32 syscon_shift;
+	u32 syscon_mask;
+};
+
+static void dw_mci_starfive_set_ios(struct dw_mci *host, struct mmc_ios *ios)
+{
+	int ret;
+	unsigned int clock;
+
+	if (ios->timing == MMC_TIMING_MMC_DDR52 || ios->timing == MMC_TIMING_UHS_DDR50) {
+		clock = (ios->clock > 50000000 && ios->clock <= 52000000) ? 100000000 : ios->clock;
+		ret = clk_set_rate(host->ciu_clk, clock);
+		if (ret)
+			dev_dbg(host->dev, "Use an external frequency divider %uHz\n", ios->clock);
+		host->bus_hz = clk_get_rate(host->ciu_clk);
+	} else {
+		dev_dbg(host->dev, "Using the internal divider\n");
+	}
+}
+
+static int dw_mci_starfive_execute_tuning(struct dw_mci_slot *slot,
+					     u32 opcode)
+{
+	static const int grade  = MAX_DELAY_CHAIN;
+	struct dw_mci *host = slot->host;
+	struct starfive_priv *priv = host->priv;
+	int rise_point = -1, fall_point = -1;
+	int err, prev_err;
+	int i;
+	bool found = 0;
+	u32 regval;
+
+	/*
+	 * Use grade as the max delay chain, and use the rise_point and
+	 * fall_point to ensure the best sampling point of a data input
+	 * signals.
+	 */
+	for (i = 0; i < grade; i++) {
+		regval = i << priv->syscon_shift;
+		err = regmap_update_bits(priv->reg_syscon, priv->syscon_offset,
+						priv->syscon_mask, regval);
+		if (err)
+			return err;
+		mci_writel(host, RINTSTS, ALL_INT_CLR);
+
+		err = mmc_send_tuning(slot->mmc, opcode, NULL);
+		if (!err)
+			found = 1;
+
+		if (i > 0) {
+			if (err && !prev_err)
+				fall_point = i - 1;
+			if (!err && prev_err)
+				rise_point = i;
+		}
+
+		if (rise_point != -1 && fall_point != -1)
+			goto tuning_out;
+
+		prev_err = err;
+		err = 0;
+	}
+
+tuning_out:
+	if (found) {
+		if (rise_point == -1)
+			rise_point = 0;
+		if (fall_point == -1)
+			fall_point = grade - 1;
+		if (fall_point < rise_point) {
+			if ((rise_point + fall_point) >
+			    (grade - 1))
+				i = fall_point / 2;
+			else
+				i = (rise_point + grade - 1) / 2;
+		} else {
+			i = (rise_point + fall_point) / 2;
+		}
+
+		regval = i << priv->syscon_shift;
+		err = regmap_update_bits(priv->reg_syscon, priv->syscon_offset,
+						priv->syscon_mask, regval);
+		if (err)
+			return err;
+		mci_writel(host, RINTSTS, ALL_INT_CLR);
+
+		dev_info(host->dev, "Found valid delay chain! use it [delay=%d]\n", i);
+	} else {
+		dev_err(host->dev, "No valid delay chain! use default\n");
+		err = -EINVAL;
+	}
+
+	mci_writel(host, RINTSTS, ALL_INT_CLR);
+	return err;
+}
+
+static int dw_mci_starfive_parse_dt(struct dw_mci *host)
+{
+	struct of_phandle_args args;
+	struct starfive_priv *priv;
+	int ret;
+
+	priv = devm_kzalloc(host->dev, sizeof(*priv), GFP_KERNEL);
+	if (!priv)
+		return -ENOMEM;
+
+	ret = of_parse_phandle_with_fixed_args(host->dev->of_node,
+						"starfive,sysreg", 3, 0, &args);
+	if (ret) {
+		dev_err(host->dev, "Failed to parse starfive,sysreg\n");
+		return -EINVAL;
+	}
+
+	priv->reg_syscon = syscon_node_to_regmap(args.np);
+	of_node_put(args.np);
+	if (IS_ERR(priv->reg_syscon))
+		return PTR_ERR(priv->reg_syscon);
+
+	priv->syscon_offset = args.args[0];
+	priv->syscon_shift  = args.args[1];
+	priv->syscon_mask   = args.args[2];
+
+	host->priv = priv;
+
+	return 0;
+}
+
+static const struct dw_mci_drv_data starfive_data = {
+	.common_caps		= MMC_CAP_CMD23,
+	.set_ios		= dw_mci_starfive_set_ios,
+	.parse_dt		= dw_mci_starfive_parse_dt,
+	.execute_tuning		= dw_mci_starfive_execute_tuning,
+};
+
+static const struct of_device_id dw_mci_starfive_match[] = {
+	{ .compatible = "starfive,jh7110-mmc",
+		.data = &starfive_data },
+	{},
+};
+MODULE_DEVICE_TABLE(of, dw_mci_starfive_match);
+
+static int dw_mci_starfive_probe(struct platform_device *pdev)
+{
+	return dw_mci_pltfm_register(pdev, &starfive_data);
+}
+
+static struct platform_driver dw_mci_starfive_driver = {
+	.probe = dw_mci_starfive_probe,
+	.remove = dw_mci_pltfm_remove,
+	.driver = {
+		.name = "dwmmc_starfive",
+		.probe_type = PROBE_PREFER_ASYNCHRONOUS,
+		.of_match_table = dw_mci_starfive_match,
+	},
+};
+module_platform_driver(dw_mci_starfive_driver);
+
+MODULE_DESCRIPTION("StarFive JH7110 Specific DW-MSHC Driver Extension");
+MODULE_LICENSE("GPL");
+MODULE_ALIAS("platform:dwmmc_starfive");
