From 66770a004afe10df11d3902e16eaa0c2c39436bb Mon Sep 17 00:00:00 2001
From: Pawel Dembicki <paweldembicki@gmail.com>
Date: Fri, 24 May 2019 17:56:19 +0200
Subject: [PATCH] powerpc: Enable kernel XZ compression option on PPC_85xx

Enable kernel XZ compression option on PPC_85xx. Tested with
simpleImage on TP-Link TL-WDR4900 (Freescale P1014 processor).

Suggested-by: Christian Lamparter <chunkeey@gmail.com>
Signed-off-by: Pawel Dembicki <paweldembicki@gmail.com>
---
 arch/powerpc/Kconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/powerpc/Kconfig
+++ b/arch/powerpc/Kconfig
@@ -221,7 +221,7 @@ config PPC
 	select HAVE_KERNEL_GZIP
 	select HAVE_KERNEL_LZMA			if DEFAULT_UIMAGE
 	select HAVE_KERNEL_LZO			if DEFAULT_UIMAGE
-	select HAVE_KERNEL_XZ			if PPC_BOOK3S || 44x
+	select HAVE_KERNEL_XZ			if PPC_BOOK3S || 44x || PPC_85xx
 	select HAVE_KPROBES
 	select HAVE_KPROBES_ON_FTRACE
 	select HAVE_KRETPROBES
