From 5f20690f77878b1ba24ec88df01b92d5131a6780 Mon Sep 17 00:00:00 2001
From: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Date: Tue, 8 Nov 2022 15:23:57 +0100
Subject: [PATCH] arm64: dts: qcom: ipq8074: align TLMM pin configuration with
 DT schema

DT schema expects TLMM pin configuration nodes to be named with
'-state' suffix and their optional children with '-pins' suffix.

Signed-off-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Reviewed-by: Konrad Dybcio <konrad.dybcio@linaro.org>
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
Link: https://lore.kernel.org/r/20221108142357.67202-2-krzysztof.kozlowski@linaro.org
---
 arch/arm64/boot/dts/qcom/ipq8074.dtsi | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

--- a/arch/arm64/boot/dts/qcom/ipq8074.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq8074.dtsi
@@ -320,35 +320,35 @@
 			interrupt-controller;
 			#interrupt-cells = <0x2>;
 
-			serial_4_pins: serial4-pinmux {
+			serial_4_pins: serial4-state {
 				pins = "gpio23", "gpio24";
 				function = "blsp4_uart1";
 				drive-strength = <8>;
 				bias-disable;
 			};
 
-			i2c_0_pins: i2c-0-pinmux {
+			i2c_0_pins: i2c-0-state {
 				pins = "gpio42", "gpio43";
 				function = "blsp1_i2c";
 				drive-strength = <8>;
 				bias-disable;
 			};
 
-			spi_0_pins: spi-0-pins {
+			spi_0_pins: spi-0-state {
 				pins = "gpio38", "gpio39", "gpio40", "gpio41";
 				function = "blsp0_spi";
 				drive-strength = <8>;
 				bias-disable;
 			};
 
-			hsuart_pins: hsuart-pins {
+			hsuart_pins: hsuart-state {
 				pins = "gpio46", "gpio47", "gpio48", "gpio49";
 				function = "blsp2_uart";
 				drive-strength = <8>;
 				bias-disable;
 			};
 
-			qpic_pins: qpic-pins {
+			qpic_pins: qpic-state {
 				pins = "gpio1", "gpio3", "gpio4",
 				       "gpio5", "gpio6", "gpio7",
 				       "gpio8", "gpio10", "gpio11",
