From c4d2b02d63ee38b381fbc886c02eecfec4f981cc Mon Sep 17 00:00:00 2001
From: Jagan Teki <jagan@amarulasolutions.com>
Date: Mon, 23 Jan 2023 12:46:51 +0530
Subject: [PATCH] arm64: dts: rockchip: Add missing CM3i fallback compatible
 for Radxa E25
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

In order to function the Radxa E25 Carrier board, it is mandatory to
mount the Radxa CM3i module. 

Add Radxa CM3i compatible as fallback compatible to string to satisfy
the Module and Carrier board topology.

Fixes: 2bf2f4d9f673 ("arm64: dts: rockchip: Add Radxa CM3I E25")
Cc: Chukun Pan <amadeus@jmu.edu.cn>
Signed-off-by: Jagan Teki <jagan@amarulasolutions.com>
Link: https://lore.kernel.org/r/20230123071654.73139-2-jagan@amarulasolutions.com
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 arch/arm64/boot/dts/rockchip/rk3568-radxa-e25.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/rockchip/rk3568-radxa-e25.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3568-radxa-e25.dts
@@ -5,7 +5,7 @@
 
 / {
 	model = "Radxa E25";
-	compatible = "radxa,e25", "rockchip,rk3568";
+	compatible = "radxa,e25", "radxa,cm3i", "rockchip,rk3568";
 
 	aliases {
 		mmc1 = &sdmmc0;
