--- a/arch/arm/boot/dts/imx7d-pico-pi.dts
+++ b/arch/arm/boot/dts/imx7d-pico-pi.dts
@@ -8,12 +8,20 @@
 	model = "TechNexion PICO-IMX7D Board and PI baseboard";
 	compatible = "technexion,imx7d-pico-pi", "fsl,imx7d";
 
+	aliases {
+		led-boot = &led_system;
+		led-failsafe = &led_system;
+		led-running = &led_system;
+		led-upgrade = &led_system;
+		label-mac-device = &fec1;
+	};
+
 	leds {
 		compatible = "gpio-leds";
 		pinctrl-names = "default";
 		pinctrl-0 = <&pinctrl_gpio_leds>;
 
-		led {
+		led_system: led {
 			label = "gpio-led";
 			gpios = <&gpio2 6 GPIO_ACTIVE_HIGH>;
 		};
