From 3b92ee7b7899b6beffb2b484c58326e36612a873 Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Thu, 23 Dec 2021 14:52:56 +0000
Subject: [PATCH] net: phy: aquantia: add PHY_ID for AQR112R

As advised by Ian Chang this PHY is used in Puzzle devices.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
---
 drivers/net/phy/aquantia/aquantia_main.c | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/drivers/net/phy/aquantia/aquantia_main.c
+++ b/drivers/net/phy/aquantia/aquantia_main.c
@@ -29,6 +29,8 @@
 #define PHY_ID_AQR813	0x31c31cb2
 #define PHY_ID_AQR112	0x03a1b662
 #define PHY_ID_AQR412	0x03a1b712
+#define PHY_ID_AQR112C	0x03a1b790
+#define PHY_ID_AQR112R	0x31c31d12
 
 #define MDIO_PHYXS_VEND_IF_STATUS		0xe812
 #define MDIO_PHYXS_VEND_IF_STATUS_TYPE_MASK	GENMASK(7, 3)
@@ -880,6 +882,30 @@ static struct phy_driver aqr_driver[] =
 	.read_status	= aqr_read_status,
 },
 {
+	PHY_ID_MATCH_MODEL(PHY_ID_AQR112C),
+	.name		= "Aquantia AQR112C",
+	.probe		= aqr107_probe,
+	.config_aneg	= aqr_config_aneg_set_prot,
+	.config_intr	= aqr_config_intr,
+	.handle_interrupt = aqr_handle_interrupt,
+	.read_status	= aqr107_read_status,
+	.get_sset_count	= aqr107_get_sset_count,
+	.get_strings	= aqr107_get_strings,
+	.get_stats	= aqr107_get_stats,
+},
+{
+	PHY_ID_MATCH_MODEL(PHY_ID_AQR112R),
+	.name		= "Aquantia AQR112R",
+	.probe		= aqr107_probe,
+	.config_aneg	= aqr_config_aneg_set_prot,
+	.config_intr	= aqr_config_intr,
+	.handle_interrupt = aqr_handle_interrupt,
+	.read_status	= aqr107_read_status,
+	.get_sset_count	= aqr107_get_sset_count,
+	.get_strings	= aqr107_get_strings,
+	.get_stats	= aqr107_get_stats,
+},
+{
 	PHY_ID_MATCH_MODEL(PHY_ID_AQR113),
 	.name		= "Aquantia AQR113",
 	.probe          = aqr107_probe,
@@ -977,6 +1003,8 @@ static struct mdio_device_id __maybe_unu
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR813) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR112) },
 	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR412) },
+	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR112C) },
+	{ PHY_ID_MATCH_MODEL(PHY_ID_AQR112R) },
 	{ }
 };
 
