From: Felix Fietkau <nbd@nbd.name>
Date: Sat, 5 Feb 2022 18:36:36 +0100
Subject: [PATCH] arm64: dts: mediatek: mt7622: introduce nodes for
 Wireless Ethernet Dispatch

Introduce wed0 and wed1 nodes in order to enable offloading forwarding
between ethernet and wireless devices on the mt7622 chipset.

Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/arch/arm64/boot/dts/mediatek/mt7622.dtsi
+++ b/arch/arm64/boot/dts/mediatek/mt7622.dtsi
@@ -894,6 +894,11 @@
 		};
 	};
 
+	hifsys: syscon@1af00000 {
+		compatible = "mediatek,mt7622-hifsys", "syscon";
+		reg = <0 0x1af00000 0 0x70>;
+	};
+
 	ethsys: syscon@1b000000 {
 		compatible = "mediatek,mt7622-ethsys",
 			     "syscon";
@@ -912,6 +917,26 @@
 		#dma-cells = <1>;
 	};
 
+	pcie_mirror: pcie-mirror@10000400 {
+		compatible = "mediatek,mt7622-pcie-mirror",
+			     "syscon";
+		reg = <0 0x10000400 0 0x10>;
+	};
+
+	wed0: wed@1020a000 {
+		compatible = "mediatek,mt7622-wed",
+			     "syscon";
+		reg = <0 0x1020a000 0 0x1000>;
+		interrupts = <GIC_SPI 214 IRQ_TYPE_LEVEL_LOW>;
+	};
+
+	wed1: wed@1020b000 {
+		compatible = "mediatek,mt7622-wed",
+			     "syscon";
+		reg = <0 0x1020b000 0 0x1000>;
+		interrupts = <GIC_SPI 215 IRQ_TYPE_LEVEL_LOW>;
+	};
+
 	eth: ethernet@1b100000 {
 		compatible = "mediatek,mt7622-eth",
 			     "mediatek,mt2701-eth",
@@ -939,6 +964,9 @@
 		mediatek,ethsys = <&ethsys>;
 		mediatek,sgmiisys = <&sgmiisys>;
 		mediatek,cci-control = <&cci_control2>;
+		mediatek,wed = <&wed0>, <&wed1>;
+		mediatek,pcie-mirror = <&pcie_mirror>;
+		mediatek,hifsys = <&hifsys>;
 		dma-coherent;
 		#address-cells = <1>;
 		#size-cells = <0>;
