From 2dd441f16d6ad6104d85c4e5dfeb6dde4df26869 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Wed, 16 Feb 2022 07:34:08 +0100
Subject: [PATCH] watchdog: bcm7038_wdt: Support BCM6345 compatible string
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

A new "compatible" value has been added in the commit 17fffe91ba36
("dt-bindings: watchdog: Add BCM6345 compatible to BCM7038 binding").
It's meant to be used for BCM63xx SoCs family but hardware block can be
programmed just like the 7038 one.

Cc: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Acked-by: Florian Fainelli <f.fainelli@gmail.com>
Reviewed-by: Guenter Roeck <linux@roeck-us.net>
Link: https://lore.kernel.org/r/20220216063408.23168-1-zajec5@gmail.com
Signed-off-by: Guenter Roeck <linux@roeck-us.net>
Signed-off-by: Wim Van Sebroeck <wim@linux-watchdog.org>
---
 drivers/watchdog/bcm7038_wdt.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/watchdog/bcm7038_wdt.c
+++ b/drivers/watchdog/bcm7038_wdt.c
@@ -212,6 +212,7 @@ static SIMPLE_DEV_PM_OPS(bcm7038_wdt_pm_
 			 bcm7038_wdt_resume);
 
 static const struct of_device_id bcm7038_wdt_match[] = {
+	{ .compatible = "brcm,bcm6345-wdt" },
 	{ .compatible = "brcm,bcm7038-wdt" },
 	{},
 };
