From c6629b9a6738a64507478527da6c7b83c10a6d2c Mon Sep 17 00:00:00 2001
From: Vasily Khoruzhick <anarsoul@gmail.com>
Date: Tue, 7 Mar 2023 22:32:40 -0800
Subject: [PATCH] arm64: dts: rockchip: Add FriendlyElec Nanopi R5S

FriendlyElec Nanopi R5S is an open-sourced mini IoT gateway device.

Board Specifications
- Rockchip RK3568
- 2 or 4GB LPDDR4X
- 8GB or 16GB eMMC, SD card slot
- GbE LAN (Native)
- 2x 2.5G LAN (PCIe)
- M.2 Connector
- HDMI 2.0, MIPI DSI/CSI
- 2xUSB 3.0 Host
- USB Type C PD, 5V/9V/12V
- GPIO: 12-pin 0.5mm FPC connector

Based on Tianling Shen's <cnsztl@gmail.com> work.

Signed-off-by: Vasily Khoruzhick <anarsoul@gmail.com>
Link: https://lore.kernel.org/r/20230308063240.107178-2-anarsoul@gmail.com
Signed-off-by: Heiko Stuebner <heiko@sntech.de>
---
 arch/arm64/boot/dts/rockchip/Makefile         |   1 +
 .../boot/dts/rockchip/rk3568-nanopi-r5s.dts   | 713 ++++++++++++++++++
 2 files changed, 714 insertions(+)
 create mode 100644 arch/arm64/boot/dts/rockchip/rk3568-nanopi-r5s.dts

--- a/arch/arm64/boot/dts/rockchip/Makefile
+++ b/arch/arm64/boot/dts/rockchip/Makefile
@@ -74,4 +74,5 @@ dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3566-ro
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3566-soquartz-cm4.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3568-bpi-r2-pro.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3568-evb1-v10.dtb
+dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3568-nanopi-r5s.dtb
 dtb-$(CONFIG_ARCH_ROCKCHIP) += rk3568-rock-3a.dtb
--- /dev/null
+++ b/arch/arm64/boot/dts/rockchip/rk3568-nanopi-r5s.dts
@@ -0,0 +1,713 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+/*
+ * Copyright (c) 2022 FriendlyElec Computer Tech. Co., Ltd.
+ * (http://www.friendlyelec.com)
+ *
+ * Copyright (c) 2023 Tianling Shen <cnsztl@gmail.com>
+ */
+
+/dts-v1/;
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/leds/common.h>
+#include <dt-bindings/pinctrl/rockchip.h>
+#include <dt-bindings/soc/rockchip,vop2.h>
+#include "rk3568.dtsi"
+
+/ {
+	model = "FriendlyElec NanoPi R5S";
+	compatible = "friendlyarm,nanopi-r5s", "rockchip,rk3568";
+
+	aliases {
+		ethernet0 = &gmac0;
+		mmc0 = &sdmmc0;
+		mmc1 = &sdhci;
+	};
+
+	chosen: chosen {
+		stdout-path = "serial2:1500000n8";
+	};
+
+	hdmi-con {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
+	gpio-leds {
+		compatible = "gpio-leds";
+		pinctrl-names = "default";
+		pinctrl-0 = <&lan1_led_pin>, <&lan2_led_pin>, <&power_led_pin>, <&wan_led_pin>;
+
+		led-lan1 {
+			color = <LED_COLOR_ID_GREEN>;
+			function = LED_FUNCTION_LAN;
+			function-enumerator = <1>;
+			gpios = <&gpio3 RK_PD6 GPIO_ACTIVE_HIGH>;
+		};
+
+		led-lan2 {
+			color = <LED_COLOR_ID_GREEN>;
+			function = LED_FUNCTION_LAN;
+			function-enumerator = <2>;
+			gpios = <&gpio3 RK_PD7 GPIO_ACTIVE_HIGH>;
+		};
+
+		power_led: led-power {
+			color = <LED_COLOR_ID_RED>;
+			function = LED_FUNCTION_POWER;
+			linux,default-trigger = "heartbeat";
+			gpios = <&gpio4 RK_PD2 GPIO_ACTIVE_HIGH>;
+		};
+
+		led-wan {
+			color = <LED_COLOR_ID_GREEN>;
+			function = LED_FUNCTION_WAN;
+			gpios = <&gpio2 RK_PC1 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
+	vdd_usbc: vdd-usbc-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "vdd_usbc";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+	};
+
+	vcc3v3_sys: vcc3v3-sys-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3_sys";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&vdd_usbc>;
+	};
+
+	vcc5v0_sys: vcc5v0-sys-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc5v0_sys";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&vdd_usbc>;
+	};
+
+	vcc3v3_pcie: vcc3v3-pcie-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3_pcie";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		enable-active-high;
+		gpios = <&gpio0 RK_PD4 GPIO_ACTIVE_HIGH>;
+		startup-delay-us = <200000>;
+		vin-supply = <&vcc5v0_sys>;
+	};
+
+	vcc5v0_usb: vcc5v0-usb-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc5v0_usb";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&vdd_usbc>;
+	};
+
+	vcc5v0_usb_host: vcc5v0-usb-host-regulator {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio0 RK_PA6 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&vcc5v0_usb_host_en>;
+		regulator-name = "vcc5v0_usb_host";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&vcc5v0_usb>;
+	};
+
+	vcc5v0_usb_otg: vcc5v0-usb-otg-regulator {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio0 RK_PA5 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&vcc5v0_usb_otg_en>;
+		regulator-name = "vcc5v0_usb_otg";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&vcc5v0_usb>;
+	};
+
+	pcie30_avdd0v9: pcie30-avdd0v9-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "pcie30_avdd0v9";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <900000>;
+		regulator-max-microvolt = <900000>;
+		vin-supply = <&vcc3v3_sys>;
+	};
+
+	pcie30_avdd1v8: pcie30-avdd1v8-regulator {
+		compatible = "regulator-fixed";
+		regulator-name = "pcie30_avdd1v8";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		vin-supply = <&vcc3v3_sys>;
+	};
+};
+
+&combphy0 {
+	status = "okay";
+};
+
+&combphy1 {
+	status = "okay";
+};
+
+&combphy2 {
+	status = "okay";
+};
+
+&cpu0 {
+	cpu-supply = <&vdd_cpu>;
+};
+
+&cpu1 {
+	cpu-supply = <&vdd_cpu>;
+};
+
+&cpu2 {
+	cpu-supply = <&vdd_cpu>;
+};
+
+&cpu3 {
+	cpu-supply = <&vdd_cpu>;
+};
+
+&gmac0 {
+	assigned-clocks = <&cru SCLK_GMAC0_RX_TX>, <&cru SCLK_GMAC0>;
+	assigned-clock-parents = <&cru SCLK_GMAC0_RGMII_SPEED>, <&cru CLK_MAC0_2TOP>;
+	assigned-clock-rates = <0>, <125000000>;
+	clock_in_out = "output";
+	phy-handle = <&rgmii_phy0>;
+	phy-mode = "rgmii-id";
+	pinctrl-names = "default";
+	pinctrl-0 = <&gmac0_miim
+		     &gmac0_tx_bus2
+		     &gmac0_rx_bus2
+		     &gmac0_rgmii_clk
+		     &gmac0_rgmii_bus>;
+	snps,reset-gpio = <&gpio0 RK_PC5 GPIO_ACTIVE_LOW>;
+	snps,reset-active-low;
+	/* Reset time is 15ms, 50ms for rtl8211f */
+	snps,reset-delays-us = <0 15000 50000>;
+	tx_delay = <0x3c>;
+	rx_delay = <0x2f>;
+	status = "okay";
+};
+
+&gpu {
+	mali-supply = <&vdd_gpu>;
+	status = "okay";
+};
+
+&hdmi {
+	avdd-0v9-supply = <&vdda0v9_image>;
+	avdd-1v8-supply = <&vcca1v8_image>;
+	status = "okay";
+};
+
+&hdmi_in {
+	hdmi_in_vp0: endpoint {
+		remote-endpoint = <&vp0_out_hdmi>;
+	};
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
+&hdmi_sound {
+	status = "okay";
+};
+
+&i2c0 {
+	status = "okay";
+
+	vdd_cpu: regulator@1c {
+		compatible = "tcs,tcs4525";
+		reg = <0x1c>;
+		fcs,suspend-voltage-selector = <1>;
+		regulator-name = "vdd_cpu";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <800000>;
+		regulator-max-microvolt = <1150000>;
+		regulator-ramp-delay = <2300>;
+		vin-supply = <&vcc5v0_sys>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+
+	rk809: pmic@20 {
+		compatible = "rockchip,rk809";
+		reg = <0x20>;
+		interrupt-parent = <&gpio0>;
+		interrupts = <RK_PA3 IRQ_TYPE_LEVEL_LOW>;
+		#clock-cells = <1>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&pmic_int>;
+		rockchip,system-power-controller;
+		vcc1-supply = <&vcc3v3_sys>;
+		vcc2-supply = <&vcc3v3_sys>;
+		vcc3-supply = <&vcc3v3_sys>;
+		vcc4-supply = <&vcc3v3_sys>;
+		vcc5-supply = <&vcc3v3_sys>;
+		vcc6-supply = <&vcc3v3_sys>;
+		vcc7-supply = <&vcc3v3_sys>;
+		vcc8-supply = <&vcc3v3_sys>;
+		vcc9-supply = <&vcc3v3_sys>;
+		wakeup-source;
+
+		regulators {
+			vdd_logic: DCDC_REG1 {
+				regulator-name = "vdd_logic";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-init-microvolt = <900000>;
+				regulator-initial-mode = <0x2>;
+				regulator-min-microvolt = <500000>;
+				regulator-max-microvolt = <1350000>;
+				regulator-ramp-delay = <6001>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdd_gpu: DCDC_REG2 {
+				regulator-name = "vdd_gpu";
+				regulator-always-on;
+				regulator-init-microvolt = <900000>;
+				regulator-initial-mode = <0x2>;
+				regulator-min-microvolt = <500000>;
+				regulator-max-microvolt = <1350000>;
+				regulator-ramp-delay = <6001>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_ddr: DCDC_REG3 {
+				regulator-name = "vcc_ddr";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-initial-mode = <0x2>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+				};
+			};
+
+			vdd_npu: DCDC_REG4 {
+				regulator-name = "vdd_npu";
+				regulator-init-microvolt = <900000>;
+				regulator-initial-mode = <0x2>;
+				regulator-min-microvolt = <500000>;
+				regulator-max-microvolt = <1350000>;
+				regulator-ramp-delay = <6001>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_1v8: DCDC_REG5 {
+				regulator-name = "vcc_1v8";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdda0v9_image: LDO_REG1 {
+				regulator-name = "vdda0v9_image";
+				regulator-min-microvolt = <950000>;
+				regulator-max-microvolt = <950000>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdda_0v9: LDO_REG2 {
+				regulator-name = "vdda_0v9";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <900000>;
+				regulator-max-microvolt = <900000>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdda0v9_pmu: LDO_REG3 {
+				regulator-name = "vdda0v9_pmu";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <900000>;
+				regulator-max-microvolt = <900000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <900000>;
+				};
+			};
+
+			vccio_acodec: LDO_REG4 {
+				regulator-name = "vccio_acodec";
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vccio_sd: LDO_REG5 {
+				regulator-name = "vccio_sd";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <3300000>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc3v3_pmu: LDO_REG6 {
+				regulator-name = "vcc3v3_pmu";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <3300000>;
+				};
+			};
+
+			vcca_1v8: LDO_REG7 {
+				regulator-name = "vcca_1v8";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcca1v8_pmu: LDO_REG8 {
+				regulator-name = "vcca1v8_pmu";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vcca1v8_image: LDO_REG9 {
+				regulator-name = "vcca1v8_image";
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_3v3: SWITCH_REG1 {
+				regulator-name = "vcc_3v3";
+				regulator-always-on;
+				regulator-boot-on;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc3v3_sd: SWITCH_REG2 {
+				regulator-name = "vcc3v3_sd";
+				regulator-always-on;
+				regulator-boot-on;
+
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+		};
+
+	};
+};
+
+&i2c5 {
+	status = "okay";
+
+	hym8563: rtc@51 {
+		compatible = "haoyu,hym8563";
+		reg = <0x51>;
+		interrupt-parent = <&gpio0>;
+		interrupts = <RK_PD3 IRQ_TYPE_LEVEL_LOW>;
+		#clock-cells = <0>;
+		clock-output-names = "rtcic_32kout";
+		pinctrl-names = "default";
+		pinctrl-0 = <&hym8563_int>;
+		wakeup-source;
+	};
+};
+
+&i2s0_8ch {
+	status = "okay";
+};
+
+&i2s1_8ch {
+	rockchip,trcm-sync-tx-only;
+	status = "okay";
+};
+
+&mdio0 {
+	rgmii_phy0: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+		pinctrl-0 = <&eth_phy0_reset_pin>;
+		pinctrl-names = "default";
+		reset-assert-us = <10000>;
+		reset-deassert-us = <50000>;
+		reset-gpios = <&gpio0 RK_PC4 GPIO_ACTIVE_LOW>;
+	};
+};
+
+&pcie2x1 {
+	num-lanes = <1>;
+	reset-gpios = <&gpio0 RK_PB6 GPIO_ACTIVE_HIGH>;
+	status = "okay";
+};
+
+&pcie30phy {
+	data-lanes = <1 2>;
+	status = "okay";
+};
+
+&pcie3x1 {
+	num-lanes = <1>;
+	reset-gpios = <&gpio0 RK_PA0 GPIO_ACTIVE_HIGH>;
+	vpcie3v3-supply = <&vcc3v3_pcie>;
+	status = "okay";
+};
+
+&pcie3x2 {
+	num-lanes = <1>;
+	num-ib-windows = <8>;
+	num-ob-windows = <8>;
+	reset-gpios = <&gpio2 RK_PD6 GPIO_ACTIVE_HIGH>;
+	vpcie3v3-supply = <&vcc3v3_pcie>;
+	status = "okay";
+};
+
+&pinctrl {
+	gmac0 {
+		eth_phy0_reset_pin: eth-phy0-reset-pin {
+			rockchip,pins = <0 RK_PC4 RK_FUNC_GPIO &pcfg_pull_down>;
+		};
+	};
+
+	gpio-leds {
+		lan1_led_pin: lan1-led-pin {
+			rockchip,pins = <3 RK_PD6 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		lan2_led_pin: lan2-led-pin {
+			rockchip,pins = <3 RK_PD7 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		power_led_pin: power-led-pin {
+			rockchip,pins = <4 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		wan_led_pin: wan-led-pin {
+			rockchip,pins = <2 RK_PC1 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	hym8563 {
+		hym8563_int: hym8563-int {
+			rockchip,pins = <0 RK_PD3 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	pmic {
+		pmic_int: pmic-int {
+			rockchip,pins = <0 RK_PA3 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	usb {
+		vcc5v0_usb_host_en: vcc5v0-usb-host-en {
+			rockchip,pins = <0 RK_PA6 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		vcc5v0_usb_otg_en: vcc5v0-usb-otg-en {
+			rockchip,pins = <0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+};
+
+&pmu_io_domains {
+	pmuio1-supply = <&vcc3v3_pmu>;
+	pmuio2-supply = <&vcc3v3_pmu>;
+	vccio1-supply = <&vccio_acodec>;
+	vccio3-supply = <&vccio_sd>;
+	vccio4-supply = <&vcc_1v8>;
+	vccio5-supply = <&vcc_3v3>;
+	vccio6-supply = <&vcc_1v8>;
+	vccio7-supply = <&vcc_3v3>;
+	status = "okay";
+};
+
+&saradc {
+	vref-supply = <&vcca_1v8>;
+	status = "okay";
+};
+
+&sdhci {
+	bus-width = <8>;
+	max-frequency = <200000000>;
+	non-removable;
+	pinctrl-names = "default";
+	pinctrl-0 = <&emmc_bus8 &emmc_clk &emmc_cmd>;
+	status = "okay";
+};
+
+&sdmmc0 {
+	max-frequency = <150000000>;
+	no-sdio;
+	no-mmc;
+	bus-width = <4>;
+	cap-mmc-highspeed;
+	cap-sd-highspeed;
+	disable-wp;
+	vmmc-supply = <&vcc3v3_sd>;
+	vqmmc-supply = <&vccio_sd>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdmmc0_bus4 &sdmmc0_clk &sdmmc0_cmd &sdmmc0_det>;
+	status = "okay";
+};
+
+&tsadc {
+	rockchip,hw-tshut-mode = <1>;
+	rockchip,hw-tshut-polarity = <0>;
+	status = "okay";
+};
+
+&uart2 {
+	status = "okay";
+};
+
+&usb_host0_ehci {
+	status = "okay";
+};
+
+&usb_host0_ohci {
+	status = "okay";
+};
+
+&usb_host0_xhci {
+	extcon = <&usb2phy0>;
+	dr_mode = "host";
+	status = "okay";
+};
+
+&usb_host1_ehci {
+	status = "okay";
+};
+
+&usb_host1_ohci {
+	status = "okay";
+};
+
+&usb_host1_xhci {
+	status = "okay";
+};
+
+&usb2phy0 {
+	status = "okay";
+};
+
+&usb2phy0_host {
+	phy-supply = <&vcc5v0_usb_host>;
+	status = "okay";
+};
+
+&usb2phy0_otg {
+	status = "okay";
+};
+
+&usb2phy1 {
+	status = "okay";
+};
+
+&usb2phy1_host {
+	phy-supply = <&vcc5v0_usb_otg>;
+	status = "okay";
+};
+
+&usb2phy1_otg {
+	status = "okay";
+};
+
+&vop {
+	assigned-clocks = <&cru DCLK_VOP0>, <&cru DCLK_VOP1>;
+	assigned-clock-parents = <&pmucru PLL_HPLL>, <&cru PLL_VPLL>;
+	status = "okay";
+};
+
+&vop_mmu {
+	status = "okay";
+};
+
+&vp0 {
+	vp0_out_hdmi: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
+		reg = <ROCKCHIP_VOP2_EP_HDMI0>;
+		remote-endpoint = <&hdmi_in_vp0>;
+	};
+};
