From 790e1157753b4dcc9bad4521987fe09aa6657876 Mon Sep 17 00:00:00 2001
From: Geert Uytterhoeven <geert@linux-m68k.org>
Date: Thu, 25 Nov 2021 14:21:18 +0100
Subject: [PATCH 1003/1024] riscv: dts: starfive: Group tuples in interrupt
 properties

To improve human readability and enable automatic validation, the tuples
in the various properties containing interrupt specifiers should be
grouped.

Fix this by grouping the tuples of "interrupts-extended" properties
using angle brackets.

Signed-off-by: Geert Uytterhoeven <geert@linux-m68k.org>
---
 arch/riscv/boot/dts/starfive/jh7100.dtsi | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

--- a/arch/riscv/boot/dts/starfive/jh7100.dtsi
+++ b/arch/riscv/boot/dts/starfive/jh7100.dtsi
@@ -118,15 +118,15 @@
 		clint: clint@2000000 {
 			compatible = "starfive,jh7100-clint", "sifive,clint0";
 			reg = <0x0 0x2000000 0x0 0x10000>;
-			interrupts-extended = <&cpu0_intc 3 &cpu0_intc 7
-					       &cpu1_intc 3 &cpu1_intc 7>;
+			interrupts-extended = <&cpu0_intc 3>, <&cpu0_intc 7>,
+					      <&cpu1_intc 3>, <&cpu1_intc 7>;
 		};
 
 		plic: interrupt-controller@c000000 {
 			compatible = "starfive,jh7100-plic", "sifive,plic-1.0.0";
 			reg = <0x0 0xc000000 0x0 0x4000000>;
-			interrupts-extended = <&cpu0_intc 11 &cpu0_intc 9
-					       &cpu1_intc 11 &cpu1_intc 9>;
+			interrupts-extended = <&cpu0_intc 11>, <&cpu0_intc 9>,
+					      <&cpu1_intc 11>, <&cpu1_intc 9>;
 			interrupt-controller;
 			#address-cells = <0>;
 			#interrupt-cells = <1>;
