From 6ddf23526955b8dbedfeaa57e691261fd73f9d4e Mon Sep 17 00:00:00 2001
From: Frank Wunderlich <frank-w@public-files.de>
Date: Sun, 20 Aug 2023 17:31:35 +0200
Subject: [PATCH 22/22] arm64: dts: mt7986: change thermal trips on BPI-R3

Apply new naming after mt7986 thermal trips were changed.

Fixes: c26f779a2295 ("arm64: dts: mt7986: add pwm-fan and cooling-maps to BPI-R3 dts")
Suggested-by: Daniel Golle <daniel@makrotopia.org>
Signed-off-by: Frank Wunderlich <frank-w@public-files.de>
---
 .../boot/dts/mediatek/mt7986a-bananapi-bpi-r3.dts      | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

--- a/arch/arm64/boot/dts/mediatek/mt7986a-bananapi-bpi-r3.dts
+++ b/arch/arm64/boot/dts/mediatek/mt7986a-bananapi-bpi-r3.dts
@@ -152,16 +152,16 @@
 			trip = <&cpu_trip_active_high>;
 		};
 
-		cpu-active-low {
+		cpu-active-med {
 			/* active: set fan to cooling level 1 */
 			cooling-device = <&fan 1 1>;
-			trip = <&cpu_trip_active_low>;
+			trip = <&cpu_trip_active_med>;
 		};
 
-		cpu-passive {
-			/* passive: set fan to cooling level 0 */
+		cpu-active-low {
+			/* active: set fan to cooling level 0 */
 			cooling-device = <&fan 0 0>;
-			trip = <&cpu_trip_passive>;
+			trip = <&cpu_trip_active_low>;
 		};
 	};
 };
