From 679ee73bbee28cab441008f8cca38160cc8f3d05 Mon Sep 17 00:00:00 2001
From: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Date: Wed, 8 Feb 2023 11:15:39 +0100
Subject: [PATCH] arm64: dts: qcom: ipq6018: align RPM G-Link node with
 bindings

Bindings expect (and most of DTS use) the RPM G-Link node name to be
"rpm-requests".

Signed-off-by: Krzysztof Kozlowski <krzysztof.kozlowski@linaro.org>
Reviewed-by: Dmitry Baryshkov <dmitry.baryshkov@linaro.org>
Signed-off-by: Bjorn Andersson <andersson@kernel.org>
Link: https://lore.kernel.org/r/20230208101545.45711-1-krzysztof.kozlowski@linaro.org
---
 arch/arm64/boot/dts/qcom/ipq6018.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/qcom/ipq6018.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq6018.dtsi
@@ -176,7 +176,7 @@
 		qcom,rpm-msg-ram = <&rpm_msg_ram>;
 		mboxes = <&apcs_glb 0>;
 
-		rpm_requests: glink-channel {
+		rpm_requests: rpm-requests {
 			compatible = "qcom,rpm-ipq6018";
 			qcom,glink-channels = "rpm_requests";
 
